Serial Port Opened
monitor start
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

4194304 bytes read
do_spi_flash_uboot_save offset[0] len[400000]
spi0 is already setup!!!
SF: spi flash status register: 0x30, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBBBBBBBBV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8000
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=214482 214466 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x880005c, status=0x4602
avcpu ver = AVCPU_VERSION:[418:98d37dc99d0d] Buildcoimer[M_c  ck20pu, ea:0: 00ar

need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8a28 48
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8000
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at May  5 2017--18:06:49 symphony

 1. mem_start[80a38160]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 8131232
**CDU UDQ**: 8af0 48
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
[AI][_ai_jpeg_init]Entry...ticks:2
[AI][_ai_i2c_qam_init]Entry...ticks:3
[AI][_ai_i2c_init]Entry...ticks:3
[AI][_ai_i2c_1_init]Entry...ticks:3
[AI][_ai_i2c_fp_init]Entry...ticks:3
[AI][_ai_i2c_hdmi_init]Entry...ticks:4
[AI][_ai_spi_init]Entry...ticks:4
[AI][_ai_dm_init]Entry...ticks:4
[AI][_ai_dm_init]dm init v2...ticks:5
[AI][_ai_dm_init]set header...ticks:5
[AI][_ai_uio_init]Entry...ticks:5
[panel_concerto_attach]Entry...
[panel_concerto_attach]End
[_fp_mgr_open]Entry...
[_fp_attach]Entry..., type:3
[AI][_ai_hdmi_init]Entry...ticks:7
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:52
[AI][_ai_video_init]Entry...ticks:52
[AI][_ai_usb_init]Entry...ticks:54
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80A76020 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80A930C0 [AI][_ai_dmx_init]Entry...ticks:55
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:57
nim1=0x80ac8500
nim_cs8k_open in
priv->cfg.p_dem_bus =0x80a40440
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a76020


 ###step3### msg.event 2
nim_cs8k_set_22k_onoff 0
nim_cs8k_set_lnb_onoff 0
nim_cs8k_open out
[AI][_ai_mute_set]Entry...ticks:180
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c40000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d40000], size[180000], align[400], cfg size[1c01000]
tcpip: May  2 2017 11:31:01/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:184
file_size 312636 p_data_buffer 80b682a0 

 unzip resource. in_addr = 0x9e2afef3, out_addr = 0x811f9400, in_len = 312636, out_len = 899096
**LCK UDQ**: 2a4b
[AI][_ai_eva_init]Entry...ticks:215
[AI][_ai_tuner_init]Entry...ticks:216
[AI][_ai_dvb_init]Entry...ticks:237
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:237
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:258
[AI][_ai_usb_monitor_init]Entry...ticks:259
[AI][_ai_iconv_init]Entry...ticks:259
[AI][_ai_antenna_lnb_init]Entry...ticks:259
*********hdmi config value=12340000
[AI][_ai_time_init]Entry...ticks:294
eve223
[AI][ap_init]End...
close_fast_logo
mmi init
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 80a74b20
hub_add_new_dev 80bf0da0
port_reset 80a74b20
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x818d0400
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
Before ui_set_subt_display
After ui_set_subt_display
EMON> UI: disable subt........AS��.
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2625088, alloced_peak = 2627168, rest_size = 5506144

[NW] Set 3g sts:2
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
   #3usb_class_config 80bf0da0
device ADD cost 164 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [524210176]
[USB]ui_upg_file_list_get:file count[0x4]
[USB]ui_upg_file_list_get:valid_file_cnt[0x2]

## timeshift exist is [524210176]
p_cont[0x80bc9790], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
update signal
p_cont[0x80bc9790], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
p_cont[0x80bc9790], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
Barcode thread exit
Upgrade thread exit
monitor exit
