---------------Time Stamp[03:00:11]----------------
---------------Time Stamp[03:00:11]----------------
---------------Time Stamp[03:05:11]----------------
---------------Time Stamp[03:10:11]----------------
---------------Time Stamp[03:15:11]----------------
Barcode thread exit
Upgrade thread exit
monitor exit
Barcode thread exit
Upgrade thread exit
monitor exit
Serial Port Opened
monitor start
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBC98CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: st ^-^
In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841]cBuild Time:[Jul  4 2017, 16:23:29]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 24 2017--13:45:24 symphony

 1. mem_start[80d15c90]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30531440
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D52FA0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D70040 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d1d3a0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d52fa0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate [AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Jul 19 2017 11:32:10/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80db9360 p_wifi_dev 80db9460 p_lld 80db93b0 p_lld_addr 80db9364 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a6cee0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a6cefc --------
wifi dev = 0x80db96e0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 439550 p_data_buffer 80e47220 

 unzip resource. in_addr = 0x9e35f21f, out_addr = 0x82a33c00, in_len = 439550, out_len = 1080544
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:247
[AI][_ai_eva_init]Entry...ticks:248
[AI][_ai_tuner_init]Entry...ticks:248
[AI][_ai_dvb_init]Entry...ticks:269
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:269
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:291
[AI][_ai_iconv_init]Entry...ticks:292
[AI][_ai_antenna_lnb_init]Entry...ticks:292
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:293
[AI][_ai_time_init]Entry...ticks:327
eve0
[AI][ap_init]End...
ports0 
 hub_add_new_dev hcd 80d51aa0
hub_add_new_dev 80e8c3c0
port_reset 80d51aa0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 &ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x83f9dc00
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
on_factory_test_uart LINE:[204]
welcome toon_factory_test_uart LINE:[231]
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
-----ui show logo v2 size 0xd599, 0, 179
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2620192, alloced_peak = 2700544, rest_size = 27911248

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 160 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x21]
[USB]ui_upg_file_list_get:valid_file_cnt[0x9]

## timeshift exist is [1393786880]
p_cont[0x80ea9278], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
update signal
_switch_playstatus
from_id = 2 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 3
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 2 to 68 
sat_id[0], sat_name[], lnb_low[5150], lnb_high[5150]
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[0], freq[3000], sym[1000], pol[0], 22k[0]
_switch_playstatus
from_id = 68 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 4
UI: switch to LOGO..........
on_factory_test_uart LINE:[204]
welcome toon_factory_test_uart LINE:[231]
switch_autoclose: from 68 to 2 

#debug:ui_music_player_init! 

##debug: music_regist_callback !

##ufs_open fail[4]:[C:\audio_fav_list]
total count = 6
_switch_playstatus
from_id = 2 to_id = 49
new_ps = 4 CURN_MENU_PLAY_STATE = 3
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 2 to 49 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
music logo clear, 0x0

##debug: music_player_stop!

#debug :ui_music_player_release!
_switch_playstatus
from_id = 49 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 4
UI: switch to LOGO..........
on_factory_test_uart LINE:[204]
welcome toon_factory_test_uart LINE:[231]
switch_autoclose: from 49 to 2 
update signal
_switch_playstatus
from_id = 2 to_id = 11
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 11 
_switch_playstatus
from_id = 11 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 11 to 2 
_switch_playstatus
from_id = 2 to_id = 11
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 11 
_switch_playstatus
from_id = 11 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 11 to 2 
_switch_playstatus
from_id = 2 to_id = 11
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 11 
_switch_playstatus
from_id = 11 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 11 to 2 
---------------Time Stamp[14:04:11]----------------
---------------Time Stamp[14:09:11]----------------
Barcode thread exit
Upgrade thread exit
monitor exit
