Can not open serial port COM4
Serial Port Opened
monitor start
Upgrade start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Waiting for client up Finished.
Check Client
Client Functionality is good.
CheckCondition.
SendFlashToSTB.
Success to set user limit.
Success to inform the STB.
Success to start the transfer session.
---------------Time Stamp[20:50:09]----------------
Burning flash, Waiting...
Success to start the burn process.
Burn process finished.
Reboot command check ok.
Reboot
Upgrade finished
Upgrade return
monitor start
NOTE:hal_pm_concerto_reset: this function needs to be implemented


 Now Reboot System ,Please Waiting...ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]B$9BBBCBCCU
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8009
**  PACKET type : SIP_68S_DDR2
*****************************************
DRAM:  
DDR is 64MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=312768 312752 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x880005c, status=0x9a02
avcpu ver = AVCPU_VERSION:[470:d2ff6ab05ca8] Build Time:[Jun 16 2017, 17:20:36]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b0d 48
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8009
**  PACKET type : SIP_68S_DDR2
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Jul 21 2017--20:37:20 symphony

 1. mem_start[809b7aa8]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 8554840
**CDU UDQ**: 0
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
VBI PES BUF ADDR:0xa1d30000, VBI_PES_BUF_SIZE:0x00010000:0xbf232014
lpower_symphony_attach
[AI][_ai_jpeg_init]Entry...ticks:3
********************pdec_symphony_open*****************
[AI][_ai_i2c_qam_init]Entry...ticks:4
[AI][_ai_i2c_init]Entry...ticks:4
[AI][_ai_i2c_1_init]Entry...ticks:4
[AI][_ai_i2c_fp_init]Entry...ticks:5
[AI][_ai_i2c_hdmi_init]Entry...ticks:5
[AI][_ai_spi_init]Entry...ticks:5
[AI][_ai_dm_init]Entry...ticks:6
[AI][_ai_dm_init]dm init v2...ticks:6
[AI][_ai_dm_init]set header...ticks:6
[AI][_ai_uio_init]Entry...ticks:7
[_fp_attach]Entry..., type:2
lpower cfg :pd_key 0x0
 
                pd_key1 0x0
 
                pd_key_fp 0x57
ASī 
                type 0x0
 
                raw_map [0x0][0x1][0x2][0x3][0x4][0x5][0x6][0x7]

[AI][_ai_hdmi_init]Entry...ticks:9
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
hdmi_debug: p_priv->is_support_dvi_mode 0 p_priv->is_fastlogo_mode 0,p_priv 0x809feb80,ahg_rw 1
hdmi in main code
HDMI:hdmi_anx8560_open, 4974
  hdmi is_initialized 1[AI][_ai_audio_init]Entry...ticks:11
symphony_audio_attach: ok


 dolby disabled!!!!


-----------------hal_pinmux_sel
[AI][_ai_video_init]Entry...ticks:12
vdec stop!!!!!!
[AI][_ai_usb_init]Entry...ticks:16
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80A00B20 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80A1DBC0 [AI][_ai_dmx_init]Entry...ticks:17
dmx_symphony_tsi_set_es_buffer error !!!
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:19
********set shared memory:0xa1d2fc00!!!!
Disp mem pool success created!!!!!!
priv->cfg.p_dem_bus =0x809bfd80

 sr old is 255
 sr cur is 5
aud_timer_cb  AC3 48 --------
audio cfg hdmi_debug: DVI mode should not cfg audio sm 1
audio concerto HDMI cfg success!!!!
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a00b20


 ###step3### msg.event 2
[AI][_ai_mute_set]Entry...ticks:143
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c40000], size[180000], align[400]
symphony aud buffer set 0x83c40000 0x180000
[AI][_ai_av_buf_init]video Buf[a1d40000], size[180000], align[400], cfg size[1c01000]
********###########################SET BUF 1!!!!
tcpip: May 23 2017 17:03:57/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:150
file_size 346115 p_data_buffer 80af48a0 

 unzip resource. in_addr = 0x9e2c5057, out_addr = 0x811e0400, in_len = 346115, out_len = 989424
**LCK UDQ**: 2ab0
[AI][_ai_usb_monitor_init]Entry...ticks:205
[AI][_ai_eva_init]Entry...ticks:205
[AI][_ai_tuner_init]Entry...ticks:205
[AI][_ai_dvb_init]Entry...ticks:226
[CA]: init
[AI][_ai_dmm_init]Entry...ticks:226
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x38, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[dbiks.80010S.001]
[AI][_ai_avc_init]Entry...ticks:314
[AI][_ai_iconv_init]Entry...ticks:314
[AI][_ai_antenna_lnb_init]Entry...ticks:314
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:315
[AI][_ai_time_init]Entry...ticks:315
[CA]===>construct_cas_policy
[CA MANAGER]: type:0, para1:0, para2:0
set ca addr is 0x0
cas_adt_ncs_attach
0x6163bd30000412a
7:b364a56bb03b
eve223
[AI][ap_init]End...
close_fast_logo
mmi init
mmi ver 395:d339c83370c6
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
REGION:alpha onoff waiting ISR finish!!!
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:1&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 809ff620
hub_add_new_dev 80c68aa0
port_reset 809ff620
2, para1:0, para2:1
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x818d0400
[CA MANAGER]: type:1, para1:0, para2:0
end desktop init
get ver 0
[CA MANAGER]: type:2, para1:0, para2:0
close_fast_logo


=====================================================ASī=

sn_num:[06163bd30000412a],mac_address:[06163bd3412a]

======================================================

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 3 CURN_M&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
ENU_PLAY_STATE = 1
UI: switch to LOGO..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
stop type[1]
==========mute :on 

==========mute on:ap_send_to_av,IPC_MSG_AUD_FW_CMD_MUTE



start 0x83c60000,len 0x40000

vdec stop!!!!!!
[aud drv] audio already stop!
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
MCAS_VIDEO_STOP
UI: disable ttx.........
vdec stop!!!!!!
-----ui show logo v2 size 0xd4a9, 0, 179
p_dev = 809ff100, p_vdec = 809ff150
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:0, para2:2
---------g_curn_menu_1=1
[CA MANAGER]: type:3, para1:0, para2:0
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 3089472, alloced_peak = 3169344, rest_size = 5465368

EMON> [NW] Set 3g sts:2
   #3device ADD cost 160 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [493793280]
[CA MANAGER]: type:10, para1:2, para2:0
[USB]ui_upg_file_list_get:file count[0x4]
[USB]ui_upg_file_list_get:valid_file_cnt[0x2]
p_cont[0x80bd6a98], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
[CA MANAGER]: type:12, para1:2, para2:24
---------------Time Stamp[20:55:09]----------------
Serial Port Closed
monitor stop
---------------Time Stamp[21:00:09]----------------
---------------Time Stamp[21:05:09]----------------
---------------Time Stamp[21:10:09]----------------
---------------Time Stamp[21:15:09]----------------
---------------Time Stamp[21:20:09]----------------
---------------Time Stamp[21:25:09]----------------
---------------Time Stamp[21:30:09]----------------
---------------Time Stamp[21:35:09]----------------
---------------Time Stamp[21:40:09]----------------
---------------Time Stamp[21:45:09]----------------
---------------Time Stamp[21:50:09]----------------
Barcode thread exit
Upgrade thread exit
monitor exit
