Serial Port Opened
monitor start
ui_stop_tkgs_monitor
ui_epg_api_stop LINE:[340]
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x00, 0x00
SPI: Detected IS25LP128 with erase size 64 KiB, total 16 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBBBB99BBV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x00, 0x00
SPI: Detected IS25LP128 with erase size 64 KiB, total 16 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=256962 256946 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: st ^-^
In main , ebase=0x87e01001, cause=0x880005c, status=0x1b02
avcpu ver = AVCPU_VERSION:[455:5a79a9c0219a]cBuild Time:[May 23 2017, 14:11:
6]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Jul 13 2017--15:05:22 symphony

 1. mem_start[80d22b30]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30888144
**CDU UDQ**: 8b6f 48
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
lpower_symphony_attach
[AI][_ai_jpeg_init]Entry...ticks:2
[AI][_ai_i2c_qam_init]Entry...ticks:3
[AI][_ai_i2c_init]Entry...ticks:3
[AI][_ai_i2c_1_init]Entry...ticks:3
[AI][_ai_i2c_fp_init]Entry...ticks:4
[AI][_ai_i2c_hdmi_init]Entry...ticks:4
[AI][_ai_spi_init]Entry...ticks:4
[flash_pro] This flash can't be protected!!!
[AI][_ai_dm_init]Entry...ticks:5
[AI][_ai_dm_init]dm init v2...ticks:5
[AI][_ai_dm_init]set header...ticks:6
[AI][_ai_uio_init]Entry...ticks:6
_ai_ir_wakeup_set LINE:[1693]  p_ir_cfg->irda_wfilt_channel is 2-----------dh
_ai_ir_wakeup_set LINE:[1694]  val is 2139097845-----------dh
_ai_ir_wakeup_set LINE:[1693]  p_ir_cfg->irda_wfilt_channelASï is 2-----------dh
_ai_ir_wakeup_set LINE:[1694]  val is 33688309-----------dh
[_fp_attach]Entry..., type:2
lpower cfg :pd_key 0x0
 
                pd_key1 0x0
 
                pd_key_fp 0x77
 
                type 0x0
 
                raw_map [0x0][0x1][0x2][0x3][0x4][0x5][0x6][0x7]

[AI][_ai_hdmi_init]Entry...ticks:10
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:15
[AI][_ai_video_init]Entry...ticks:15
[AI][_ai_usb_init]Entry...ticks:17
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D60A80 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D7DB20 [AI][_ai_dmx_init]Entry...ticks:18
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:21
priv->cfg.p_dem_bus =0x80d2ae00
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d60a80


 ###step3### msg.event 2
[AI][_ai_mute_set]Entry...ticks:144
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: May 23 2017 17:03:45/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80dc6e40 p_wifi_dev 80dc6f40 p_lld 80dc6e90 p_lld_addr 80dc6e44 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a71fa0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a71fbc --------
wifi dev = 0x80dc71c0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:150
file_size 439550 p_data_buffer 80e54d00 

 unzip resource. in_addr = 0x9e35e809, out_addr = 0x82a97c00, in_len = 439550, out_len = 1080544
**LCK UDQ**: 2ab0
[AI][_ai_usb_monitor_init]Entry...ticks:189
[AI][_ai_eva_init]Entry...ticks:190
[AI][_ai_tuner_init]Entry...ticks:190
[AI][_ai_dvb_init]Entry...ticks:211
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:211
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:226
[AI][_ai_iconv_init]Entry...ticks:226
[AI][_ai_antenna_lnb_init]Entry...ticks:226
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:227
[AI][_ai_time_init]Entry...ticks:261
eve223
[AI][ap_init]End...
close_fast_logo
mmi init
mmi ver 415:bb1cc3ef0e6d
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_i&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 80d5f580
hub_add_new_dev 80f61d60
port_reset 80d5f580
d = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x83f9dc00
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcdASï_poll_rh_status 
UI: disable ttx.........
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2623296, alloced_peak = 2624288, rest_size = 28264848

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 159 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [493793280]
[USB]ui_upg_file_list_get:file count[0x2]
[USB]ui_upg_file_list_get:valid_file_cnt[0x1]

## timeshift exist is [493793280]
p_cont[0x80eb6b58], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
update signal
Barcode thread exit
Upgrade thread exit
monitor exit
