Serial Port Opened
monitor start
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
video_out_ticks 941
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a18b80


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 80a17680
hub_add_new_dev 80ce2c00
port_reset 80a17680
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
   #3device ADD cost 163 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [0]

##try timeshift [865150976]byte

##try timeshift [432575488]byte

##try timeshift [136314880]byte
[CA MANAGER]: type:10, para1:1, para2:0
[USB]ui_upg_file_list_get:file count[0xb]
[USB]ui_upg_file_list_get:valid_file_cnt[0x7]
p_cont[0x80c17a1c], root[0]
_switch_playstatus
from_id = 1 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 24 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:24
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

4194304 bytes read
do_spi_flash_uboot_save offset[0] len[400000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected PN25F32 with erase size 64 KiB, total 4 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]B$99BBCBCCU
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8009
**  PACKET type : SIP_68S_DDR2
*****************************************
DRAM:  
DDR is 64MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=213946 213930 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x880005c, status=0x9b02
avcpu ver = AVCPU_VERSION:[506:bee78f98ed8a] Build Time:[Jul 25 2017, 10:29:12]

 DebugInfo:  
 av request irq[0x4], pipenum[0x20], pipe_startonder[o_8heak_9pu,resdya srar0
83ea91ec]
p_g_pipe is 83EA279C 
AV cpu create a pipe for 0xa000a000----->0xb000b000
AV CPU has started, clock 54000000
AV CPU id get pass 
aud fw init 0x83eade80 0x83eadd40
p_g_pipe is 83EA279C 
AV cpu create o pepeofoh 0k10p00r07d-- ->ax2
000407
vid fw init
p_g_pipe is 83EA279C 
AV cpu create a pipe for 0x10000413----->0x20000413
av_vdec_kernel_init done
AV_GB: enable: [0]
avsync_module_init ok
avsync_attach_symphony_audio_render: ok[-1]
avsynconterco_shepk_npuvreedyr sdar:
ok
vid fw init 222
symphony_set_local_cpu_ready: end
aud stack 0x83e89784
avmain:schedMain status=0x1001

 av_timer_id2 = 0x2concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_appASï 0x89 
10123**CDU UDQ**: 8b0d 48
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8009
**  PACKET type : SIP_68S_DDR2
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Jul 26 2017--14:54:37 symphony

 1. mem_start[80971160]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 5735072
**CDU UDQ**: 8b6f
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
VBI PES BUF ADDR:0xa1a20000, VBI_PES_BUF_SIZE:0x00010000:0xbf232014
lpower_symphony_attach
[AI][_ai_jpeg_init]Entry...ticks:3
********************pdec_symphony_open*****************
[AI][_ai_i2c_qam_init]Entry...ticks:4
[AI][_ai_i2c_init]Entry...ticks:4
[AI][_ai_i2c_1_init]Entry...ticks:4
[AI][_ai_i2c_fp_init]Entry...ticks:5
[AI][_ai_i2c_hdmi_init]Entry...ticks:5
[AI][_ai_spi_init]Entry...ticks:5
[AI][_ai_dm_init]Entry...ticks:6
[AI][_ai_dm_init]dm init v2...ticks:6
[AI][_ai_dm_init]set header...ticks:6
[AI][_ai_uio_init]Entry...ticks:7
_ai_ir_wakeup_set LINE:[1693]  p_ir_cfg->irda_wfilt_channel is 2-----------dh
_ai_ir_wakeup_set LINE:[1694]  valASï is 2139097845-----------dh
_ai_ir_wakeup_set LINE:[1693]  p_ir_cfg->irda_wfilt_channel is 2-----------dh
_ai_ir_wakeup_set LINE:[1694]  val is 33688309-----------dh
[_fp_attach]Entry..., type:3
lpower cfg :pd_key 0x0
 
                pd_key1 0x0
 
                pd_key_fp 0x77
 
                type 0x0
 
                raw_map [0x0][0x1][0x2][0x3][0x4][0x5][0x6][0x7]

[AI][_ai_hdmi_init]Entry...ticks:11
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
hdmi_debug: p_priv->is_support_dvi_mode 0 p_priv->is_fastlogo_mode 0,p_priv 0x809ad040,ahg_rw 1
hdmi in main code
HDMI:hdmi_anx8560_open, 4974
  hdmi is_initialized 1[AI][_ai_audio_init]Entry...ticks:14
symphony_audio_attach: ok


 dolby disabled!!!!


-----------------hal_pinmux_sel
[AI][_ai_video_init]Entry...ticks:15
av_vdec_kernel_process.....cmd 110413 
av_vdec_kernel_process.....cmd 20413 
vdec stop!!!!!!
[AI][_ai_usb_init]Entry...ticks:18
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 809AEFE0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 809CC080 [AI][_ai_dmx_init]Entry...ticks:19
dmx_symphony_tsi_set_es_buffer error !!!
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:22
av_vdec_kernel_process.....cmd 220413 
********set shared memory:0xa1a1fc00!!!!
Disp mem pool success created!!!!!!
priv->cfg.p_dem_bus =0x80979440
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809aefe0


 ###step3### msg.event 2
[AI][_ai_mute_set]Entry...ticks:146
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c40000], size[180000], align[400]
symphony aud buffer set 0x83c40000 0x180000
[AI][_ai_av_buf_init]video Buf[a1a30000], size[180000], align[400], cfg size[1f11000]
********###########################SET BUF 1!!!!
av_vdec_kernel_process.....cmd 100413 
$$$$$$ 1, 80000000 
tcpip: May 23 2017 17:03:57/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
usb_eth_asix_attach asix done
asix_open new done
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:151
file_size 313141 p_data_buffer 80aa87c0 

 unzip resource. in_addr = 0x9e29c0f7, out_addr = 0x80ee9400, in_len = 313141, out_len = 905568
**LCK UDQ**: 2ab0
[AI][_ai_usb_monitor_init]Entry...ticks:201
[AI][_ai_eva_init]Entry...ticks:201
[AI][_ai_tuner_init]Entry...ticks:202
tuner 0 init edbert
nc_svc_init,support dvbs_2[1]
_switch_ctrl , line 1439
[AI][_ai_dvb_init]Entry...ticks:223
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:223
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:250
[AI][_ai_iconv_init]Entry...ticks:250
[AI][_ai_antenna_lnb_init]Entry...ticks:250
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:251
[AI][_ai_time_init]Entry...ticks:251
eve223
[AI][ap_init]End...
close_fast_logo
mmi init
mmi ver 415:bb1cc3ef0e6d
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
REGION:alpha onoff waiting ISR finish!!!
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 809adae0
hub_add_new_dev 80bb4440
port_reset 809adae0
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap ASïplayback
UI: active playback.........
_ui_epg_api_init epg addr 0x815c0400
db config :total mem size:2097152; net size:24;ts size:1536;svc size:10240;evt size:1823208
db config :net_node_num:2; ts_node_num:128
db config :svc_node_num:512;evt_node_num:15717
db config :total mem size:2097152; net size:24;ts size:1536;
db config :svc size:10240;evt size:1823172;non_fix size:262180
####debug memp headle[0x80bb4670] add:0x817803dc  end addr:0x817c0400ui_epg_api_start LINE:[350]
ui_epg_api_stop LINE:[340]
mul_epg&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
_filter_policy LINE:[411]
mul_epg_filter_policy LINE:[490]
epg_pin_start_info: [0xffff], t[0xffff], s[0xffff];pf table:2,sch table:0
###debug epg_pin_request_pf_eit[0x4e] filter:netid=0x65535,tsid=0x65535,sid=65535
###debug epg_pin_request_pf_eit[0x4f] filter:netid=0x65535,tsid=0x65535,sid=65535
ui_epg_api_start LINE:[409]
ui_epg_api_start LINE:[412]
end desktop init
get ver 0
close_fast_logo
@@@uASïi_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
PB_CMD_STOP_SYNC
##########do_stop 0x0 0x1##
^^^^^^^^^^  stop start ticks 270
==========mute :on 

msg enter id is 90407
==========mute on:ap_send_to_av,IPC_MSG_AUD_FW_CMD_MUTE



start 0x83c60000,len 0x40000

^^^^^^^^^^  step1 : 272
vdec stop!!!!!!
^^^^^^^^^^  step2 : 272
[aud drv] audio already stop!
^^^^^^^^^^  step3 : 272
^^^^^^^^^^  step4 : 272
^^^^^^^^^^  step5 : 273
^^^^^^^^^^  step6 : 273
dmx_symphony_chan_reset >>>>>>>>>> 
^^^^^^^^^^  step7 : 273
^^^^^^^^^^  step8 : 274
PB stop by sync ticks 274
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt

 sr old is 255
 sr cur is 5
aud_timer_cb  AC3 48 --------
audio cfg hdmi_debug: DVI mode should not cfg audio sm 1
audio concerto HDMI cfg success!!!!
got VBI_TTX_STOPPED
UI: disable ttx.........
switch_autoclose: from 0 to 2 
sASïwitch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2639840, alloced_peak = 2640832, rest_size = 3095232

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 161 ts 
HP_BUS_PLUG_IN

##VFS_PLUG_IN_EVENT ready usb1
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [0]

##try timeshift [865150976]byte

##try timeshift [432575488]byte

##try timeshift [136314880]byte

##debug: ufs_readdir end!

[1][C][u][156804]
[2][C][a][186300]
[3][C][f][4194304]
[4][C][f][4194304]
[5][C][a][891144]
[6][C][f][4194304]
[7][C][f][8388608]
[8][C][f][4194304]
[9][C][f][4194304]
[10][C][i][4194304]
[11][C][f][4194304]
[USB]ui_upg_file_list_get:file count[0xb]
[USB]ui_upg_file_list_get:valid_file_cnt[0x7]
p_cont[0x80b0a478], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
EIT section table[0x4e] time out:EIT_TIMEOUT_EVENT
EIT section table[0x4f] time out:EIT_TIMEOUT_EVENT
dvbs_switch_nimtype,nim_type[1]
dvbs_lock_again,nimtype[2]
dvbs_lock_again,has checked again
nc: send evt lock[0]
!!!!!PB:PB_EVT_LOCK_RSL 0
^^^^^^^^^^ ret lock1 457
dvbs_calc_search_info: 22k 1, polarization: 1
PB play ticks 458  status 1
^^^^^^^^^^  step9 : 458
==========mute :on 

msg enter id is 90407
==========mute on:ap_send_to_av,IPC_MSG_AUD_FW_CMD_MUTE



start 0x83c60000,len 0x40000

Mark ap playback 1 do play:  vpid =6601 , apid = 6401, mode 3
av_vdec_kernel_process.....cmd d0413 
fw: disable file playback mode!!!
avsync set mode:[0]
^^^^^^^^^^  step10 : 461
set video mode 3
symphony_vdec_start >>>> format = 1
av_vdec_kernel_process.....cmd 10413 
VIDEO FORMAT:1,video state:2, mode:3, page_size_mode:0 
s_vdec_kernel_info.v_format= 1
ves_addr=3940000, ves_size = 300000
vdec_heap_addr = 1a30000, vdec_dpb_addr=1aac000
vdec_heap_szie = 7bd48, vdec_dpb_size=1b00000
vdec_fw: get_ts_pts_mode_symphony [0] [ff000201]
 es_mode = 0
+++++++++video_dec_init+++++++++
mem_addr addr:1aac000, 
before protect reg_88:30002000, reg_4c(mbinfo):80000800, reg_60(dbk):0, reg_54(not coded):0
end protect reg_88:d560d56, reg_4c(mbinfo):80003558ASï, reg_60(dbk):0, reg_54(not coded):1aac7f
vdec_major_version_id:1
vdec support stds:400009f
bit[0]:h264, bit[1]avs, bit[2]:mpeg2, bit[3]mpeg4
bit[4]:vc1, bit[5]vp8, bit[6]:rv, bit[7]hevc
init pts mode:1
policy_sd_only:0, support_hevc:0
policy not support hevc
hd close di, no motion memory
hevc/h264: addr:1aac000, size:deac3de9
memory B address:329c000, size:310000 bytes

H.264 Dec...
set dirty picture error percent 83e88d50
p_vhdl_h = 81a30000, 83eb5700
 avsync_module_restart:[3550]
avsync_video_init end vfm = 2
AAAA: av_irq_request (*((volatile u32*)(0xbf110060))) = fff7dfe8 
^^^^^^^^^^  step11 : 471
^^^^^^^^^^  s rate[25][0]=[0]
=========concerto_aud_start :entered  1  0 

msg enter id is 407
msg enter id is 50407
aud_kernel buf info: id=[1] buf=[83dc0000] end=[83ddffff] size=[20000] rd_reg=[bf26022c] wr_reg=[bf260234]
aud_avsync_on_symphony: [100] [1]
aud_fw_kernel_start_symphony:
aud_avsync_on_symphony: [100] [1]
avsync_audio_init
avsync_module_restart:[3327]
A: render reset
avsync_audio_init end
aud_es_bASïuf: [83dc0000][83ddffff] [83dc0000]
aud_avsync_on_symphony: [100] [1]
concerto_aud_start:ap_send_to_av,IPC_MSG_AUD_FW_CMD_START


  hdmi dbg mode offfffffffffffffffffffff
^^^^^^^^^^  step1a : 476
==========level :2 
==========scale :786 

msg enter id is 110407

 output fmt is set to 0

Mark ap playback 1 1 line :929 tick=477
^^^^^^^^^^  step13 : 478
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
tuner[0], get_lock[0], repeat_time[0]
status[0][2]
tuner[0], get_lock[0], repeat_time[1]
status[0][2]
tuner[0], get_lock[0], repeat_time[2]
status[0][0]
!!!!Signal monitor id[0], lock[0]
update signal
tuner[0], get_lock[0], repeat_time[0]
status[0][2]
###nc_monitor
dvbs_switch_nimtype,nim_type[2]
dvbs tc lock tuner freq 1315000, sym 30000, polar 1, pol 1, nim type[1], 22K[1]
move ahead 2

 $$$$ print_diseqcinfo
tuner_id=0
is_fixed=1
position_type=0
position=0
diseqc_type_1_0=0
diseqc_port_1_0=0
diseqc_type_1_1=0
diseqc_port_1_1=0
used_DiSEqC12=0
d_sat_longitude=%f
d_local_longitude=%f
d_local_latitude=%f
diseqc_1_1_mode=0
tuner[0], get_lock[0], repeat_time[1]
status[0][2]
tuner[0], get_lock[0], repeat_time[2]
status[0][0]
!!!!Signal monitor id[0], lock[0]
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
Serial Port Closed
upg or dump task  is canceled!
monitor stop
Barcode thread exit
Upgrade thread exit
monitor exit
Serial Port Opened
monitor start
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB9B9BBBV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
Run avcpu fail.
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

4194304 bytes read
do_spi_flash_uboot_save offset[0] len[400000]
spi0 is already setup!!!
SF: spi flash status register: 0x00, 0x00
SPI: Detected IS25LP128 with erase size 64 KiB, total 16 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB9B99BBV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=214118 214102 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x880005c, status=0x1b02
avcpu ver = AVCPU_VERSION:[506:bee78f98ed8a] Build Time:[Jul 26 2017, 
6:22:35]

 DebugInfo:  
 av request irq[0x4], pipenum[0x20], pipe_startaddr [0x83ea289c], msg_addr [0x83ea92ec]
h_g_pipe is 83EA289C 

V cpu create a pipe for 0xa000a000----->0xb000b000
AV CPU has started, clock 54000000
AV CPU id get pasco
cud fw init 0x83eadf80 0x83ea
e40
p_g_pipe is 83EA289C 
AV cpu create a pipe for 0x10000407----->0x20000407
vid fw init
p_g_pipe is 8coA289C 
cV cpu create a pipe fo
 0x10000413----->0x20000413
av_vdec_kernel_init done
AV_GB: enable: [0]
avsync_module_init ok
avsync_attach_symphony_audio_render: ok[-
]
avsync_attach_symphony_video_render: ok
vid fw init 222
symphony_set_local_cpu_ready: end
aud stack 0c83e89884
avmain:schedMain statu
=0x1001
t
 av_timer_id2 = 0x2o_to_block_app 0x89 
10123**CDU UDQ**: 8b0d 48
Serial Port Closed
upg or dump task  is canceled!
monitor stop
---------------Time Stamp[16:42:59]----------------
---------------Time Stamp[16:47:59]----------------
---------------Time Stamp[16:52:59]----------------
---------------Time Stamp[16:57:59]----------------
---------------Time Stamp[17:02:59]----------------
---------------Time Stamp[17:07:59]----------------
---------------Time Stamp[17:12:59]----------------
---------------Time Stamp[17:17:59]----------------
Barcode thread exit
Upgrade thread exit
monitor exit
