Serial Port Opened
monitor start
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77567788V
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x00, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668878V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657777V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658878V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77567787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657788V
---------------Time Stamp[18:03:53]----------------
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657777V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667777V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77567788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77558888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I67558888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667777V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657777V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77567788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657777V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667777V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657777V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667787V
---------------Time Stamp[18:08:53]----------------
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77558878V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658878V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568878V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77557788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657788V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77657778V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77557787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77458888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77558888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658878V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77558888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568887V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77568888V
---------------Time Stamp[18:13:53]----------------
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668878V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77667787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77668888V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77567787V
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_44_3b48b76987f7] Build Time:[Aug 10 2017, 16:40:22]I77658888V
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x00, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BCB99CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x00, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: st ^-^
In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841]cBuild Time:[Jul  4 2017, 16:23:
9]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 23 2017--18:13:28 symphony

 1. mem_start[80d14890]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30946160
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D51BA0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D6EC40 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d1bfa0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d51ba0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Jul 19 2017 11:32:10/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80db7f60 p_wifi_dev 80db8060 p_lld 80db7fb0 p_lld_addr 80db7f64 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a6bae0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a6bafc --------
wifi dev = 0x80db82e0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 439550 p_data_buffer 80e45e20 

 unzip resource. in_addr = 0x9e35f25f, out_addr = 0x82a97c00, in_len = 439550, out_len = 1080544
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:247
[AI][_ai_eva_init]Entry...ticks:248
[AI][_ai_tuner_init]Entry...ticks:248
[AI][_ai_dvb_init]Entry...ticks:269
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:269
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:291
[AI][_ai_iconv_init]Entry...ticks:292
[AI][_ai_antenna_lnb_init]Entry...ticks:292
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:293
[AI][_ai_time_init]Entry...ticks:327
eve0
[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80d506a0
hub_add_new_dev 80e8afc0
port_reset 80d506a0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 &ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x83f9dc00
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
on_factory_test_uart LINE:[204]
welcome toon_factory_test_uart LINE:[231]
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
-----ui show logo v2 size 0xd599, 0, 179
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2620192, alloced_peak = 2700544, rest_size = 28325968

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 160 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x21]
[USB]ui_upg_file_list_get:valid_file_cnt[0x9]

## timeshift exist is [1393786880]
p_cont[0x80ea7e78], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
update signal
---------------Time Stamp[18:18:53]----------------
---------------Time Stamp[18:23:53]----------------
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb`0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
usage: fatload <interface> <dev[:part]> <addr> <filename> [bytes]
do_spi_flash_uboot_save offset[0] len[2d600000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
---------------Time Stamp[18:28:53]----------------
ROSerial Port Closed
upg or dump task  is canceled!
monitor stop
---------------Time Stamp[18:33:53]----------------
Serial Port Opened
monitor start
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: sta^-^ In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Jul  4 2017, 16:23:
9]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0
---------------Time Stamp[18:38:53]----------------


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 23 2017--18:36:31 symphony

 1. mem_start[80d15c90]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30941040
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D52FA0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D70040 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d1d3a0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d52fa0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate [AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Jul 19 2017 11:32:10/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80db9360 p_wifi_dev 80db9460 p_lld 80db93b0 p_lld_addr 80db9364 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a6cee0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a6cefc --------
wifi dev = 0x80db96e0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 564267 p_data_buffer 80e47220 

ASSERT:D:\Work\Vendace\Vendace_428_NewSDK_\stboxge-tech\prj\dvbs\vendace\ui\ui_init.c line 370
#AP!# exception!
Breakpoint exception
EPC[0x80158a18], CAUSE[0x10800024], SR[0x1100ff03], SP[0x80ab20b8]!

s_log_buff( 80ED0EA0) s_log_len=100

showcs 80158a18 80ab20b8 80158a18

 OSIntNesting=0 OSLockNesting=0 

 current task priority is 6, stack cur is 80ab1da0   bottom at :80aaa300  Size=8192 


 task name initT1 

stkcur=0x80ab20b8   top=0x80ab2300 


<0x80ab20a0> 0x64        0xfffffffe  0x1100ff03  0x80158a18  0x0         0x0         0x80058524  0x800583d0  
<0x80ab20c0> 0x800583e4  0x172       0x89c2b     0x80e47220  0x110000    0x8022c024  0x80ab0000  0x80d16d20  
<0x80ab20e0> 0x4000      0x807c0000  0x80050000  0x8022c024  0x0         0x0         0x80229a00  0x80126a20  
<0x80ab2100> 0x800553f4  0x807bf394  0xd0        0x80dca178  0x0         0x0         0x0         0x0         
<0x80ab2120> 0x0         0x0         0x0         0x0         0x0         0x0         0x0 iEď        0x0         
<0x80ab2140> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2160> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2180> 0x80d16d00  0x80220154  0x0         0x0         0x0         0x0         0x1100ff01  0x0         
<0x80ab21a0> 0x0         0x80a80000  0x8d2e      0x80a8ba38  0x8021ff1c  0x80223e70  0x1040      0x80ab22b8  
<0x80ab21c0> 0x20        0x1000      0x80127ba4  0x80a80000  0x80d16d20  0x80229a00  0x8022ce6c  0x80223e70  
<0x80ab21e0> 0x0         0x0         0x0         0x0         0x20        0x8022c87c  0x0         0x0         
<0x80ab2200> 0x0         0x0         0x20        0x0         0x80ab22b8  0x1000      0x80229a00  0x8022ce6c  
<0x80ab2220> 0x2a        0x5b        0x16c       0x80127d68  0x0         0x80029d38  0x0         0x0         
<0x80ab2240> 0x20        0x0         0x400       0x0         0x3         0x8022cc78  0x5b        0x80d16d20  
<0x80ab2260> iEď0x5b        0x0         0x5b        0x80d16d20  0x5b        0x802d6ab8  0x80aa13a8  0x80aa13d8  
<0x80ab2280> 0x1d81f70   0x80d16d20  0x80050000  0x80d16d20  0x80229a00  0x8022ce6c  0x80228e30  0x0         
<0x80ab22a0> 0x80050000  0x80d16d20  0x80229a00  0x8022ce6c  0x80228e30  0x0         0x0         0x0         
<0x80ab22c0> 0x0         0x80127c30  0x80055a30  0x80055a24  0x80ab22a0  0x808c0000  0x80d16d20  0x1000      
<0x80ab22e0> 0x2aea5400  0x0         0x0         0x0         0x0         0x0         0x0         0x8002adfc  
<0x80ab2300> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         

prio[6  ] pc[0x0] state=0  [dely=0       ] top=0x80ab2300  bottom=0x80aaa300  cur_sp=0x80ab1e20, ra[0x0] initT1, bottomMagic=0x0
prio[7  ] pc[0x80025500] state=32 [dely=0       ] top=0x80d16cc0  bottom=0x80d15cc0  cur_sp=0x80d16be8, ra[0x80025500] Timer, bottomMagic=0x0
prio[9  ] pc[0x8044ee10] state=0  [dely=0       ] top=0x80db9200  bottom=0x80db1200  cur_sp=0x80db9200, riEďa[0x8002adfc] tcpip_thread, bottomMagic=0x0
prio[17 ] pc[0x802e9e24] state=0  [dely=0       ] top=0x80d52f40  bottom=0x80d51f40  cur_sp=0x80d52948, ra[0x8022a2c8] usb_bus, bottomMagic=0x0
prio[53 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d1c580  bottom=0x80d18580  cur_sp=0x80d1c4a0, ra[0x80025500] , bottomMagic=0x0
prio[86 ] pc[0x80024010] state=0  [dely=0       ] top=0x80dad120  bottom=0x80dab120  cur_sp=0x80dad120, ra[0x8002adfc] , bottomMagic=0x0
prio[89 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d22300  bottom=0x80d1e300  cur_sp=0x80d222c8, ra[0x80025500] dm_v2, bottomMagic=0x0
prio[91 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d17d20  bottom=0x80d16d20  cur_sp=0x80d17ce0, ra[0x80025500] Bus monitor, bottomMagic=0x0
prio[254] pc[0x8002aa84] state=0  [dely=0       ] top=0x80afe160  bottom=0x80afa160  cur_sp=0x80afe128, ra[0x802d696c] Idle, bottomMagic=0x0
exc_stack_hi=0x808c8900 exc_stack_low=0x808c4d00 

ra:[0x80158a18]  fp:[0x00110000]  gp:[0x808bf5c8]  at:[0xfffffffe]  
t9:[0x80025iEď514]  t8:[0x0000002e]  t7:[0x80e47220]  t6:[0x00000030]  t5:[0x8080f840]  
t4:[0x0000000f]  t3:[0x0000000a]  t2:[0x00000000]  t1:[0x00000003]  t0:[0x00000003]  
s7:[0x9e35f233]  s6:[0x8004aa10]  s5:[0x80229a00]  s4:[0x82a97c00]  s3:[0x80dca1c0]  
s2:[0x00089c2b]  s1:[0x80e47220]  s0:[0x80060000]  
a3:[0x80ed0f04]  a2:[0xfffffffb]  a1:[0x00000000]  a0:[0x80ed0f03]  
v1:[0x80ed0f03 ]  v0:[0x00000064]  

!!!alloc cnt[0]
---------------Time Stamp[18:42:20]----------------
---------------Time Stamp[18:43:53]----------------
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: st ^-^
In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Jul  4 2017, 16:23:29]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 23 2017--18:43:50 symphony

 1. mem_start[80d15c90]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30941040
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D52FA0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D70040 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d1d3a0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d52fa0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate [AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Jul 19 2017 11:32:10/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80db9360 p_wifi_dev 80db9460 p_lld 80db93b0 p_lld_addr 80db9364 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a6cee0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a6cefc --------
wifi dev = 0x80db96e0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 564267 p_data_buffer 80e60220 

ASSERT:D:\Work\Vendace\Vendace_428_NewSDK_\stboxge-tech\prj\dvbs\vendace\ui\ui_init.c line 370
#AP!# exception!
Breakpoint exception
EPC[0x80158a18], CAUSE[0x10800024], SR[0x1100ff03], SP[0x80ab20b8]!

s_log_buff( 80EE9EA0) s_log_len=100

showcs 80158a18 80ab20b8 80158a18

 OSIntNesting=0 OSLockNesting=0 

 current task priority is 6, stack cur is 80ab1da0   bottom at :80aaa300  Size=8192 


 task name initT1 

stkcur=0x80ab20b8   top=0x80ab2300 


<0x80ab20a0> 0x64        0xfffffffe  0x1100ff03  0x80158a18  0x0         0x0         0x80058524  0x800583d0  
<0x80ab20c0> 0x800583e4  0x172       0x89c2b     0x80e60220  0x110000    0x8022c024  0x80ab0000  0x80d16d20  
<0x80ab20e0> 0x4000      0x807c0000  0x80050000  0x8022c024  0x0         0x0         0x80229a00  0x80126a20  
<0x80ab2100> 0x800553f4  0x807bf394  0xd0        0x80dca178  0x0         0x0         0x0         0x0         
<0x80ab2120> 0x0         0x0         0x0         0x0         0x0         0x0         0x0 iEď        0x0         
<0x80ab2140> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2160> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2180> 0x80d16d00  0x80220154  0x0         0x0         0x0         0x0         0x1100ff01  0x0         
<0x80ab21a0> 0x0         0x80a80000  0x8d2e      0x80a8ba38  0x8021ff1c  0x80223e70  0x1040      0x80ab22b8  
<0x80ab21c0> 0x20        0x1000      0x80127ba4  0x80a80000  0x80d16d20  0x80229a00  0x8022ce6c  0x80223e70  
<0x80ab21e0> 0x0         0x0         0x0         0x0         0x20        0x8022c87c  0x0         0x0         
<0x80ab2200> 0x0         0x0         0x20        0x0         0x80ab22b8  0x1000      0x80229a00  0x8022ce6c  
<0x80ab2220> 0x2a        0x5b        0x16c       0x80127d68  0x0         0x80029d38  0x0         0x0         
<0x80ab2240> 0x20        0x0         0x400       0x0         0x3         0x8022cc78  0x5b        0x80d16d20  
<0x80ab2260> iEď0x5b        0x0         0x5b        0x80d16d20  0x5b        0x802d6ab8  0x80aa13a8  0x80aa13d8  
<0x80ab2280> 0x1d81f70   0x80d16d20  0x80050000  0x80d16d20  0x80229a00  0x8022ce6c  0x80228e30  0x0         
<0x80ab22a0> 0x80050000  0x80d16d20  0x80229a00  0x8022ce6c  0x80228e30  0x0         0x0         0x0         
<0x80ab22c0> 0x0         0x80127c30  0x80055a30  0x80055a24  0x80ab22a0  0x808c0000  0x80d16d20  0x1000      
<0x80ab22e0> 0x2aea5400  0x0         0x0         0x0         0x0         0x0         0x0         0x8002adfc  
<0x80ab2300> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         

prio[6  ] pc[0x0] state=0  [dely=0       ] top=0x80ab2300  bottom=0x80aaa300  cur_sp=0x80ab1e20, ra[0x0] initT1, bottomMagic=0x0
prio[7  ] pc[0x80025500] state=32 [dely=0       ] top=0x80d16cc0  bottom=0x80d15cc0  cur_sp=0x80d16be8, ra[0x80025500] Timer, bottomMagic=0x0
prio[9  ] pc[0x8044ee10] state=0  [dely=0       ] top=0x80db9200  bottom=0x80db1200  cur_sp=0x80db9200, riEďa[0x8002adfc] tcpip_thread, bottomMagic=0x0
prio[17 ] pc[0x802e9e24] state=0  [dely=0       ] top=0x80d52f40  bottom=0x80d51f40  cur_sp=0x80d52948, ra[0x8022a2c8] usb_bus, bottomMagic=0x0
prio[53 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d1c580  bottom=0x80d18580  cur_sp=0x80d1c4a0, ra[0x80025500] , bottomMagic=0x0
prio[86 ] pc[0x80024010] state=0  [dely=0       ] top=0x80dad120  bottom=0x80dab120  cur_sp=0x80dad120, ra[0x8002adfc] , bottomMagic=0x0
prio[89 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d22300  bottom=0x80d1e300  cur_sp=0x80d222c8, ra[0x80025500] dm_v2, bottomMagic=0x0
prio[91 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d17d20  bottom=0x80d16d20  cur_sp=0x80d17ce0, ra[0x80025500] Bus monitor, bottomMagic=0x0
prio[254] pc[0x8002aa84] state=0  [dely=0       ] top=0x80afe160  bottom=0x80afa160  cur_sp=0x80afe128, ra[0x802d696c] Idle, bottomMagic=0x0
exc_stack_hi=0x808c8900 exc_stack_low=0x808c4d00 

ra:[0x80158a18]  fp:[0x00110000]  gp:[0x808bf5c8]  at:[0xfffffffe]  
t9:[0x80025514]  t8:[0x0000002e]  t7:[0x80e60220]  t6:[0x00000030]  t5:[0x8080f840]  
t4:[0x0000000f]  t3:[0x0000000a]  t2:[0x00000000]  t1:[0x00000003]  t0:[0x00000003]  
s7:[0x9e35f277]  s6:[0x8004aa10]  s5:[0x80229a00]  s4:[0x82a97c00]  s3:[0x80dca1c0]  
s2:[0x00089c2b]  s1:[0x80e60220]  s0:[0x80060000]  
a3:[0x80ee9f04]  a2:[0xfffffffb]  a1:[0x00000000]  a0:[0x80ee9f03]  
v1:[0x80ee9f03 ]  v0:[0x00000064]  

!!!alloc cnt[0]
---------------Time Stamp[18:47:20]----------------
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
---------------Time Stamp[18:48:53]----------------
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: sta^-^
In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841]cBuild Time:[Jul  4 2017, 16:23:
9]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 23 2017--18:48:20 symphony

 1. mem_start[80d15c90]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30941040
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D52FA0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D70040 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d1d3a0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d52fa0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate [AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Jul 19 2017 11:32:10/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80db9360 p_wifi_dev 80db9460 p_lld 80db93b0 p_lld_addr 80db9364 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a6cee0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a6cefc --------
wifi dev = 0x80db96e0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 564267 p_data_buffer 80f28220 

ASSERT:D:\Work\Vendace\Vendace_428_NewSDK_\stboxge-tech\prj\dvbs\vendace\ui\ui_init.c line 370
#AP!# exception!
Breakpoint exception
EPC[0x80158a18], CAUSE[0x10800024], SR[0x1100ff03], SP[0x80ab20b8]!

s_log_buff( 80FB1EA0) s_log_len=100

showcs 80158a18 80ab20b8 80158a18

 OSIntNesting=0 OSLockNesting=0 

 current task priority is 6, stack cur is 80ab1da0   bottom at :80aaa300  Size=8192 


 task name initT1 

stkcur=0x80ab20b8   top=0x80ab2300 


<0x80ab20a0> 0x64        0xfffffffe  0x1100ff03  0x80158a18  0x0         0x0         0x80058524  0x800583d0  
<0x80ab20c0> 0x800583e4  0x172       0x89c2b     0x80f28220  0x110000    0x8022c024  0x80ab0000  0x80d16d20  
<0x80ab20e0> 0x4000      0x807c0000  0x80050000  0x8022c024  0x0         0x0         0x80229a00  0x80126a20  
<0x80ab2100> 0x800553f4  0x807bf394  0xd0        0x80dca178  0x0         0x0         0x0         0x0         
<0x80ab2120> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2140> 0x0         0x0         0xiEď0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2160> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2180> 0x80d16d00  0x80220154  0x0         0x0         0x0         0x0         0x1100ff01  0x0         
<0x80ab21a0> 0x0         0x80a80000  0x8d2e      0x80a8ba38  0x8021ff1c  0x80223e70  0x1040      0x80ab22b8  
<0x80ab21c0> 0x20        0x1000      0x80127ba4  0x80a80000  0x80d16d20  0x80229a00  0x8022ce6c  0x80223e70  
<0x80ab21e0> 0x0         0x0         0x0         0x0         0x20        0x8022c87c  0x0         0x0         
<0x80ab2200> 0x0         0x0         0x20        0x0         0x80ab22b8  0x1000      0x80229a00  0x8022ce6c  
<0x80ab2220> 0x2a        0x5b        0x16c       0x80127d68  0x0         0x80029d38  0x0         0x0         
<0x80ab2240> 0x20        0x0         0x400       0x0         0x3         0x8022cc78  0x5b        0x80d16d20  
<0x80ab2260> 0x5b        0x0         0x5b        0x80d16d20  0x5b        iEď0x802d6ab8  0x80aa13a8  0x80aa13d8  
<0x80ab2280> 0x1d81f70   0x80d16d20  0x80050000  0x80d16d20  0x80229a00  0x8022ce6c  0x80228e30  0x0         
<0x80ab22a0> 0x80050000  0x80d16d20  0x80229a00  0x8022ce6c  0x80228e30  0x0         0x0         0x0         
<0x80ab22c0> 0x0         0x80127c30  0x80055a30  0x80055a24  0x80ab22a0  0x808c0000  0x80d16d20  0x1000      
<0x80ab22e0> 0x2aea5400  0x0         0x0         0x0         0x0         0x0         0x0         0x8002adfc  
<0x80ab2300> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         

prio[6  ] pc[0x0] state=0  [dely=0       ] top=0x80ab2300  bottom=0x80aaa300  cur_sp=0x80ab1e20, ra[0x0] initT1, bottomMagic=0x0
prio[7  ] pc[0x80025500] state=32 [dely=0       ] top=0x80d16cc0  bottom=0x80d15cc0  cur_sp=0x80d16be8, ra[0x80025500] Timer, bottomMagic=0x0
prio[9  ] pc[0x8044ee10] state=0  [dely=0       ] top=0x80db9200  bottom=0x80db1200  cur_sp=0x80db9200, ra[0x8002adfc] tcpip_thread, bottomMagic=0x0
prio[17 ] pc[0x8iEď02e9e28] state=0  [dely=0       ] top=0x80d52f40  bottom=0x80d51f40  cur_sp=0x80d52948, ra[0x8022a2c8] usb_bus, bottomMagic=0x0
prio[53 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d1c580  bottom=0x80d18580  cur_sp=0x80d1c4a0, ra[0x80025500] , bottomMagic=0x0
prio[86 ] pc[0x80024010] state=0  [dely=0       ] top=0x80dad120  bottom=0x80dab120  cur_sp=0x80dad120, ra[0x8002adfc] , bottomMagic=0x0
prio[89 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d22300  bottom=0x80d1e300  cur_sp=0x80d222c8, ra[0x80025500] dm_v2, bottomMagic=0x0
prio[91 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d17d20  bottom=0x80d16d20  cur_sp=0x80d17ce0, ra[0x80025500] Bus monitor, bottomMagic=0x0
prio[254] pc[0x8002aa84] state=0  [dely=0       ] top=0x80afe160  bottom=0x80afa160  cur_sp=0x80afe128, ra[0x802d696c] Idle, bottomMagic=0x0
exc_stack_hi=0x808c8900 exc_stack_low=0x808c4d00 

ra:[0x80158a18]  fp:[0x00110000]  gp:[0x808bf5c8]  at:[0xfffffffe]  
t9:[0x80025514]  t8:[0x0000002e]  t7:[0x80f28220]  t6:[0x00000030]  t5:[0x8080f840]  
t4:[0x0000000f]  t3:[0x0000000a]  t2:[0x00000000]  t1:[0x00000003]  t0:[0x00000003]  
s7:[0x9e35f177]  s6:[0x8004aa10]  s5:[0x80229a00]  s4:[0x82a97c00]  s3:[0x80dca1c0]  
s2:[0x00089c2b]  s1:[0x80f28220]  s0:[0x80060000]  
a3:[0x80fb1f04]  a2:[0xfffffffb]  a1:[0x00000000]  a0:[0x80fb1f03]  
v1:[0x80fb1f03 ]  v0:[0x00000064]  

!!!alloc cnt[0]
---------------Time Stamp[18:52:20]----------------
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
---------------Time Stamp[18:53:53]----------------
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CBCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: sta^-^ In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Jul  4 2017, 16:23:
9]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 23 2017--18:52:42 symphony

 1. mem_start[80d15c90]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30941040
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D52FA0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D70040 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d1d3a0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d52fa0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Jul 19 2017 11:32:10/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80db9360 p_wifi_dev 80db9460 p_lld 80db93b0 p_lld_addr 80db9364 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a6cee0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a6cefc --------
wifi dev = 0x80db96e0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 564267 p_data_buffer 80f28220 

ASSERT:D:\Work\Vendace\Vendace_428_NewSDK_\stboxge-tech\prj\dvbs\vendace\ui\ui_init.c line 370
#AP!# exception!
Breakpoint exception
EPC[0x80158a10], CAUSE[0x10800024], SR[0x1100ff03], SP[0x80ab20b8]!

s_log_buff( 80FB1EA0) s_log_len=100

showcs 80158a10 80ab20b8 80158a10

 OSIntNesting=0 OSLockNesting=0 

 current task priority is 6, stack cur is 80ab1da0   bottom at :80aaa300  Size=8192 


 task name initT1 

stkcur=0x80ab20b8   top=0x80ab2300 


<0x80ab20a0> 0x64        0xfffffffe  0x1100ff03  0x80158a10  0x0         0x0         0x80058524  0x800583d0  
<0x80ab20c0> 0x800583e4  0x172       0x89c2b     0x80f28220  0x110000    0x8022c01c  0x80ab0000  0x80d16d20  
<0x80ab20e0> 0x4000      0x807c0000  0x80050000  0x8022c01c  0x0         0x0         0x802299f8  0x80126a20  
<0x80ab2100> 0x800553f4  0x807bf38c  0xd0        0x80dca178  0x0         0x0         0x0         0x0         
<0x80ab2120> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2140> 0x0         0x0 iEď        0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2160> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2180> 0x80d16d00  0x8022014c  0x0         0x0         0x0         0x0         0x1100ff01  0x0         
<0x80ab21a0> 0x0         0x80a80000  0x8d2e      0x80a8ba38  0x8021ff14  0x80223e68  0x1040      0x80ab22b8  
<0x80ab21c0> 0x20        0x1000      0x80127b9c  0x80a80000  0x80d16d20  0x802299f8  0x8022ce64  0x80223e68  
<0x80ab21e0> 0x0         0x0         0x0         0x0         0x20        0x8022c874  0x0         0x0         
<0x80ab2200> 0x0         0x0         0x20        0x0         0x80ab22b8  0x1000      0x802299f8  0x8022ce64  
<0x80ab2220> 0x2a        0x5b        0x16c       0x80127d60  0x0         0x80029d38  0x0         0x0         
<0x80ab2240> 0x20        0x0         0x400       0x0         0x3         0x8022cc70  0x5b        0x80d16d20  
<0x80ab2260> 0x5b        0x0         0x5b        0x80d16d20  0xiEď5b        0x802d6ab0  0x80aa13a8  0x80aa13d8  
<0x80ab2280> 0x1d81f70   0x80d16d20  0x80050000  0x80d16d20  0x802299f8  0x8022ce64  0x80228e28  0x0         
<0x80ab22a0> 0x80050000  0x80d16d20  0x802299f8  0x8022ce64  0x80228e28  0x0         0x0         0x0         
<0x80ab22c0> 0x0         0x80127c28  0x80055a30  0x80055a24  0x80ab22a0  0x808c0000  0x80d16d20  0x1000      
<0x80ab22e0> 0x2aea5400  0x0         0x0         0x0         0x0         0x0         0x0         0x8002adfc  
<0x80ab2300> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         

prio[6  ] pc[0x0] state=0  [dely=0       ] top=0x80ab2300  bottom=0x80aaa300  cur_sp=0x80ab1e20, ra[0x0] initT1, bottomMagic=0x0
prio[7  ] pc[0x80025500] state=32 [dely=0       ] top=0x80d16cc0  bottom=0x80d15cc0  cur_sp=0x80d16be8, ra[0x80025500] Timer, bottomMagic=0x0
prio[9  ] pc[0x8044ee08] state=0  [dely=0       ] top=0x80db9200  bottom=0x80db1200  cur_sp=0x80db9200, ra[0x8002adfc] tcpip_thread, bottomMagic=0x0
prio[1iEď7 ] pc[0x802e9e1c] state=0  [dely=0       ] top=0x80d52f40  bottom=0x80d51f40  cur_sp=0x80d52948, ra[0x8022a2c0] usb_bus, bottomMagic=0x0
prio[53 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d1c580  bottom=0x80d18580  cur_sp=0x80d1c4a0, ra[0x80025500] , bottomMagic=0x0
prio[86 ] pc[0x80024010] state=0  [dely=0       ] top=0x80dad120  bottom=0x80dab120  cur_sp=0x80dad120, ra[0x8002adfc] , bottomMagic=0x0
prio[89 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d22300  bottom=0x80d1e300  cur_sp=0x80d222c8, ra[0x80025500] dm_v2, bottomMagic=0x0
prio[91 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d17d20  bottom=0x80d16d20  cur_sp=0x80d17ce0, ra[0x80025500] Bus monitor, bottomMagic=0x0
prio[254] pc[0x8002aa84] state=0  [dely=0       ] top=0x80afe160  bottom=0x80afa160  cur_sp=0x80afe128, ra[0x802d6964] Idle, bottomMagic=0x0
exc_stack_hi=0x808c8900 exc_stack_low=0x808c4d00 

ra:[0x80158a10]  fp:[0x00110000]  gp:[0x808bf5c8]  at:[0xfffffffe]  
t9:[0x80025514]  t8:[0x0000002e]  t7:[0x80f28220]  t6:[0x00000030]  t5:[0x8080f838]  
t4:[0x0000000f]  t3:[0x0000000a]  t2:[0x00000000]  t1:[0x00000003]  t0:[0x00000003]  
s7:[0x9e35f24b]  s6:[0x8004aa10]  s5:[0x802299f8]  s4:[0x82a97c00]  s3:[0x80dca1c0]  
s2:[0x00089c2b]  s1:[0x80f28220]  s0:[0x80060000]  
a3:[0x80fb1f04]  a2:[0xfffffffb]  a1:[0x00000000]  a0:[0x80fb1f03]  
v1:[0x80fb1f03 ]  v0:[0x00000064]  

!!!alloc cnt[0]
Serial Port Closed
upg or dump task  is canceled!
monitor stop
Serial Port Opened
monitor start
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
---------------Time Stamp[18:57:20]----------------
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: st ^-^
In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Jul  4 2017, 16:23:29]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 23 2017--18:55:55 symphony

 1. mem_start[80d15c90]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30941040
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D52FA0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D70040 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d1d3a0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d52fa0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Jul 19 2017 11:32:10/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80db9360 p_wifi_dev 80db9460 p_lld 80db93b0 p_lld_addr 80db9364 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a6cee0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a6cefc --------
wifi dev = 0x80db96e0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 564267 p_data_buffer 80fca220 

ASSERT:D:\Work\Vendace\Vendace_428_NewSDK_\stboxge-tech\prj\dvbs\vendace\ui\ui_init.c line 370
#AP!# exception!
Breakpoint exception
EPC[0x80158a04], CAUSE[0x10800024], SR[0x1100ff03], SP[0x80ab20b8]!

s_log_buff( 81053EA0) s_log_len=100

showcs 80158a04 80ab20b8 80158a04

 OSIntNesting=0 OSLockNesting=0 

 current task priority is 6, stack cur is 80ab1da0   bottom at :80aaa300  Size=8192 


 task name initT1 

stkcur=0x80ab20b8   top=0x80ab2300 


<0x80ab20a0> 0x64        0xfffffffe  0x1100ff03  0x80158a04  0x0         0x0         0x80058524  0x800583d0  
<0x80ab20c0> 0x800583e4  0x172       0x89c2b     0x80fca220  0x110000    0x8022c010  0x80ab0000  0x80d16d20  
<0x80ab20e0> 0x4000      0x807c0000  0x80050000  0x8022c010  0x0         0x0         0x802299ec  0x80126a20  
<0x80ab2100> 0x800553f4  0x807bf384  0xd0        0x80dca178  0x0         0x0         0x0         0x0         
<0x80ab2120> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0    iEď     
<0x80ab2140> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2160> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80ab2180> 0x80d16d00  0x80220140  0x0         0x0         0x0         0x0         0x1100ff01  0x0         
<0x80ab21a0> 0x0         0x80a80000  0x8d2e      0x80a8ba38  0x8021ff08  0x80223e5c  0x1040      0x80ab22b8  
<0x80ab21c0> 0x20        0x1000      0x80127b9c  0x80a80000  0x80d16d20  0x802299ec  0x8022ce58  0x80223e5c  
<0x80ab21e0> 0x0         0x0         0x0         0x0         0x20        0x8022c868  0x0         0x0         
<0x80ab2200> 0x0         0x0         0x20        0x0         0x80ab22b8  0x1000      0x802299ec  0x8022ce58  
<0x80ab2220> 0x2a        0x5b        0x16c       0x80127d60  0x0         0x80029d38  0x0         0x0         
<0x80ab2240> 0x20        0x0         0x400       0x0         0x3         0x8022cc64  0x5b        0x80d16d20  
<0x80ab2260> 0x5b        0x0iEď         0x5b        0x80d16d20  0x5b        0x802d6aa4  0x80aa13a8  0x80aa13d8  
<0x80ab2280> 0x1d81f70   0x80d16d20  0x80050000  0x80d16d20  0x802299ec  0x8022ce58  0x80228e1c  0x0         
<0x80ab22a0> 0x80050000  0x80d16d20  0x802299ec  0x8022ce58  0x80228e1c  0x0         0x0         0x0         
<0x80ab22c0> 0x0         0x80127c28  0x80055a30  0x80055a24  0x80ab22a0  0x808c0000  0x80d16d20  0x1000      
<0x80ab22e0> 0x2aea5400  0x0         0x0         0x0         0x0         0x0         0x0         0x8002adfc  
<0x80ab2300> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         

prio[6  ] pc[0x0] state=0  [dely=0       ] top=0x80ab2300  bottom=0x80aaa300  cur_sp=0x80ab1e20, ra[0x0] initT1, bottomMagic=0x0
prio[7  ] pc[0x80025500] state=32 [dely=0       ] top=0x80d16cc0  bottom=0x80d15cc0  cur_sp=0x80d16be8, ra[0x80025500] Timer, bottomMagic=0x0
prio[9  ] pc[0x8044edfc] state=0  [dely=0       ] top=0x80db9200  bottom=0x80db1200  cur_sp=0x80db9200, ra[0x8002adfc] tiEďcpip_thread, bottomMagic=0x0
prio[17 ] pc[0x802e9e10] state=0  [dely=0       ] top=0x80d52f40  bottom=0x80d51f40  cur_sp=0x80d52948, ra[0x8022a2b4] usb_bus, bottomMagic=0x0
prio[53 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d1c580  bottom=0x80d18580  cur_sp=0x80d1c4a0, ra[0x80025500] , bottomMagic=0x0
prio[86 ] pc[0x80024010] state=0  [dely=0       ] top=0x80dad120  bottom=0x80dab120  cur_sp=0x80dad120, ra[0x8002adfc] , bottomMagic=0x0
prio[89 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d22300  bottom=0x80d1e300  cur_sp=0x80d222c8, ra[0x80025500] dm_v2, bottomMagic=0x0
prio[91 ] pc[0x80025500] state=0  [dely=0       ] top=0x80d17d20  bottom=0x80d16d20  cur_sp=0x80d17ce0, ra[0x80025500] Bus monitor, bottomMagic=0x0
prio[254] pc[0x8002aa84] state=0  [dely=0       ] top=0x80afe160  bottom=0x80afa160  cur_sp=0x80afe128, ra[0x802d6958] Idle, bottomMagic=0x0
exc_stack_hi=0x808c8900 exc_stack_low=0x808c4d00 

ra:[0x80158a04]  fp:[0x00110000]  gp:[0x808bf5c8]  at:[0xfffffffe]  
t9:[0x80025514]  t8:[0x0000002e]  t7:[0x80fca220]  t6:[0x00000030]  t5:[0x8080f830]  
t4:[0x0000000f]  t3:[0x0000000a]  t2:[0x00000000]  t1:[0x00000003]  t0:[0x00000003]  
s7:[0x9e35f2f3]  s6:[0x8004aa10]  s5:[0x802299ec]  s4:[0x82a97c00]  s3:[0x80dca1c0]  
s2:[0x00089c2b]  s1:[0x80fca220]  s0:[0x80060000]  
a3:[0x81053f04]  a2:[0xfffffffb]  a1:[0x00000000]  a0:[0x81053f03]  
v1:[0x81053f03 ]  v0:[0x00000064]  

!!!alloc cnt[0]
---------------Time Stamp[18:58:53]----------------
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
---------------Time Stamp[19:02:20]----------------
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: st ^-^
In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Jul  4 2017, 16:23:29]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 23 2017--18:59:06 symphony

 1. mem_start[80d15c90]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30941040
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D52FA0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D70040 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d1d3a0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d52fa0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Jul 19 2017 11:32:10/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80db9360 p_wifi_dev 80db9460 p_lld 80db93b0 p_lld_addr 80db9364 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a6cee0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a6cefc --------
wifi dev = 0x80db96e0 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 439550 p_data_buffer 80e47220 

 unzip resource. in_addr = 0x9e35f27b, out_addr = 0x82a97c00, in_len = 439550, out_len = 1080544
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:247
[AI][_ai_eva_init]Entry...ticks:248
[AI][_ai_tuner_init]Entry...ticks:248
[AI][_ai_dvb_init]Entry...ticks:269
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:269
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:292
[AI][_ai_iconv_init]Entry...ticks:292
[AI][_ai_antenna_lnb_init]Entry...ticks:292
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:293
[AI][_ai_time_init]Entry...ticks:327
eve0
[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80d51aa0
hub_add_new_dev 80e8c3c0
port_reset 80d51aa0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x83f9dc00
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
on_factory_test_uart LINE:[204]
welcome toon_factory_test_uart LINE:[231]
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
-----ui show logo v2 size 0xd599, 0, 179
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2620192, alloced_peak = 2700544, rest_size = 28320848

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 159 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x21]
[USB]ui_upg_file_list_get:valid_file_cnt[0x9]

## timeshift exist is [1393786880]
p_cont[0x80ea9278], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
update signal
---------------Time Stamp[19:03:53]----------------
