---------------Time Stamp[10:09:01]----------------
---------------Time Stamp[10:14:01]----------------
Serial Port Opened
monitor start
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

4194304 bytes read
do_spi_flash_uboot_save offset[0] len[400000]
spi0 is already setup!!!
SF: spi flash status register: 0x00, 0x00
SPI: Detected IS25LP128 with erase size 64 KiB, total 16 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBBBB99BBV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=213990 213974 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x880005c, status=0x1b02
avcpu ver = AVCPU_VERSION:[501:723fde4cc841] Build Time:[Jul  4 2017, 
6:23:47]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b0d 48
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--16:07:45 symphony

 1. mem_start[8095b5c0]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 9035328
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[flash_pro] This flash can't be protected!!!
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:13
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:14
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:18
[AI][_ai_video_init]Entry...ticks:18
[AI][_ai_usb_init]Entry...ticks:22
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80999540 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 809B65E0 [AI][_ai_dmx_init]Entry...ticks:23
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:25
priv->cfg.p_dem_bus =0x809638e0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80999540


 ###step3### msg.event 2
[AI][_ai_mute_set]Entry...ticks:148
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c40000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d40000], size[180000], align[400], cfg size[1c01000]
tcpip: Aug 25 2017 19:23:17/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:152
file_size 313141 p_data_buffer 80a92d20 

 unzip resource. in_addr = 0x9e297d07, out_addr = 0x811f9400, in_len = 313141, out_len = 905568
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:181
[AI][_ai_eva_init]Entry...ticks:182
[AI][_ai_tuner_init]Entry...ticks:182
[AI][_ai_dvb_init]Entry...ticks:203
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:203
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:219
[AI][_ai_iconv_init]Entry...ticks:219
[AI][_ai_antenna_lnb_init]Entry...ticks:219
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:220
[AI][_ai_time_init]Entry...ticks:254
eve0
[AI][ap_init]End...
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 80998040
hub_add_new_dev 80b9e9a0
port_reset 80998040
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x818d0400
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_iEwsubt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 0 to 2 
switch_autoclose: de&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
stroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2640096, alloced_peak = 2641088, rest_size = 6395232

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 160 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0xb]
[USB]ui_upg_file_list_get:valid_file_cnt[0x5]
p_cont[0x80af49d8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
update signal

## timeshift exist is [1393786880]
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80999540


 ###step3### msg.event 3
###ui_nw_api_on_plug_out dev_type[1]
p_cont[0x80af49d8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
thread usb_stor_control_thread exit
usb_bus notify device REMOVE 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
update signal
---------------Time Stamp[10:19:01]----------------
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80999540


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 80998040
hub_add_new_dev 80b9e9a0
port_reset 80998040
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8001205
###step1.2### 0 usb_hcd_poll_rh_status 
   #3device ADD cost 161 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0xb]
[USB]ui_upg_file_list_get:valid_file_cnt[0x5]
p_cont[0x80af49d8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
[USB]ui_upg_file_list_get:file count[0xb]
[USB]ui_upg_file_list_get:valid_file_cnt[0x5]
_switch_playstatus
from_id = 2 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 47 
UI: deactive playback.........
update signal

## timeshift exist is [1393786880]
p_cont[0x80af4d3c], root[0]
_switch_playstatus
from_id = 47 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 24 
_switch_playstatus
from_id = 47 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 47 
p_cont[0x80af4d3c], root[0]
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB9B9BBBV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=214127 214111 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x18800000, status=0xff01
avcpu ver = AVCPU_VERSION:[490:0584ac198239] Build Time:[Jun 20 2017,
14:01:31]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b8e 48
[FastLogo][ap_init:964]Entry...
[FastLogo][_ai_dm_init]Entry...ticks:0
[FastLogo][_ai_dm_init]dm init v2...ticks:0
[FastLogo][_ai_dm_init]set header...ticks:0
[FastLogo][ap_init:1017]End...
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 3. sys partition size(free_mem) 9934168
**CDU UDQ**: 8b8e 48
[AI]chip id:1
[flash_pro] This flash can't be protected!!!
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 809B2E20 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 809CFEC0 priv->cfg.p_dem_bus =0x8096d180
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809b2e20


 ###step3### msg.event 2
tcpip: May 25 2017 17:28:55/nthread task for ethernet 9 
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
**LCK UDQ**: 2ab6
[AI][_ai_mdl_init]Software Ver[1000000]
eve223
mmi ver 395:d339c83370c6
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 809b1920
hub_add_new_dev 80bec520
port_reset 809b1920
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
EMON>    #3device ADD cost 160 ts 
---------------Time Stamp[10:24:02]----------------
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809b2e20


 ###step3### msg.event 3
thread usb_stor_control_thread exit
usb_bus notify device REMOVE 
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809b2e20


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 809b1920
hub_add_new_dev 80bec520
port_reset 809b1920
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8001205
###step1.2### 0 usb_hcd_poll_rh_status 
   #3device ADD cost 629 ts 
---------------Time Stamp[10:29:02]----------------
enter wifi_wpa_supplicant_task tick:53455
>>>wpa_start_loop
>>>STEP 2

global=0x80c2e4e0,wpa_start_loop

>>>STEP 2-1
wpa_supplicant_add_iface,3238
g_wifi_vendor_name##2
wpa_net_dev##0
g_wifi_vendor_name##2
wpa_net_dev##0
wpa_supplicant_add_iface,3268

wpa_supplicant_add_iface004

wpa_supplicant_add_iface005
WIFI State: DISCONNECTED -> DISCONNECTED
WIFI State: 0 -> 0;8->9

###############wpa connect NG 53490 ############

Added interface wlan0eloop_run 751 tick:53491
WIFI State: DISCONNECTED -> ASSOCIATING
WIFI State: 0 -> 5;8->9
WIFI State: ASSOCIATING -> ASSOCIATED
WIFI State: 5 -> 6;8->9
WIFI State: ASSOCIATED -> 4WAY_HANDSHAKE
WIFI State: 6 -> 7;8->9
WPA: RX message 1 of 4-Way Handshake from a4:2b:8c:91:ca:fc (ver=2)##1/4 4-Way Handshake D:\Mars\Peon_111\release\MainBranchDev_Drv\stboxge-tech\src\kware\network\wpa\wpa.c::wpa_sm_rx_eapol,1848
WIFI State: 4WAY_HANDSHAKE -> 4WAY_HANDSHAKE
WIFI State: 7 -> 7;8->9
WIFI State: 4WAY_HANDSHAKE -> GROUP_HANDSHAKE
WIFI State: 7 -> 8;8->9
complete#######wpa###############3
WIFI State: GROUP_HANDSHAKE -> COMPLETED
WIFI State: 8 -> 9;8->9

###############wpa connect OK 53559############

[file_seq_create] start start ...
[file_seq_create] [changeset:   35726:ed8dd7d3f9c6 and current parents changeset:   35726:ed8dd7d3f9c6] ...
[file_seq_create] unknow driver branch !!!!!!!!!!!!!!!!!..
[file_seq_create] Player Support Network Stream  !!!!
[file_seq_create] pb_seq_mem_size[4063232] ...
[file_seq_create] pb_seq_mem_start[0x815d0400] ...
[file_seq_create] stack_start[0x819b0400] ...
[file_seq_create] stack_size[131072] ...
[file_seq_create] task_priority[27] ...
[file_seq_create] stack_preload_size[131072] ...
[file_seq_create] task_preload_priority[26] ...
[file_seq_create] vdec_policy[1] ...

get_chip_type 7593 chip type:4
[file_seq_create]----------value[0x0]
[file_seq_create]----------value[0]
[file_seq_create] disable_avsync[0]
[file_seq_create] stop stop ...
[x_get_av_dec_cap] ves 3145728 aes 131072...
[file_seq_register_cb] start start ...
[file_seq_register_cb] end end ...
[NetMedia_initDataProvider] start start ...
[DP_startDoCmdTask] statck size :65536...
[x_push_cmd] end end ...
 [NetMedia_initDataProvider] end end ...
[x_pop_cmd][OK] end end ...
 [get_drv_hg_version] [changeset:   36081:4a3fcf80078a] ...
[get_drv_hg_version] [commit 901435fe0a3127025319d2418df8ed57b764ecdc] ...
[get_drv_hg_version] [version = 36081] ...
[x_push_cmd] end end ...
 [x_pop_cmd][OK] end end ...
 [NetMedia_deinitDataProvider] start start ...
[x_clear_fifo] start start ...
 [x_clear_fifo] end end ...
 [do_NetMedia_deinitWebsite_cmd] deinit end ! ...
[NetMedia_deinitDataProvider] destory  p_website_info ...
tmp file r:website_info is not exist
[NetMedia_deinitDataProvider] end end ...
[file_seq_destroy] start start ...
[file_seq_force_stop] start start ...

@@@@modify_sockets 259 
[file_seq_force_stop] do nothing...
[file_seq_force_stop] state[1].
[aud_sync_switch]--- file_playback av sync is on
[file_seq_force_stop] stop stop ...
[file_seq_destroy] stop stop ...
[file_seq_create] start start ...
[file_seq_create] [changeset:   35726:ed8dd7d3f9c6 and current parents changeset:   35726:ed8dd7d3f9c6] ...
[file_seq_create] unknow driver branch !!!!!!!!!!!!!!!!!..
[file_seq_create] Player Support Network Stream  !!!!
[file_seq_create] pb_seq_mem_size[4063232] ...
[file_seq_create] pb_seq_mem_start[0x815d0400] ...
[file_seq_create] stack_start[0x819b0400] ...
[file_seq_create] stack_size[131072] ...
[file_seq_create] task_priority[27] ...
[file_seq_create] stack_preload_size[131072] ...
[file_seq_create] task_preload_priority[26] ...
[file_seq_create] vdec_policy[1] ...

get_chip_type 7593 chip type:4
[file_seq_create]----------value[0x0]
[file_seq_create]----------value[0]
[file_seq_create] disable_avsync[0]
[file_seq_create] stop stop ...
[x_get_av_dec_cap] ves 3145728 aes 131072...
[file_seq_register_cb] start start ...
[file_seq_register_cb] end end ...
[DP_startDoCmdTask] statck size :65536...
[x_push_cmd] end end ...
 [x_pop_cmd][OK] end end ...
 [get_drv_hg_version] [changeset:   36081:4a3fcf80078a] ...
[get_drv_hg_version] [commit 901435fe0a3127025319d2418df8ed57b764ecdc] ...
[get_drv_hg_version] [version = 36081] ...
[Nw_Http_Download_Start] connect error
[Nw_Http_Download_Start] connect error
[Nw_Http_Download_Start] connect error
[Nw_Http_Download_Start] connect error
[Nw_Http_Download_Start] connect error
[Nw_Http_Download_Start] connect error
lws add [open_xstream_inputbox]function [234]line
--- [ on_edit_dns_addr ] -- Line [368] ---
--- [ on_edit_dns_addr ] -- Line [374] ---
--- [ on_edit_dns_addr ] -- Line [368] ---
--- [ on_edit_dns_addr ] -- Line [374] ---
---------------Time Stamp[10:34:02]----------------
--- [ edit_dns_addr_update ] -- Line [353] ---
[x_push_cmd] end end ...
 [x_pop_cmd][OK] end end ...
  gosat.2580.fr 80 chntst1 chnamy
lws add [on_xstream_confirm]function [177]line [url=gosat.2580.fr&port=80&username=chntst1&password=chnamy]url
lws add [al_livetv_dp_app_init]function [759]line [url=gosat.2580.fr&port=80&username=chntst1&password=chnamy]url [46223452]type@@@@@@@@@@@
lws add [al_livetv_dp_app_init]function [794]line [url=gosat.2580.fr&port=80&username=chntst1&password=chnamy]url@@@@@@@@@@@
lws add [al_livetv_dp_app_init]function [796]line [url=gosat.2580.fr&port=80&username=chntst1&password=chnamy]url@@@@@@@@@@@
[x_push_cmd] end end ...
 [x_pop_cmd][OK] end end ...
 
ASSERT:commonData.cpp line 2977
#AP!# exception!
Breakpoint exception
EPC[0x8041d8dc], CAUSE[0x10800024], SR[0x1100ff03], SP[0x80e4d028]!

s_log_buff( 80ECFD60) s_log_len=37

showcs 8041d8dc 80e4d028 8041d8dc

 OSIntNesting=0 OSLockNesting=0 

 current task priority is 34, stack cur is 80e4bfe0   bottom at :80e3dbc0  Size=16384 


 task name do command task for dp 

stkcur=0x80e4d028   top=0x80e4dbc0 


<0x80e4d020> 0x0         0x0         0x0         0x806aa9b8  0x806aa8a4  0xba1       0x0         0x0         
<0x80e4d040> 0x0         0x0         0x3a0072    0x620061    0x61006f    0x640072    0x69005f    0x740070    
<0x80e4d060> 0x310076    0x5f0032    0x6d0078    0x6c        0x0         0x0         0x0         0x0         
<0x80e4d080> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d0a0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d0c0> 0x0         0x0         0x0         0x0         0x0         0x0         iEw0x0         0x0         
<0x80e4d0e0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d100> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d120> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d140> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d160> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d180> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d1a0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d1c0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d1e0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d2iEw00> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d220> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d240> 0x0         0x0         0x0         0x0         0x0         0x806acdf0  0x80037e10  0x806ad2e0  
<0x80e4d260> 0xa1d40008  0x80038850  0x80de5c20  0x3         0x80e4d4e8  0x80427cbc  0x0         0x80e4d288  
<0x80e4d280> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d2a0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d2c0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d2e0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d300> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d320> 0x0         0x0         0x0   iEw      0x0         0x0         0x0         0x0         0x0         
<0x80e4d340> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d360> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d380> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d3a0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d3c0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d3e0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d400> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d420> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d440> 0x0         0x0         0x0         0x0         0xa1d40008  0x80305f70  0x0         0x80e4d7c8  
<0x80e4d460> 0x806acdf0  0x80e4d7c8  0x80182e84  0x8041adb4  0x800300d0  0xfffffffe  0x80e4d7c8  0x8080170c  
<0x80e4d480> 0x0         0x0         0x0         0x0         0x80e4d4e8  0x80e4d648  0x80037e10  0x806acdf0  
<0x80e4d4a0> 0xa1d40008  0x80038850  0x80de5c20  0x0         0x0         0x80428064  0x3         0xfffffffe  
<0x80e4d4c0> 0xa1d40008  0x80e4d648  0x3         0x0         0x0         0x0         0x0         0x0         
<0x80e4d4e0> 0x1100ff01  0x7465675b  0x68747561  0x0         0x0         0x0         0x0         0x0         
<0x80e4d500> 0x0         0x0         0x74617473  0x7375      0x0         0x0         0x0         0x0         
<0x80e4d520> 0x0         0x0         0x5f707865  0x65746164  0x0         0x0         0x0         0x0         
<0x80e4d540> 0x0         0x0         0x2e2e2e20  0x200a      0x0         0x0         0x0     iEw    0x0         
<0x80e4d560> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d580> 0x0         0x0         0x0         0x0         0x0         0x0         0x80e4dae4  0x0         
<0x80e4d5a0> 0x806aaa14  0x80e4dae4  0x80e4d5dc  0xa07f8ce0  0x80e4f06c  0x0         0x807f6f48  0x0         
<0x80e4d5c0> 0x0         0x80183728  0x0         0x0         0x0         0x0         0x1100ff01  0x705f785b  
<0x80e4d5e0> 0x635f706f  0x5b5d646d  0x205d4b4f  0x20646e65  0x20646e65  0xa2e2e2e   0x20        0x0         
<0x80e4d600> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d620> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d640> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d660> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d680> 0x0 iEw        0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d6a0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d6c0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d6e0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d700> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d720> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d740> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d760> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d780> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4d7a0> 0x0         0x0         0x0         0xiEw0         0x0         0x0         0x0         0x0         
<0x80e4d7c0> 0x0         0x0         0x70747468  0x672f2f3a  0x7461736f  0x3835322e  0x72662e30  0x2f30383a  
<0x80e4d7e0> 0x656e6170  0x70615f6c  0x68702e69  0x73753f70  0x616e7265  0x633d656d  0x73746e68  0x70263174  
<0x80e4d800> 0x77737361  0x3d64726f  0x616e6863  0x8000796d  0x0         0x80010984  0x0         0x0         
<0x80e4d820> 0x0         0x0         0x80e4d888  0x80aac8a0  0x8e        0x80010c40  0x80058600  0x8e        
<0x80e4d840> 0x8e0000    0x80de5780  0x0         0x1         0x71c00000  0x80de5780  0x0         0x0         
<0x80e4d860> 0x0         0x0         0x80050000  0x80de5860  0x90        0x8011b8b4  0x0         0x0         
<0x80e4d880> 0x0         0x0         0x8e0000    0x80de5780  0x80de5700  0x8017b000  0x0         0x0         
<0x80e4d8a0> 0x0         0x0         0x1100ff01  0x0         0x0         0x0         0x0         0x0         
<0x80e4d8c0> 0x0         0x0         0x40        0x80e4d9c8  0x1a        0x6         0x8041e4cc  0x40        
<0x80e4d8e0> 0x0         0x0         0x80de5700  0x8017cfb8  0x80de5db8  0x80182e84  0x806c0000  0x8017de8c  
<0x80e4d900> 0x20        0x80185cd8  0x13        0xd         0x8041c808  0x40        0x20        0x90        
<0x80e4d920> 0x80e4d9c8  0x6         0x80038ad0  0x8041b7c8  0x80037e10  0x0         0x80de5c20  0x80186068  
<0x80e4d940> 0x80e4dc20  0x80e4da68  0x8041b7c8  0x8017de8c  0x20        0x0         0x80e4da00  0x6         
<0x80e4d960> 0x80e4d9c8  0x801860d4  0x80de5780  0x8041c7ac  0x80de5c20  0x80186068  0x80e4da20  0x90        
<0x80e4d980> 0x80037e10  0x8041b7c8  0x20        0x0         0x0         0x806ab0fc  0x80038ad0  0x8041b7c8  
<0x80e4d9a0> 0x80037e10  0x0         0x80de5c20  0x0         0x0         0x80186280  0x80e4da20  0x801860d4  
<0x80e4d9c0> 0x80017de0  0x0         0x0         0x80de5c20  0x80037e10  0x8041b7c8  0x80037e10  0x0 iEw        
<0x80e4d9e0> 0x80de5c20  0x8042c400  0x80e4dc20  0x80e4dc20  0x80e4dc28  0x8017de8c  0x19999999  0x0         
<0x80e4da00> 0x0         0x806aa7ea  0x1         0x0         0x0         0x1100ff01  0x29        0x22        
<0x80e4da20> 0x80819fd8  0x0         0x80e4dba8  0x80423b40  0x1100ff00  0x80017de0  0x280       0x230       
<0x80e4da40> 0x8041b7c8  0x80037e10  0x0         0x0         0xa         0x0         0x0         0x0         
<0x80e4da60> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4da80> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4daa0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4dac0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4dae0> 0x801821bc  0x80e4dc20  0x80e4db18  0x8041b7c8  0x80037e10  0x0         0x0         0x0         
<0x80e4db00> 0x0         iEw0x8041b9e8  0x0         0x0         0x0         0x0         0xa         0x0         
<0x80e4db20> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4db40> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4db60> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4db80> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x0         
<0x80e4dba0> 0x0         0x0         0x0         0x0         0x0         0x0         0x0         0x8001d6dc  
<0x80e4dbc0> 0x88888888  0x88888888  0x88888888  0x88888888  0x88888888  0x88888888  0x88888888  0x88888888  

prio[7  ] pc[0x80017de0] state=32 [dely=0       ] top=0x80966ae0  bottom=0x80965ae0  cur_sp=0x80966a08, ra[0x80017de0] Timer, bottomMagic=0x0
prio[8  ] pc[0x80017de0] state=32 [dely=0       ] top=0x80dd8360  bottom=0x80dd4360  cur_sp=0x80dd8280, ra[0x80017de0] , bottomMagic=0x0iEw
prio[9  ] pc[0x80017de0] state=4  [dely=7       ] top=0x80a19080  bottom=0x80a11080  cur_sp=0x80a18f90, ra[0x80017de0] tcpip_thread, bottomMagic=0x0
prio[10 ] pc[0x80017de0] state=32 [dely=0       ] top=0x80ddc720  bottom=0x80dd8720  cur_sp=0x80ddc640, ra[0x80017de0] , bottomMagic=0x0
prio[11 ] pc[0x80017de0] state=1  [dely=0       ] top=0x80dd0ae0  bottom=0x80dcfae0  cur_sp=0x80dd09f8, ra[0x80017de0] RtmpTimerTask, bottomMagic=0x0
prio[12 ] pc[0x80017de0] state=1  [dely=0       ] top=0x80dd1b40  bottom=0x80dd0b40  cur_sp=0x80dd1a58, ra[0x80017de0] RtmpMlmeTask, bottomMagic=0x0
prio[13 ] pc[0x80017de0] state=1  [dely=0       ] top=0x80dd2ba0  bottom=0x80dd1ba0  cur_sp=0x80dd2ab0, ra[0x80017de0] RtmpCmdQTask, bottomMagic=0x0
prio[15 ] pc[0x80017de0] state=4  [dely=0       ] top=0x80aa5a60  bottom=0x80aa1a60  cur_sp=0x80aa57e0, ra[0x80017de0] Subt_task, bottomMagic=0x0
prio[17 ] pc[0x80017de0] state=4  [dely=0       ] top=0x809b2dc0  bottom=0x809b1dc0  cur_sp=0x809b2c40, ra[0x80017de0] usb_bus, bottomMagic=0x0
prio[20 ] pc[0x80017de0] state=1  [dely=654     ] top=0x80df27a0  bottom=0x80dea7a0  cur_sp=0x80df2408, ra[0x80017de0] wpa_supplicant, bottomMagic=0x0
prio[21 ] pc[0x80017de0] state=0  [dely=121     ] top=0x80de53e0  bottom=0x80ddd3e0  cur_sp=0x80de5358, ra[0x80017de0] wifi_link, bottomMagic=0x0
prio[22 ] pc[0x80017de0] state=4  [dely=4       ] top=0x80b11760  bottom=0x80b0d760  cur_sp=0x80b11628, ra[0x80017de0] ap_framework, bottomMagic=0x0
prio[23 ] pc[0x80017de0] state=4  [dely=0       ] top=0x80b25820  bottom=0x80b15820  cur_sp=0x80b25658, ra[0x80017de0] ui_frm, bottomMagic=0x0
prio[25 ] pc[0x80017de0] state=4  [dely=7       ] top=0x80af83e0  bottom=0x80af43e0  cur_sp=0x80af82f0, ra[0x80017de0] app uio, bottomMagic=0x0
prio[34 ] pc[0x1] state=0  [dely=0       ] top=0x80e4dbc0  bottom=0x80e3dbc0  cur_sp=0x80e4c060, ra[0x80017de0] do command task for dp, bottomMagic=0x0
prio[41 ] iEwpc[0x80017de0] state=4  [dely=7       ] top=0x80ab1140  bottom=0x80aad140  cur_sp=0x80ab1050, ra[0x80017de0] app playback, bottomMagic=0x0
prio[54 ] pc[0x80017de0] state=0  [dely=0       ] top=0x80a37a80  bottom=0x80a33a80  cur_sp=0x80a37988, ra[0x80017de0] eva_server, bottomMagic=0x0
prio[58 ] pc[0x80017de0] state=0  [dely=0       ] top=0x80bffcc0  bottom=0x80befcc0  cur_sp=0x80bffc18, ra[0x80017de0] epg_chain, bottomMagic=0x0
prio[66 ] pc[0x80017de0] state=0  [dely=0       ] top=0x8096c3a0  bottom=0x809683a0  cur_sp=0x8096c2c0, ra[0x80017de0] , bottomMagic=0x0
prio[67 ] pc[0x800124ac] state=8  [dely=0       ] top=0x80b0d560  bottom=0x80b09560  cur_sp=0x80b0d560, ra[0x8001d6dc] app userdb, bottomMagic=0x0
prio[68 ] pc[0x80017de0] state=4  [dely=7       ] top=0x80ab6800  bottom=0x80ab2800  cur_sp=0x80ab6710, ra[0x80017de0] app ca, bottomMagic=0x0
prio[73 ] pc[0x800124ac] state=8  [dely=0       ] top=0x80b04ba0  bottom=0x80b00ba0  cur_sp=0x80b04ba0, ra[0x8001d6dc] app scan, bottomMagic=0x0
prio[74 ] pc[0x80017iEwde0] state=4  [dely=4       ] top=0x80afc440  bottom=0x80af8440  cur_sp=0x80afc350, ra[0x80017de0] app singal monitor, bottomMagic=0x0
prio[77 ] pc[0x800124ac] state=8  [dely=0       ] top=0x80b09360  bottom=0x80b05360  cur_sp=0x80b09360, ra[0x8001d6dc] app usb upgrade, bottomMagic=0x0
prio[80 ] pc[0x80017de0] state=4  [dely=4       ] top=0x80b00520  bottom=0x80afc520  cur_sp=0x80b00430, ra[0x80017de0] app time, bottomMagic=0x0
prio[91 ] pc[0x80017de0] state=4  [dely=0       ] top=0x80aaa820  bottom=0x80aa6820  cur_sp=0x80aaa668, ra[0x80017de0] VBI_task, bottomMagic=0x0
prio[92 ] pc[0x80017de0] state=0  [dely=0       ] top=0x80a48a20  bottom=0x80a40a20  cur_sp=0x80a48930, ra[0x80017de0] dvb, bottomMagic=0x0
prio[93 ] pc[0x80017de0] state=0  [dely=0       ] top=0x80a3e0e0  bottom=0x80a3a0e0  cur_sp=0x80a3dff0, ra[0x80017de0] nim_ctrl, bottomMagic=0x0
prio[95 ] pc[0x80017de0] state=0  [dely=0       ] top=0x80a2dd80  bottom=0x80a29d80  cur_sp=0x80a2dc90, ra[0x80017de0] pnp svc, bottomMagic=0x0
prio[97 ] pc[0x800iEw17de0] state=0  [dely=0       ] top=0x80a84e60  bottom=0x80a80e60  cur_sp=0x80a84d70, ra[0x80017de0] net svc, bottomMagic=0x0
prio[98 ] pc[0x80017de0] state=0  [dely=0       ] top=0x80a96280  bottom=0x80a8e280  cur_sp=0x80a96118, ra[0x80017de0] net_src_svc, bottomMagic=0x0
prio[99 ] pc[0x80017de0] state=32 [dely=0       ] top=0x80a0cfa0  bottom=0x80a0afa0  cur_sp=0x80a0cec0, ra[0x80017de0] , bottomMagic=0x0
prio[102] pc[0x80017de0] state=0  [dely=4       ] top=0x80972160  bottom=0x8096e160  cur_sp=0x80972128, ra[0x80017de0] dm_v2, bottomMagic=0x0
prio[104] pc[0x80017de0] state=0  [dely=59      ] top=0x80967b40  bottom=0x80966b40  cur_sp=0x80967b00, ra[0x80017de0] Bus monitor, bottomMagic=0x0
prio[106] pc[0x80017de0] state=0  [dely=6       ] top=0x80b157c0  bottom=0x80b117c0  cur_sp=0x80b155e0, ra[0x80017de0] emon, bottomMagic=0x0
prio[254] pc[0x8001d364] state=0  [dely=0       ] top=0x8085d308  bottom=0x80859308  cur_sp=0x8085d2d0, ra[0x8022e788] Idle, bottomMagic=0x0
exc_stack_hi=0x80708300 exc_stack_low=0x80704700 

ra:[0x8041d8dc]  fp:[0x80e4d4e8]  gp:[0x806f4ab8]  at:[0xfffffffe]  
t9:[0x80017df4]  t8:[0x00000022]  t7:[0x00000000]  t6:[0x65746164]  t5:[0x5f707865]  
t4:[0x00007375]  t3:[0x0000000a]  t2:[0x00000000]  t1:[0x00000004]  t0:[0x00000004]  
s7:[0x806acdf0]  s6:[0x80037e10]  s5:[0x0003f4c6]  s4:[0x80e4d048]  s3:[0x0003f4c7]  
s2:[0x00000000]  s1:[0x80df3780]  s0:[0x806b0000]  
a3:[0x80ecfd85]  a2:[0xfffffffa]  a1:[0x00000000]  a0:[0x80ecfd84]  
v1:[0x80ecfd84 ]  v0:[0x00000025]  

!!!alloc cnt[0]
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBBBB99BBV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=214127 214111 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x880005c, status=0x1b02
avcpu ver = AVCPU_VERSION:[490:0584ac1c8239] Build Time:[Jun 20 2017, 
4:01:31]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b8e 48
[FastLogo][ap_init:964]Entry...
[FastLogo][_ai_dm_init]Entry...ticks:0
[FastLogo][_ai_dm_init]dm init v2...ticks:0
[FastLogo][_ai_dm_init]set header...ticks:1
[FastLogo][ap_init:1017]End...
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 3. sys partition size(free_mem) 9934168
**CDU UDQ**: 8b8e 48
[AI]chip id:1
[flash_pro] This flash can't be protected!!!
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 809B2E20 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 809CFEC0 priv->cfg.p_dem_bus =0x8096d180
tcpip: May 25 2017 17:28:55/nthread task for ethernet 9 
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
**LCK UDQ**: 2ab6
[AI][_ai_mdl_init]Software Ver[1000000]
eve223
mmi ver 395:d339c83370c6
EMON> &ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809b2e20


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports3c08bfc0 
 hub_add_new_dev hcd 809b1920
hub_add_new_dev 80c2d300
port_reset 809b1920
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
   #3device ADD cost 161 ts 
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB9B9BB9V
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=214127 214111 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x8800000, status=0xff01
avcpu ver = AVCPU_VERSION:[490:0584ac1co239] Build Time:[Jun 20 2017, 
4:01:31]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b8e 48
[FastLogo][ap_init:964]Entry...
[FastLogo][_ai_dm_init]Entry...ticks:0
[FastLogo][_ai_dm_init]dm init v2...ticks:0
[FastLogo][_ai_dm_init]set header...ticks:1
---------------Time Stamp[10:39:02]----------------
---------------Time Stamp[10:44:02]----------------
Serial Port Closed
monitor stop
Serial Port Opened
monitor start
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBBBB9BB9V
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8001
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=214127 214111 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x18800000, status=0xff01
avcpu ver = AVCPU_VERSION:[490:0584ac198239] Build Time:[Jun 20 2017, 14:01:31]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b8e 48
[FastLogo][ap_init:964]Entry...
[FastLogo][_ai_dm_init]Entry...ticks:0
[FastLogo][_ai_dm_init]dm init v2...ticks:0
[FastLogo][_ai_dm_init]set header...ticks:1
Serial Port Closed
monitor stop
---------------Time Stamp[10:49:02]----------------
---------------Time Stamp[13:37:50]----------------
---------------Time Stamp[13:42:50]----------------
---------------Time Stamp[13:47:50]----------------
---------------Time Stamp[13:52:50]----------------
---------------Time Stamp[13:57:50]----------------
---------------Time Stamp[14:02:50]----------------
---------------Time Stamp[14:07:50]----------------
---------------Time Stamp[14:12:50]----------------
---------------Time Stamp[14:17:50]----------------
---------------Time Stamp[14:22:50]----------------
---------------Time Stamp[14:27:50]----------------
---------------Time Stamp[14:32:50]----------------
---------------Time Stamp[14:37:50]----------------
---------------Time Stamp[14:42:50]----------------
---------------Time Stamp[14:47:50]----------------
---------------Time Stamp[14:52:50]----------------
---------------Time Stamp[14:57:50]----------------
---------------Time Stamp[15:02:50]----------------
---------------Time Stamp[15:07:50]----------------
---------------Time Stamp[15:12:50]----------------
---------------Time Stamp[15:17:50]----------------
