---------------Time Stamp[15:24:47]----------------
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d5cec0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports0 
 hub_add_new_dev hcd 80d5b9c0
hub_add_new_dev 80fa5220
port_reset 80d5b9c0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
   #3device ADD cost 161 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x7]

## timeshift exist is [1393786880]
p_cont[0x80eb8a18], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
update signal
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

4194304 bytes read
do_spi_flash_uboot_save offset[0] len[400000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=269586 269570 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Aug  1 2017, 
8:44:59]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123
 FastLogo_TaskStart

 Built at Jun 23 2017--18:04:55 symphony

 1. mem_start[8040ef98]

 2. whole memory size[4000000]

 3. System start: [0x1b8a800], rest size[0x58a800]
**CDU UDQ**: 8b6f 48
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[FastLogo][ap_init:687]Entry...
[FastLogo][_ai_spi_init]Entry...ticks:2
[FastLogo][_ai_dm_init]Entry...ticks:2
[FastLogo][_ai_dm_init]dm init v2...ticks:2
[FastLogo][_ai_dm_init]set header...ticks:3
#### tkgs flag is false!!
[FastLogo][drv_init]Entry...
[FastLogo][_ai_jpeg_init]Entry...ticks:3
[FastLogo][_ai_i2c_fp_init]Entry...ticks:4
[FastLogo][_ai_i2c_hdmi_init]Entry...ticks:4
[FastLogo][_ai_uio_init]Entry...ticks:5
[_fp_attach]Entry..., type:2
[FastLogo][_ai_hdmi_init]Entry...ticks:6
[FastLogo][_ai_display_init:492]Entry...ticks:60
[FastLogo][_ai_display_init:521]init...ticks:61
[FastLogo][_ai_display_init]End...ticks:61
fp  key[0x 7]
ir1 key[0x1a], usr[0xff1c]
ir2 key[0x42], usr[0x a22]
_check_force_upg_key,line 167, 21
_check_force_upg_key,line 195
show logo blockid[93]
[FastLogo][ap_init:740]End...
boot_para1: addr 0xbf140038 = 0x12340088
boot_para2: addr 0xbf14003c = 0x80008000
boot_para3: addr 0xbf30f060 = 0x12340001
FastLogo_TaskEnd, Jump:0x80100000
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 0MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--15:20:33 symphony

 1. mem_start[809de008]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 8074232
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
lpower_symphony_attach
[AI][_ai_jpeg_init]Entry...ticks:2
[AI][_ai_i2c_qam_init]Entry...ticks:3
[AI][_ai_i2c_init]Entry...ticks:3
[AI][_ai_i2c_1_init]Entry...ticks:3
[AI][_ai_i2c_fp_init]Entry...ticks:4
[AI][_ai_i2c_hdmi_init]Entry...ticks:4
[AI][_ai_spi_init]Entry...ticks:4
[AI][_ai_dm_init]Entry...ticks:5
[AI][_ai_dm_init]dm init v2...ticks:5
[AI][_ai_dm_init]set header...ticks:5
[AI][_ai_uio_init]Entry...ticks:6
[_fp_attach]Entry..., type:2
lpower cfg :pd_key 0x0
 
                pd_key1 0x0
 
                pd_key_fp 0x57
 
                type 0x3
 
                raw_map [0x0][0x1][0x2][0x3][0x4][0x5][0x6][0x7]

[AI][_ai_hdmi_init]EntriEïy...ticks:8
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
hdmi_debug: p_priv->is_support_dvi_mode 0 p_priv->is_fastlogo_mode 0,p_priv 0x80a262e0,ahg_rw 1
hdmi in main code
HDMI:hdmi_anx8560_open, 5278
  hdmi is_initialized 1hdmi_anx8560_open receiver BKSV is 47 74 18 2b bb
[AI][_ai_audio_init]Entry...ticks:56
[AI][_ai_video_init]Entry...ticks:56
[AI][_ai_usb_init]Entry...ticks:60
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80A28280 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80A45320 [AI][_ai_dmx_init]Entry...ticks:61
dmx modify  version: 36142
dmx_symphony_tsi_set_es_buffer error !!!
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:63
priv->cfg.p_dem_bus =0x809e6320
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a28280


 ###step3### msg.event 2
hdmi_hdcp: anx8560_service 3688    events 48 a1 0x0 irq_id 0x16
video format change line 2910
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:196
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c20000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d20000], size[180000], align[400], cfg size[1c01000]
tcpip: Jul 19 2017 11:32:22/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:201
file_size 345801 p_data_buffer 80b1c000 

 unzip resource. in_addr = 0x9e2c3358, out_addr = 0x81191400, in_len = 345801, out_len = 989176
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:233
[AI][_ai_eva_init]Entry...ticks:234
[AI][_ai_tuner_init]Entry...ticks:234
[AI][_ai_dvb_init]Entry...ticks:255
[CA]: init
[AI][_ai_dmm_init]Entry...ticks:255
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x38, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[H0.95.80010S.021]
[AI][_ai_avc_init]Entry...ticks:358
[AI][_ai_iconv_init]Entry...ticks:358
[AI][_ai_antenna_lnb_init]Entry...ticks:359
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:359
hdmi_anx8560_video_config start res6, pn 2 
hdmi_tx_de_gen_en!


 @@@@@@@@@@@@@@@ cspace_y2r 0 up_sample 0 range_y2r 0 cspace_r2y 0 down_sample 0 p_output_cfg->csc 2
MISC_Reset!
hdmi_debug : hdcp off, g_hdmi_edid_result.is_hdmi 1



 new:  mute 0 is_in_mute 0 prio6 
hdmi_debug : g_hdmi_edid_result.is_hdmi 1
 !!!!!!!!!!!!!!!!!!!!!!!!!    hdmi analog reset   reg 0xbf157000, value 0x1000080 
 !!!!!!!!!!!!!!!!!!!!!!!!!     hdmi analog reset  reg 0xbf157000, value 0x1000000 
[AI][_ai_time_init]Entry...ticks:397
[CA]===>construct_cas_policy
[CA MANAGER]: type:0, para1:0, para2:0
set ca addr is 0x0
cas_adt_ncs_attach
0x000000000
7:b364a56bb03b
eve0
5876[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80a26d80
hub_add_new_dev 80b7d900
port_reset 80a26d80
close_fast_logo
mmi init
mmi ver 
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:0, para2:1
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg ad&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
dr 0x818b0400
[CA MANAGER]: type:1, para1:0, para2:0
end desktop init
get ver 0
[CA MANAGER]: type:2, para1:0, para2:0
close_fast_logo


======================================================

sn_num:[0000000000000000],mac_address:[000000000000]

===========================iEï===========================

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
audio cfg @HDMI_TX_SYS_CTRL1_REG@   3
audio_type = 0x02
config i2s channel, c = 0x04
config i2s format, c = 0x00
down sample, c = 0x00
audio sample rate set to 48K
Audio MCLK input mode is: 01
anx8560_audio_input_cfg 1742 
audio cfg success 
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
MCAS_VIDEO_STOP
UI: disable ttx.........
-----ui show logo v2 size 0xd4a9, 0, 179
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:0, para2:2
---------g_curn_menu_1=1
[CA MANAGER]: type:3, para1:0, para2:0
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 3231072, alloced_peak = 3310688, rest_size = 4843160

EMON> [NW] Set 3g sts:2
   #3device ADD cost 159 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[CA MANAGER]: type:10, para1:2, para2:0
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80c274b8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
[CA MANAGER]: type:12, para1:2, para2:24
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
[CA MANAGER]: type:12, para1:2, para2:2
update signal

## timeshift exist is [1393786880]

## timeshift exist is [1393786880]
--chip id- file.txt already exist,remove it
update signal
_switch_playstatus
from_id = 2 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 3
UI: switch to STOP..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 2 to 68 
[CA MANAGER]: type:12, para1:2, para2:68
sat_id[0], sat_name[T], lnb_low[9750], lnb_high[10600]
MCAS_VIDEO_STOP
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 9750 high = 10600
---lnb pow = 0 22k = 0
---diseqc type = 1 port = 0
---nim type = 0
- set transpond id = 1
---freq = 11747
---symbol = 27500
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[1], freq[11747], sym[27500], pol[0], 22k[0]
update signal
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 119, p_sat->is_t2_sat: 0
---lnb low = 9750 high = 10600
---lnb pow = 0 22k = 0
---diseqc type = 1 port = 1
---nim type = 0
- set transpond id = 120
---freq = 10719
---symbol = 27500
---polarity = V
---tuner_id = 0
----------------------------------
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 220, p_sat->is_t2_sat: 0
---lnb low = 9750 high = 10600
---lnb pow = 0 22k = 0
---diseqc type = 1 port = 3
---nim type = 0
- set transpond id = 221
---freq = 10729
---symbol = 22000
---polarity = V
---tuner_id = 0
----------------------------------
update signal
p_cont[0x80c27d70], root[0]
_switch_playstatus
from_id = 68 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 24 
[CA MANAGER]: type:12, para1:68, para2:24
_switch_playstatus
from_id = 68 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 68 
[CA MANAGER]: type:12, para1:68, para2:68
p_cont[0x80c27d70], root[0]
Delete Book Node [0]
Delete Book Node [1]
Delete Book Node [2]
Delete Book Node [3]
Delete Book Node [4]
Delete Book Node [5]
Delete Book Node [6]
Delete Book Node [7]
Delete Book Node [8]
Delete Book Node [9]
Delete Book Node [10]
Delete Book Node [11]
Delete Book Node [12]
Delete Book Node [13]
Delete Book Node [14]
Delete Book Node [15]
Delete Book Node [16]
Delete Book Node [17]
Delete Book Node [18]
Delete Book Node [19]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 68 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 73 
[CA MANAGER]: type:12, para1:68, para2:73
_switch_playstatus
from_id = 73 to_id = 64
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 64 
[CA MANAGER]: type:12, para1:73, para2:64
_switch_playstatus
from_id = 64 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 64 to 73 
[CA MANAGER]: type:12, para1:64, para2:73
ui_antenna_set: add sat is OK!
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 73 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 68 
[CA MANAGER]: type:12, para1:73, para2:68
PROGBAR: can NOT get pg!
_switch_playstatus
from_id = 68 to_id = 7
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 7 
[CA MANAGER]: type:12, para1:68, para2:7
ui_tp_set: add tp is OK!
sat_id[0], sat_name[0], lnb_low[5150], lnb_high[5150]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 1
---freq = 3150
---symbol = 27500
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[1], freq[3150], sym[27500], pol[0], 22k[0]
_switch_playstatus
from_id = 7 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 7 to 68 
[CA MANAGER]: type:12, para1:7, para2:68
update signal
on_epg_request_table_policy_switch
_switch_playstatus
from_id = 68 to_id = 8
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 8 
[CA MANAGER]: type:12, para1:68, para2:8
on_epg_request_table_policy_switch
do scan pre open
set book flag
UI: deactive playback.........
set front panel
init static data
init scan
create timer for animation
_switch_playstatus
from_id = 8 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 8 to 9 
[CA MANAGER]: type:12, para1:8, para2:9
load sat id 0
PROCESS -> add/change sat[-2116624496]
PROCESS -> add/change tp
ADD TP -> freq[3150]
END ADD TP ->freq[3150]
PROCESS -> update progress
UPDATE PROGRESS -> 18
PROCESS -> update progress
UPDATE PROGRESS -> 36
PROCESS -> update progress
UPDATE PROGRESS -> 64
Found PG: s_id[6], v_pid[0], a_pid_0[915], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT FM], pmt_pid[357],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[7], v_pid[0], a_pid_0[916], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Ankara], pmt_pid[358],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[15], v_pid[0], a_pid_0[1117], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT EAST], pmt_pid[559],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[8], v_pid[0], a_pid_0[917], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 6], pmt_pid[359],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->serviiEïce_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[10], v_pid[0], a_pid_0[1016], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WORLD], pmt_pid[457],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[11], v_pid[0], a_pid_0[1017], a_pid_1[0],a_pid_2[0], trace num[1], name[TSR TURKCE], pmt_pid[458],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[13], v_pid[0], a_pid_0[1115], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT NAGME], pmt_pid[557],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[14], v_pid[0], a_pid_0[1116], a_pid_1[0],a_pid_2[0], traceiEï num[1], name[TRT TURKU], pmt_pid[558],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[25], v_pid[1312], a_pid_0[1313], a_pid_1[1314],a_pid_2[0], trace num[2], name[TRT SPOR], pmt_pid[1056],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[28], v_pid[0], a_pid_0[1316], a_pid_1[0],a_pid_2[0], trace num[1], name[DIS YAY ORTA DALGA ARAPCA], pmt_pid[1257],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[D]
END ADD PG -> name[D]
Found PG: s_id[22], v_pid[0], a_pid_0[1315], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WEST], pmt_pid[757],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESSiEï -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[1], v_pid[512], a_pid_0[513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT 1], pmt_pid[256],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[5], v_pid[612], a_pid_0[613], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT HABER], pmt_pid[356],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[9], v_pid[712], a_pid_0[713], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURK], pmt_pid[456],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[12], v_pid[812], a_pid_0[813], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT MUZIK], pmt_pid[556],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[16], v_pid[912], a_pid_0[913], a_pid_1[914],a_pid_2[0], trace num[2], name[TRT COCUK], pmt_pid[656],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[21], v_pid[1012], a_pid_0[1013], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT AVAZ], pmt_pid[756],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[23], v_pid[1112], a_pid_0[1113], a_pid_1[0],a_pid_2[0], trace num[1], name[EURONEWS TURKCE], pmt_pid[856],scramble[0] 
is_invalid_tv_service_type LINE:[318] thiEïe p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[24], v_pid[1212], a_pid_0[1213], a_pid_1[1214],a_pid_2[0], trace num[2], name[TRT ARAPCA], pmt_pid[956],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[26], v_pid[1412], a_pid_0[1413], a_pid_1[1416],a_pid_2[0], trace num[2], name[TRT KURDI], pmt_pid[1156],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[27], v_pid[1512], a_pid_0[1513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT DIYANET], pmt_pid[1256],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[20], v_pid[0], a_pid_0[121iEï7], a_pid_1[0],a_pid_2[0], trace num[1], name[Trabzon Radyosu], pmt_pid[659],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[19], v_pid[0], a_pid_0[1216], a_pid_1[0],a_pid_2[0], trace num[1], name[Erzurum Radyosu], pmt_pid[658],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[18], v_pid[0], a_pid_0[1215], a_pid_1[0],a_pid_2[0], trace num[1], name[Cukurova Radyosu], pmt_pid[657],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[C]
END ADD PG -> name[C]
Found PG: s_id[2], v_pid[0], a_pid_0[815], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 1], pmt_pid[257],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[3], v_pid[0], a_pid_0[816], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 3], pmt_pid[258],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[4], v_pid[0], a_pid_0[817], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Istanbul], pmt_pid[259],scramble[0] 
is_invalid_tv_serviciEïe_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[17], v_pid[0], a_pid_0[1018], a_pid_1[0],a_pid_2[0], trace num[1], name[Antalya Radyosu], pmt_pid[459],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[A]
END ADD PG -> name[A]
db done ok
PROCESS -> update progress
UPDATE PROGRESS -> 100
PROCESS -> finish
*************************on finished : 8165
p_cont[0x80c27d70], root[0]
_switch_playstatus
from_id = 9 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 24 
[CA MANAGER]: type:12, para1:9, para2:24
_switch_playstatus
from_id = 9 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 9 
[CA MANAGER]: type:12, para1:9, para2:9
*************************process finished : 8228
DO_SEARCH: before MSG_SAVE!
*************************do_search_post_close 1 : 8228
p_cont[0x80c27d70], root[0]
do_search_post_close: reset the desktop notify func
------------->>active ap playback
UI: active playback.........
*************************do_search_post_close 2 : 8259
_switch_playstatus
from_id = 9 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
ui_start_tkgs_monitor
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[0] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
update signal
[CA MANAGER]: type:4, para1:10, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 1056 
CA: set sid pgid: 10
MCAS_VIDEO_STOP
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
switch_autoclose: from 9 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:9, para2:1
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3038336, alloced_peak = 3576608, rest_size = 5035896

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818b0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
ui_is_ttx_data_ready: -----1
*************************close all menus : 8281
audio cfg @HDMI_TX_SYS_CTRL1_REG@   3
audio_type = 0x02
config i2s channel, c = 0x84
config i2s format, c = 0x00
down sample, c = 0x01
audio sample rate set to 48K
Audio MCLK input mode is: 01
anx8560_audio_input_cfg 1742 
HDMI_TX_INFO_PKTCTRL2_REG = 1
HDMI_TX_INFO_PKTCTRL2_REG = 1
audio cfg success 
TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
MCAS_NEW_CAT
ui_is_ttx_data_ready: -----1
video_out_ticks 8332
video pid 520 descr id: 1101
audio pid 521 descr id: 1d02

ui_is_ttx_data_ready: -----1
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
update signal
[CA MANAGER]: type:4, para1:13, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 256 
CA: set sid pgid: 13
MCAS_VIDEO_STOP
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
MCAS_NEW_CAT
on_epg_request_table_policy_switch
on_ttx_ready: prog id = 13, curn pg =13 
video pid 200 descr id: 1d01
audio pid 201 descr id: 1102

Type[12], i[1]
video_out_ticks 8582
on_ttx_ready: prog id = 13, curn pg =13 
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ts data overflow:0x13
ts data overflow:0x13
ui_stop_tkgs_monitor
TKGS IMPL DEBUG : function  iti_clear_attach_block, line 303clear attach block 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:40
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:40, para2:1
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3725056, alloced_peak = 3799264, rest_size = 4349176

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
ui_start_tkgs_monitor
Type[12], i[1]
TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ui_stop_tkgs_monitor
TKGS IMPL DEBUG : function  iti_clear_attach_block, line 303clear attach block 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:40
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:40, para2:1
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3762176, alloced_peak = 3799264, rest_size = 4312056

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
ui_start_tkgs_monitots data overflow:0x13
r
Type[12], i[1]
TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743424, alloced_peak = 3799264, rest_size = 4330808

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
ts data overflow:0x13
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3761984, alloced_peak = 3799264, rest_size = 4312248

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3799264, rest_size = 4330680

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ui_stop_tkgs_monitor
TKGS IMPL DEBUG : function  iti_clear_attach_block, line 303clear attach block 
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 262 
_switch_playstatus : 267 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:57
update signal
ts data overflow:0x13
ts data overflow:0x13
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
ts data overflow:0x13
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
ts data overflow:0x13
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
ui_start_tkgs_monitor
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:57, para2:1
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3790944, alloced_peak = 3828704, rest_size = 4283288

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
on_epg_request_table_policy_switch
on_ttx_ready: prog id = 13, curn pg =13 
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3828704, rest_size = 4330680

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_auts data overflow:0x13
toclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ui_stop_tkgs_monitor
TKGS IMPL DEBUG : function  iti_clear_attach_block, line 303clear attach block 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
MCAS_VIDEO_STOP
UI: disable ttx.........
-----ui show logo v2 size 0xd4a9, 0, 179
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:2
---------g_curn_menu_1=1
---------------Time Stamp[15:29:47]----------------
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a28280


 ###step3### msg.event 3
[CA MANAGER]: type:11, para1:2, para2:0
###ui_nw_api_on_plug_out dev_type[1]
p_cont[0x80c274b8], root[0]
_switch_plathread usb_stor_control_thread exit
ystatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autocusb_bus notify device REMOVE 
lose: from 2 to 24 
[CA MANAGER]: type:12, para1:2, para2:24
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
[CA MANAGER]: type:12, para1:2, para2:2
update signal
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 2 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 3
UI: switch to PLAY..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
ui_start_tkgs_monitor
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
MCAS_VIDEO_STOP
update signal
[CA MANAGER]: type:4, para1:13, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 256 
CA: set sid pgid: 13
MCAS_VIDEO_STOP
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
switch_autoclose: from 2 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:2, para2:1
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3015584, alloced_peak = 3828704, rest_size = 5058648

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818b0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
ui_is_ttx_data_ready: -----1
TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
video pid 200 descr id: 101
audio pid 201 descr id: 1302
cas_adt_ncs_table_process() the same pmt 

MCAS_NEW_CAT
ui_is_ttx_data_ready: -----1
ui_is_ttx_data_ready: -----1
video_out_ticks 37192
on_epg_request_table_policy_switch
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3756544, alloced_peak = 3828704, rest_size = 4317688

@@@ui_util_api_release_vsurf-------
@@@ui_util_aiEïpi_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3719424, alloced_peak = 3828704, rest_size = 4354808

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg alreiEïady init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3719424, alloced_peak = 3828704, rest_size = 4354808

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3719424, alloced_peak = 3828704, rest_size = 4354808

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3737984, alloced_peak = 3828704, rest_size = 4336248

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
ts data overflow:0x12
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3737984, alloced_peak = 3828704, rest_size = 4336248

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3719424, alloced_peak = 3828704, rest_size = 4354808

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3737856, alloced_peak = 3828704, rest_size = 4336376

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3719296, alloced_peak = 3828704, rest_size = 4354936

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
ts data overflow:0x12
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3737984, alloced_peak = 3828704, rest_size = 4336248

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3737856, alloced_peak = 3828704, rest_size = 4336376

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3719424, alloced_peak = 3828704, rest_size = 4354808

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3737984, alloced_peak = 3828704, rest_size = 4336248

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ts data overflow:0x12
ts data overflow:0x12
ts data overflow:0x12
ts data overflow:0x12
ts data overflow:0x12
ts data overflow:0x12
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a28280


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports0 
 hub_add_new_dev hcd 80a26d80
hub_add_new_dev 80cf2a40
port_reset 80a26d80
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8001205
###step1.2### 0 usb_hcd_poll_rh_status 
ts data overflow:0x12
   #3device ADD cost 161 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[CA MANAGER]: type:10, para1:1, para2:0
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80c2743c], root[0]
_switch_playstatus
from_id = 1 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 24 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:24
_switch_playstatus
from_id = 1 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:1, para2:1
[USB]ui_upg_file_list_get:file count[0x22]
ts data overflow:0x12
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
_switch_playstatus
from_id = 1 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
MCAS_VIDEO_STOP
UI: disable ttx.........
switch_autoclose: from 1 to 47 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:47
UI: deactive playback.........
update signal

## timeshift exist is [1393786880]

## timeshift exist is [1393786880]

##ufs_open fail[4]:[C:\chip_id.txt]
--- file.txt write size 31
update signal
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80c27bfc], root[0]
_switch_playstatus
from_id = 47 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 24 
[CA MANAGER]: type:12, para1:47, para2:24
_switch_playstatus
from_id = 47 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 47 
[CA MANAGER]: type:12, para1:47, para2:47
p_cont[0x80c27bfc], root[0]
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=269586 269570 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x8800000, status=0xff01
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Aug  1 2017, 
8:44:59]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123
 FastLogo_TaskStart

 Built at Jun 23 2017--18:04:55 symphony

 1. mem_start[8040ef98]

 2. whole memory size[4000000]

 3. System start: [0x1b8a800], rest size[0x58a800]
**CDU UDQ**: 8b6f 48
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[FastLogo][ap_init:687]Entry...
[FastLogo][_ai_spi_init]Entry...ticks:2
[FastLogo][_ai_dm_init]Entry...ticks:2
[FastLogo][_ai_dm_init]dm init v2...ticks:2
[FastLogo][_ai_dm_init]set header...ticks:3
#### tkgs flag is false!!
[FastLogo][drv_init]Entry...
[FastLogo][_ai_jpeg_init]Entry...ticks:3
[FastLogo][_ai_i2c_fp_init]Entry...ticks:4
[FastLogo][_ai_i2c_hdmi_init]Entry...ticks:4
[FastLogo][_ai_uio_init]Entry...ticks:5
[_fp_attach]Entry..., type:2
[FastLogo][_ai_hdmi_init]Entry...ticks:6
[FastLogo][_ai_display_init:492]Entry...ticks:60
[FastLogo][_ai_display_init:521]init...ticks:61
[FastLogo][_ai_display_init]End...ticks:61
fp  key[0x 7]
ir1 key[0x1a], usr[0xff1c]
ir2 key[0x42], usr[0x a22]
_check_force_upg_key,line 167, 21
_check_force_upg_key,line 195
show logo blockid[93]
---------------Time Stamp[15:34:47]----------------
[FastLogo][ap_init:740]End...
boot_para1: addr 0xbf140038 = 0x12340088
boot_para2: addr 0xbf14003c = 0x80008000
boot_para3: addr 0xbf30f060 = 0x12340001
FastLogo_TaskEnd, Jump:0x80100000
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 0MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--15:31:41 symphony

 1. mem_start[809de108]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 8073976
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
lpower_symphony_attach
[AI][_ai_jpeg_init]Entry...ticks:2
[AI][_ai_i2c_qam_init]Entry...ticks:3
[AI][_ai_i2c_init]Entry...ticks:3
[AI][_ai_i2c_1_init]Entry...ticks:3
[AI][_ai_i2c_fp_init]Entry...ticks:4
[AI][_ai_i2c_hdmi_init]Entry...ticks:4
[AI][_ai_spi_init]Entry...ticks:4
[AI][_ai_dm_init]Entry...ticks:5
[AI][_ai_dm_init]dm init v2...ticks:5
[AI][_ai_dm_init]set header...ticks:6
[AI][_ai_uio_init]Entry...ticks:6
[_fp_attach]Entry..., type:2
lpower cfg :pd_key 0x0
 
                pd_key1 0x0
 
                pd_key_fp 0x57
 
                type 0x3
 
                raw_map [0x0][0x1][0x2][0x3][0x4][0x5][0x6][0x7]

[AI][_ai_hdmi_init]EntriEïy...ticks:8
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
hdmi_debug: p_priv->is_support_dvi_mode 0 p_priv->is_fastlogo_mode 0,p_priv 0x80a263e0,ahg_rw 1
hdmi in main code
HDMI:hdmi_anx8560_open, 5278
  hdmi is_initialized 1hdmi_anx8560_open receiver BKSV is 47 74 18 2b bb
[AI][_ai_audio_init]Entry...ticks:56
[AI][_ai_video_init]Entry...ticks:56
[AI][_ai_usb_init]Entry...ticks:60
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80A28380 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80A45420 [AI][_ai_dmx_init]Entry...ticks:61
dmx modify  version: 36142
dmx_symphony_tsi_set_es_buffer error !!!
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:63
priv->cfg.p_dem_bus =0x809e6420
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a28380


 ###step3### msg.event 2
hdmi_hdcp: anx8560_service 3688    events 48 a1 0x0 irq_id 0x16
video format change line 2&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:196
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c20000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d20000], size[180000], align[400], cfg size[1c01000]
tcpip: Jul 19 2017 11:32:22/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:201
file_size 345801 p_data_buffer 80b1c100 

 unzip resource. in_addr = 0x9e2c3098, out_addr = 0x81191400, in_len = 345801, out_len = 989176
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:233
[AI][_ai_eva_init]Entry...ticks:234
[AI][_ai_tuner_init]Entry...ticks:234
[AI][_ai_dvb_init]Entry...ticks:255
[CA]: init
[AI][_ai_dmm_init]Entry...ticks:255
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x38, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[H0.95.80010S.021]
[AI][_ai_avc_init]Entry...ticks:355
[AI][_ai_iconv_init]Entry...ticks:356
[AI][_ai_antenna_lnb_init]Entry...ticks:356
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:357
hdmi_anx8560_video_config start res6, pn 2 
hdmi_tx_de_gen_en!


 @@@@@@@@@@@@@@@ cspace_y2r 0 up_sample 0 range_y2r 0 cspace_r2y 0 down_sample 0 p_output_cfg->csc 2
MISC_Reset!
hdmi_debug : hdcp off, g_hdmi_edid_result.is_hdmi 1



 new:  mute 0 is_in_mute 0 prio6 
hdmi_debug : g_hdmi_edid_result.is_hdmi 1
 !!!!!!!!!!!!!!!!!!!!!!!!!    hdmi analog reset   reg 0xbf157000, value 0x1000080 
 !!!!!!!!!!!!!!!!!!!!!!!!!     hdmi analog reset  reg 0xbf157000, value 0x1000000 
[AI][_ai_time_init]Entry...ticks:394
[CA]===>construct_cas_policy
[CA MANAGER]: type:0, para1:0, para2:0
set ca addr is 0x0
cas_adt_ncs_attach
0x000000000
7:b364a56bb03b
eve0
5876[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80a26e80
hub_add_new_dev 80b7da00
port_reset 80a26e80
close_fast_logo
mmi init
mmi ver 
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:0, para2:1
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg ad&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
dr 0x818b0400
[CA MANAGER]: type:1, para1:0, para2:0
end desktop init
get ver 0
[CA MANAGER]: type:2, para1:0, para2:0
close_fast_logo


======================================================

sn_num:[0000000000000000],mac_address:[000000000000]

================iEï======================================

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
910
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
MCAS_VIDEO_STOP
audio cfg @HDMI_TX_SYS_CTRL1_REG@   3
audio_type = 0x02
config i2s channel, c = 0x04
config i2s format, c = 0x00
down sample, c = 0x00
audio sample rate set to 48K
Audio MCLK input mode is: 01
anx8560_audio_input_cfg 1742 
audio cfg success 
UI: disable ttx.........
-----ui show logo v2 size 0xd4a9, 0, 179
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:0, para2:2
---------g_curn_menu_1=1
[CA MANAGER]: type:3, para1:0, para2:0
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 3231072, alloced_peak = 3310688, rest_size = 4842904

[NW] Set 3g sts:2
EMON>    #3device ADD cost 159 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[CA MANAGER]: type:10, para1:2, para2:0
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80c275b8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
[CA MANAGER]: type:12, para1:2, para2:24
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
[CA MANAGER]: type:12, para1:2, para2:2
update signal

## timeshift exist is [1393786880]

## timeshift exist is [1393786880]
--chip id- file.txt already exist,remove it
update signal
p_cont[0x80c275b8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
[CA MANAGER]: type:12, para1:2, para2:24
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
[CA MANAGER]: type:12, para1:2, para2:2
p_cont[0x80c275b8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
[CA MANAGER]: type:12, para1:2, para2:24
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
[CA MANAGER]: type:12, para1:2, para2:2
_switch_playstatus
from_id = 2 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 3
UI: switch to STOP..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 2 to 68 
[CA MANAGER]: type:12, para1:2, para2:68
sat_id[0], sat_name[T], lnb_low[9750], lnb_high[10600]
MCAS_VIDEO_STOP
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 9750 high = 10600
---lnb pow = 0 22k = 0
---diseqc type = 1 port = 0
---nim type = 0
- set transpond id = 1
---freq = 11747
---symbol = 27500
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[1], freq[11747], sym[27500], pol[0], 22k[0]
update signal
p_cont[0x80c27e70], root[0]
_switch_playstatus
from_id = 68 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 24 
[CA MANAGER]: type:12, para1:68, para2:24
_switch_playstatus
from_id = 68 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 68 
[CA MANAGER]: type:12, para1:68, para2:68
p_cont[0x80c27e70], root[0]
Delete Book Node [0]
Delete Book Node [1]
Delete Book Node [2]
Delete Book Node [3]
Delete Book Node [4]
Delete Book Node [5]
Delete Book Node [6]
Delete Book Node [7]
Delete Book Node [8]
Delete Book Node [9]
Delete Book Node [10]
Delete Book Node [11]
Delete Book Node [12]
Delete Book Node [13]
Delete Book Node [14]
Delete Book Node [15]
Delete Book Node [16]
Delete Book Node [17]
Delete Book Node [18]
Delete Book Node [19]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 68 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 73 
[CA MANAGER]: type:12, para1:68, para2:73
_switch_playstatus
from_id = 73 to_id = 64
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 64 
[CA MANAGER]: type:12, para1:73, para2:64
_switch_playstatus
from_id = 64 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 64 to 73 
[CA MANAGER]: type:12, para1:64, para2:73
ui_antenna_set: add sat is OK!
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 73 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 68 
[CA MANAGER]: type:12, para1:73, para2:68
PROGBAR: can NOT get pg!
_switch_playstatus
from_id = 68 to_id = 7
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 7 
[CA MANAGER]: type:12, para1:68, para2:7
update signal
ui_tp_set: add tp is OK!
sat_id[0], sat_name[0], lnb_low[5150], lnb_high[5150]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 1
---freq = 3150
---symbol = 27500
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[1], freq[3150], sym[27500], pol[0], 22k[0]
_switch_playstatus
from_id = 7 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 7 to 68 
[CA MANAGER]: type:12, para1:7, para2:68
on_epg_request_table_policy_switch
update signal
_switch_playstatus
from_id = 68 to_id = 8
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 8 
[CA MANAGER]: type:12, para1:68, para2:8
do scan pre open
set book flag
UI: deactive playback.........
set front panel
init static data
init scan
create timer for animation
_switch_playstatus
from_id = 8 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 8 to 9 
[CA MANAGER]: type:12, para1:8, para2:9
load sat id 0
PROCESS -> add/change sat[-2116624496]
PROCESS -> add/change tp
ADD TP -> freq[3150]
END ADD TP ->freq[3150]
PROCESS -> update progress
UPDATE PROGRESS -> 18
PROCESS -> update progress
UPDATE PROGRESS -> 36
PROCESS -> update progress
UPDATE PROGRESS -> 64
Found PG: s_id[6], v_pid[0], a_pid_0[915], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT FM], pmt_pid[357],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[7], v_pid[0], a_pid_0[916], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Ankara], pmt_pid[358],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[15], v_pid[0], a_pid_0[1117], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT EAST], pmt_pid[559],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[8], v_pid[0], a_pid_0[917], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 6], pmt_pid[359],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[10], v_pid[0], a_pid_0[1016], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WORLD], pmt_pid[457],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[11], v_pid[0], a_pid_0[1017], a_pid_1[0],a_pid_2[0], trace num[1], name[TSR TURKCE], pmt_pid[458],scramble[0] 
is_invalid_tv_service_type LINE:[318] iEïthe p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[13], v_pid[0], a_pid_0[1115], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT NAGME], pmt_pid[557],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[14], v_pid[0], a_pid_0[1116], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURKU], pmt_pid[558],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[25], v_pid[1312], a_pid_0[1313], a_pid_1[1314],a_pid_2[0], trace num[2], name[TRT SPOR], pmt_pid[1056],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[28], v_pid[0], a_pid_0[1316], a_pid_1[iEï0],a_pid_2[0], trace num[1], name[DIS YAY ORTA DALGA ARAPCA], pmt_pid[1257],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[D]
END ADD PG -> name[D]
Found PG: s_id[22], v_pid[0], a_pid_0[1315], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WEST], pmt_pid[757],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[1], v_pid[512], a_pid_0[513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT 1], pmt_pid[256],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[5], v_pid[612], a_pid_0[613], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT HABER], pmt_pid[356],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new iEïpg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[9], v_pid[712], a_pid_0[713], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURK], pmt_pid[456],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[12], v_pid[812], a_pid_0[813], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT MUZIK], pmt_pid[556],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[16], v_pid[912], a_pid_0[913], a_pid_1[914],a_pid_2[0], trace num[2], name[TRT COCUK], pmt_pid[656],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[21], v_pid[1012], a_pid_0[1013], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT AVAZ], pmt_pid[756],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[23], v_pid[1112], a_pid_0[1113], a_pid_1[0],a_pid_2[0], trace num[1], name[EURONEWS TURKCE], pmt_pid[856],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[24], v_pid[1212], a_pid_0[1213], a_pid_1[1214],a_pid_2[0], trace num[2], name[TRT ARAPCA], pmt_pid[956],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[20], v_pid[0], a_pid_0[1217], a_pid_1[0],a_pid_2[0], trace num[1], name[Trabzon Radyosu], pmt_pid[659],scramble[0] 
is_invalid_tviEï_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[26], v_pid[1412], a_pid_0[1413], a_pid_1[1416],a_pid_2[0], trace num[2], name[TRT KURDI], pmt_pid[1156],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[27], v_pid[1512], a_pid_0[1513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT DIYANET], pmt_pid[1256],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x01
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[19], v_pid[0], a_pid_0[1216], a_pid_1[0],a_pid_2[0], trace num[1], name[Erzurum Radyosu], pmt_pid[658],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[18], v_pid[0], a_pid_0[1215], a_pid_1[0],a_pid_2[0], trace num[1], name[Cukurova Radyosu], pmt_pid[657],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[C]
END ADD PG -> name[C]
Found PG: s_id[2], v_pid[0], a_pid_0[815], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 1], pmt_pid[257],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[3], v_pid[0], a_pid_0[816], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 3], pmt_pid[258],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[4], v_pid[0], a_pid_0[817], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Istanbul], pmt_pid[259],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[17], v_pid[0], a_pid_0[1018], a_pid_1[0],a_pid_2[0], trace num[1], name[Antalya Radyosu], pmt_pid[459],scramble[0] 
is_invalid_tv_service_type LINE:[318] the p_pg->service_type is 0x02
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[A]
END ADD PG -> name[A]
db done ok
PROCESS -> update progress
UPDATE PROGRESS -> 100
PROCESS -> finish
*************************on finished : 5950
p_cont[0x80c27e70], root[0]
_switch_playstatus
from_id = 9 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 24 
[CA MANAGER]: type:12, para1:9, para2:24
_switch_playstatus
from_id = 9 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 9 
[CA MANAGER]: type:12, para1:9, para2:9
*************************process finished : 6015
DO_SEARCH: before MSG_SAVE!
*************************do_search_post_close 1 : 6015
p_cont[0x80c27e70], root[0]
do_search_post_close: reset the desktop notify func
------------->>active ap playback
UI: active playback.........
*************************do_search_post_close 2 : 6050
_switch_playstatus
from_id = 9 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
ui_start_tkgs_monitor
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[0] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
update signal
[CA MANAGER]: type:4, para1:10, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 1056 
CA: set sid pgid: 10
MCAS_VIDEO_STOP
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
switch_autoclose: from 9 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:9, para2:1
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3038336, alloced_peak = 3576608, rest_size = 5035640

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818b0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autocloseiEï: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
ui_is_ttx_data_ready: -----1
*************************close all menus : 6073
audio cfg @HDMI_TX_SYS_CTRL1_REG@   3
audio_type = 0x02
config i2s channel, c = 0x84
config i2s format, c = 0x00
down sample, c = 0x01
audio sample rate set to 48K
Audio MCLK input mode is: 01
anx8560_audio_input_cfg 1742 
HDMI_TX_INFO_PKTCTRL2_REG = 1
HDMI_TX_INFO_PKTCTRL2_REG = 1
audio cfg success 
TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
video pid 520 descr id: 1101
audio pid 521 descr id: 1d02

MCAS_NEW_CAT
ui_is_ttx_data_ready: -----1
video_out_ticks 6171
ui_is_ttx_data_ready: -----1
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
update signal
[CA MANAGER]: type:4, para1:13, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 256 
CA: set sid pgid: 13
MCAS_VIDEO_STOP
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
MCAS_NEW_CAT
video pid 200 descr id: 1d01
audio pid 201 descr id: 1102

on_epg_request_table_policy_switch
ui_is_ttx_data_ready: -----1
video_out_ticks 6404
pg is scramble = 0, play type = 0
on_ttx_ready: prog id = 13, curn pg =14 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
update signal
[CA MANAGER]: type:4, para1:14, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 356 
CA: set sid pgid: 14
MCAS_VIDEO_STOP
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x5
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
MCAS_NEW_CAT
video pid 264 descr id: 1101
audio pid 265 descr id: 1d02

ui_is_ttx_data_ready: -----1
video_out_ticks 6672
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
update signal
[CA MANAGER]: type:4, para1:15, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 456 
CA: set sid pgid: 15
MCAS_VIDEO_STOP
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x9
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
video pid 2c8 descr id: 1d01
audio pid 2c9 descr id: 1102

MCAS_NEW_CAT
ts data overflow:0x13
ui_is_ttx_data_ready: -----1
video_out_ticks 6934
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
update signal
[CA MANAGER]: type:4, para1:14, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 356 
CA: set sid pgid: 14
MCAS_VIDEO_STOP
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x5
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
on_ttx_ready: prog id = 14, curn pg =14 
video pid 264 descr id: 1101
audio pid 265 descr id: 1d02

MCAS_NEW_CAT
pg is scramble = 0, play type = 0
ui_is_ttx_data_ready: -----1
video_out_ticks 7130
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
update signal
[CA MANAGER]: type:4, para1:13, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 256 
CA: set sid pgid: 13
MCAS_VIDEO_STOP
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
video pid 200 descr id: 1d01
audio pid 201 descr id: 1102

ts data overflow:0x13
MCAS_NEW_CAT
ui_is_ttx_data_ready: -----1
video_out_ticks 7284
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3762112, alloced_peak = 3818336, rest_size = 4311864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
ts data overflow:0x13
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ui_stop_tkgs_monitor
TKGS IMPL DEBUG : function  iti_clear_attach_block, line 303clear attach block 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:40
ts data overflow:0x13
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:40, para2:1
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3725056, alloced_peak = 3818336, rest_size = 4348920

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
ui_start_tkgs_monitor
Type[12], i[1]
TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
ts data overflow:0x13
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3762112, alloced_peak = 3818336, rest_size = 4311864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3762112, alloced_peak = 3818336, rest_size = 4311864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
ts data overflow:0x13
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3762112, alloced_peak = 3818336, rest_size = 4311864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
ts data overflow:0x13
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3762112, alloced_peak = 3818336, rest_size = 4311864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3762112, alloced_peak = 3818336, rest_size = 4311864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
ts data overflow:0x13
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3762112, alloced_peak = 3818336, rest_size = 4311864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ts data overflow:0x13
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3743552, alloced_peak = 3818336, rest_size = 4330424

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:63
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:63, para2:31
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ts data overflow:0x13
ui_stop_tkgs_monitor
TKGS IMPL DEBUG : function  iti_clear_attach_block, line 303clear attach block 
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 262 
_switch_playstatus : 267 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:57
update signal
ts data overflow:0x13
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2ts data overflow:0x13
:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
[CA MANAGER]: type:12, para1:57, para2:36
ui_epg_api_get_evt_detail LINE:[582]
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
[CA MANAGER]: type:12, para1:36, para2:57
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
ui_start_tkgs_monitor
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:57, para2:1
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3790944, alloced_peak = 3829152, rest_size = 4283032

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:1, para2:31
Type[12], i[1]
TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:31, para2:1
ui_stop_tkgs_monitor
TKGS IMPL DEBUG : function  iti_clear_attach_block, line 303clear attach block 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
MCAS_VIDEO_STOP
UI: disable ttx.........
-----ui show logo v2 size 0xd4a9, 0, 179
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:1, para2:2
---------g_curn_menu_1=1
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a28380


 ###step3### msg.event 3
[CA MANAGER]: type:11, para1:2, para2:0
###ui_nw_api_on_plug_out dev_type[1]
p_cont[0x80c27824], root[0]
_switch_playstatus
thread usb_stor_control_thread exit
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: frousb_bus notify device REMOVE 
m 2 to 24 
[CA MANAGER]: type:12, para1:2, para2:24
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
[CA MANAGER]: type:12, para1:2, para2:2
update signal
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
---------------Time Stamp[15:39:47]----------------
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x0c000000 
auto_detect_usb_port --- usb sel port 1
USB:   Error, couldn't init Lowlevel part

** Invalid boot device **
do_spi_flash_uboot_save offset[0] len[2d600000]
spi0 is already setup!!!
SF: spi flash status register: 0x30, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x20, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x20, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: st ^-^
In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Jul  4 2017, 16:23:
9]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--15:38:22 symphony

 1. mem_start[80d1fbb0]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30490704
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D5CEC0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D79F60 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d272c0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d5cec0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Aug 25 2017 19:23:04/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80dc3280 p_wifi_dev 80dc3380 p_lld 80dc32d0 p_lld_addr 80dc3284 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a76de0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a76dfc --------
wifi dev = 0x80dc3600 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 564795 p_data_buffer 80e56ba0 

 unzip resource. in_addr = 0x9e362673, out_addr = 0x82a33c00, in_len = 564795, out_len = 1344464
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:258
[AI][_ai_eva_init]Entry...ticks:258
[AI][_ai_tuner_init]Entry...ticks:259
[AI][_ai_dvb_init]Entry...ticks:280
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:280
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:303
[AI][_ai_iconv_init]Entry...ticks:303
[AI][_ai_antenna_lnb_init]Entry...ticks:303
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:304
[AI][_ai_time_init]Entry...ticks:338
eve0
[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80d5b9c0
hub_add_new_dev 80e9bd40
port_reset 80d5b9c0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x83f9dc00
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
on_factory_test_uart LINE:[207]
welcome toon_factory_test_uart LINE:[234]
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
-----ui show logo v2 size 0xd599, 0, 179
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2646560, alloced_peak = 2723680, rest_size = 27844144

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON[NW] Set 3g sts:2
>    #3device ADD cost 159 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x8]

## timeshift exist is [1393786880]
p_cont[0x80eb8bf8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
update signal
_switch_playstatus
from_id = 2 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 3
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 2 to 68 
sat_id[0], sat_name[], lnb_low[5150], lnb_high[5150]
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[0], freq[3000], sym[1000], pol[0], 22k[0]
p_cont[0x80eb94b0], root[0]
_switch_playstatus
from_id = 68 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 24 
_switch_playstatus
from_id = 68 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 68 
p_cont[0x80eb94b0], root[0]
Delete Book Node [0]
Delete Book Node [1]
Delete Book Node [2]
Delete Book Node [3]
Delete Book Node [4]
Delete Book Node [5]
Delete Book Node [6]
Delete Book Node [7]
Delete Book Node [8]
Delete Book Node [9]
Delete Book Node [10]
Delete Book Node [11]
Delete Book Node [12]
Delete Book Node [13]
Delete Book Node [14]
Delete Book Node [15]
Delete Book Node [16]
Delete Book Node [17]
Delete Book Node [18]
Delete Book Node [19]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 68 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 73 
_switch_playstatus
from_id = 73 to_id = 64
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 64 
_switch_playstatus
from_id = 64 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 64 to 73 
ui_antenna_set: add sat is OK!
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 73 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 68 
PROGBAR: can NOT get pg!
_switch_playstatus
from_id = 68 to_id = 7
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 7 
update signal
ui_tp_set: add tp is OK!
sat_id[0], sat_name[0], lnb_low[5150], lnb_high[5150]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 1
---freq = 3150
---symbol = 27500
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[1], freq[3150], sym[27500], pol[0], 22k[0]
_switch_playstatus
from_id = 7 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 7 to 68 
update signal
_switch_playstatus
from_id = 68 to_id = 8
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 8 
on_epg_request_table_policy_switch
do scan pre open
set book flag
UI: deactive playback.........
set front panel
init static data
init scan
create timer for animation
_switch_playstatus
from_id = 8 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 8 to 9 
load sat id 0
PROCESS -> add/change sat[-2072879216]
PROCESS -> add/change tp
ADD TP -> freq[3150]
END ADD TP ->freq[3150]
PROCESS -> update progress
UPDATE PROGRESS -> 18
PROCESS -> update progress
UPDATE PROGRESS -> 36
PROCESS -> update progress
UPDATE PROGRESS -> 64
Found PG: s_id[6], v_pid[0], a_pid_0[915], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT FM], pmt_pid[357],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[7], v_pid[0], a_pid_0[916], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Ankara], pmt_pid[358],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[15], v_pid[0], a_pid_0[1117], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT EAST], pmt_pid[559],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[8], v_pid[0], a_pid_0[917], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 6], pmt_pid[359],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[10], v_pid[0], a_pid_0[1016], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WORLD], pmt_pid[457],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PiEïG -> name[V]
Found PG: s_id[11], v_pid[0], a_pid_0[1017], a_pid_1[0],a_pid_2[0], trace num[1], name[TSR TURKCE], pmt_pid[458],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[13], v_pid[0], a_pid_0[1115], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT NAGME], pmt_pid[557],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[14], v_pid[0], a_pid_0[1116], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURKU], pmt_pid[558],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[25], v_pid[1312], a_pid_0[1313], a_pid_1[1314],a_pid_2[0], trace num[2], name[TRT SPOR], pmt_pid[1056],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[28], v_pid[0], a_pid_0[1316], a_pid_1[0],a_pid_2[0], trace num[1], name[DIS YAY ORTA DALGA ARAPCA], pmt_pid[1257],scramble[0] 
impl_proceiEïss_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[D]
END ADD PG -> name[D]
Found PG: s_id[22], v_pid[0], a_pid_0[1315], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WEST], pmt_pid[757],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[1], v_pid[512], a_pid_0[513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT 1], pmt_pid[256],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[5], v_pid[612], a_pid_0[613], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT HABER], pmt_pid[356],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[9], v_pid[712], a_pid_0[713], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURK], pmt_pid[456],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[12], v_pid[812], a_pid_0[813], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT MUZIK], iEïpmt_pid[556],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[16], v_pid[912], a_pid_0[913], a_pid_1[914],a_pid_2[0], trace num[2], name[TRT COCUK], pmt_pid[656],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[21], v_pid[1012], a_pid_0[1013], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT AVAZ], pmt_pid[756],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[23], v_pid[1112], a_pid_0[1113], a_pid_1[0],a_pid_2[0], trace num[1], name[EURONEWS TURKCE], pmt_pid[856],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[24], v_pid[1212], a_pid_0[1213], a_pid_1[1214],a_pid_2[0], trace num[2], name[TRT ARAPCA], pmt_pid[956],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[26], v_pid[1412], a_pid_0[1413], a_pid_1[1416],a_pid_2[0], trace num[2], name[TRT KURDI], pmt_pid[1156],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[27], v_pid[1512], a_pid_0[1513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT DIYANET], pmt_pid[1256],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[20], v_pid[0], a_pid_0[1217], a_pid_1[0],a_pid_2[0], trace num[1], name[Trabzon Radyosu], pmt_pid[659],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[19], v_pid[0], a_pid_0[1216], a_pid_1[0],a_pid_2[0], trace num[1], name[Erzurum Radyosu], pmt_pid[658],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[18], v_pid[0], a_pid_0[1215], a_pid_1[0],a_pid_2[0], trace num[1], name[Cukurova Radyosu], pmt_pid[657],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[C]
END ADD PG -> name[C]
Found PG: s_id[2], v_pid[0], a_pid_0[815], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 1], pmt_pid[257],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[3], v_pid[0], a_pid_0[816], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 3], pmt_pid[258],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[4], v_pid[0], a_pid_0[817], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Istanbul], pmt_pid[259],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[17], v_pid[0], a_pid_0[1018], a_pid_1[0],a_pid_2[0], trace num[1], name[Antalya Radyosu], pmt_pid[459],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[A]
END ADD PG -> name[A]
db done ok
PROCESS -> update progress
UPDATE PROGRESS -> 100
PROCESS -> finish
*************************on finished : 3518
p_cont[0x80eb94b0], root[0]
_switch_playstatus
from_id = 9 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 24 
_switch_playstatus
from_id = 9 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 9 
*************************process finished : 3677
DO_SEARCH: before MSG_SAVE!
*************************do_search_post_close 1 : 3677
p_cont[0x80eb94b0], root[0]
do_search_post_close: reset the desktop notify func
------------->>active ap playback
UI: active playback.........
*************************do_search_post_close 2 : 3721
_switch_playstatus
from_id = 9 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[0] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 9 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2451136, alloced_peak = 2989408, rest_size = 28039568

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x83f9dc00
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
*************************close all menus : 3743
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 3829
ui_is_ttx_data_ready: -----1
on_prog_bar_notify_unsupport_format   para1 = 0
_check_hd_prog unsupport_flag = 0 
ui_is_ttx_data_ready: -----1
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 4037
ui_is_ttx_data_ready: -----1
on_prog_bar_notify_unsupport_format   para1 = 0
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3220960, alloced_peak = 3222880, rest_size = 27269744

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x5
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 5060
ui_is_ttx_data_ready: -----1
on_prog_bar_notify_unsupport_format   para1 = 0
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 14, curn pg =14 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 5366
ui_is_ttx_data_ready: -----1
on_prog_bar_notify_unsupport_format   para1 = 0
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3220928, alloced_peak = 3222880, rest_size = 27269776

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3220960, alloced_peak = 3222880, rest_size = 27269744

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 292 
_switch_playstatus : 297 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3221568, alloced_peak = 3222880, rest_size = 27269136

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
on_factory_test_uart LINE:[207]
welcome toon_factory_test_uart LINE:[234]
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
-----ui show logo v2 size 0xd599, 0, 179
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
---------------Time Stamp[15:44:47]----------------
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 2 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 3
UI: switch to PLAY..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 2 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2451840, alloced_peak = 3223456, rest_size = 28038864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x83f9dc00
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
ui_is_ttx_data_ready: -----1
video_out_ticks 27227
ui_is_ttx_data_ready: -----1
on_prog_bar_notify_unsupport_format   para1 = 0
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3202816, alloced_peak = 3223456, rest_size = 27287888

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
on_factory_test_uart LINE:[207]
welcome toon_factory_test_uart LINE:[234]
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
-----ui show logo v2 size 0xd599, 0, 179
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 2 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 3
UI: switch to PLAY..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 2 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2451840, alloced_peak = 3223456, rest_size = 28038864

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x83f9dc00
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 28175
ui_is_ttx_data_ready: -----1
on_prog_bar_notify_unsupport_format   para1 = 0
_check_hd_prog unsupport_flag = 0 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
on_factory_test_uart LINE:[207]
welcome toon_factory_test_uart LINE:[234]
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
-----ui show logo v2 size 0xd599, 0, 179
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d5cec0


 ###step3### msg.event 3
###ui_nw_api_on_plug_out dev_type[1]
p_cont[0x80eb8bf8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
thread usb_stor_control_thread exit
usb_bus notify device REMOVE 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
update signal
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d5cec0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports0 
 hub_add_new_dev hcd 80d5b9c0
hub_add_new_dev 80e9bd40
port_reset 80d5b9c0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8001205
###step1.2### 0 usb_hcd_poll_rh_status 
---------------Time Stamp[15:49:48]----------------
---------------Time Stamp[15:54:48]----------------
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d5cec0


 ###step3### msg.event 3
###ui_nw_api_on_plug_out dev_type[1]
p_cont[0x80eb8c74], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
thread usb_stor_control_thread exit
usb_bus notify device REMOVE 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
update signal
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d5cec0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports0 
 hub_add_new_dev hcd 80d5b9c0
hub_add_new_dev 80e9bd40
port_reset 80d5b9c0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8001205
###step1.2### 0 usb_hcd_poll_rh_status 
   #3device ADD cost 161 ts 
[AI][_ai_usb_plug_in_cb]Enter...
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run failed.
download failed!
monitor start
uboot run successful
download successful!

U-boot# 
U-boot# 
U-boot# 
U-boot# 
U-boot# 
U-boot# 
U-boot# 
U-boot# usb start 
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
U-boot# fatload usb 0 83000000 flash.bin
reading flash.bin

4194304 bytes read
U-boot# sf burn 83000000 0 400000
do_spi_flash_uboot_save offset[0] len[400000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
U-boot# ---------------Time Stamp[15:59:48]----------------
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BCB98CCCCV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=213990 213974 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4co841] Build Time:[Jul  4 2017, 
6:23:47]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b0d 48
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--15:56:28 symphony

 1. mem_start[8095b5c0]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 9035328
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:63
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 809994C0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 809B6560 [AI][_ai_dmx_init]Entry...ticks:64
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:66
priv->cfg.p_dem_bus =0x809638e0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:200
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c40000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d40000], size[180000], align[400], cfg size[1c01000]
tcpip: Aug 25 2017 19:23:17/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:204
file_size 313141 p_data_buffer 80a92ca0 

 unzip resource. in_addr = 0x9e297d07, out_addr = 0x811f9400, in_len = 313141, out_len = 905568
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:233
[AI][_ai_eva_init]Entry...ticks:234
[AI][_ai_tuner_init]Entry...ticks:234
[AI][_ai_dvb_init]Entry...ticks:255
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:255
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:279
[AI][_ai_iconv_init]Entry...ticks:279
[AI][_ai_antenna_lnb_init]Entry...ticks:279
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:280
[AI][_ai_time_init]Entry...ticks:314
eve0
[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80997fc0
hub_add_new_dev 80ad7c80
port_reset 80997fc0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x818d0400
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_siEïet_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2639968, alloced_peak = 2640960, rest_size = 6395360

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 160 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af4b38], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
update signal

## timeshift exist is [1393786880]
_switch_playstatus
from_id = 2 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 68 
sat_id[0], sat_name[], lnb_low[5150], lnb_high[5150]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[0], freq[3000], sym[1000], pol[0], 22k[0]
p_cont[0x80af53f0], root[0]
_switch_playstatus
from_id = 68 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 24 
_switch_playstatus
from_id = 68 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 68 
p_cont[0x80af53f0], root[0]
Delete Book Node [0]
Delete Book Node [1]
Delete Book Node [2]
Delete Book Node [3]
Delete Book Node [4]
Delete Book Node [5]
Delete Book Node [6]
Delete Book Node [7]
Delete Book Node [8]
Delete Book Node [9]
Delete Book Node [10]
Delete Book Node [11]
Delete Book Node [12]
Delete Book Node [13]
Delete Book Node [14]
Delete Book Node [15]
Delete Book Node [16]
Delete Book Node [17]
Delete Book Node [18]
Delete Book Node [19]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 68 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 73 
_switch_playstatus
from_id = 73 to_id = 64
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 64 
_switch_playstatus
from_id = 64 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 64 to 73 
ui_antenna_set: add sat is OK!
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 73 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 68 
PROGBAR: can NOT get pg!
_switch_playstatus
from_id = 68 to_id = 7
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 7 
ui_tp_set: add tp is OK!
sat_id[0], sat_name[0], lnb_low[5150], lnb_high[5150]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 1
---freq = 3150
---symbol = 27500
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[1], freq[3150], sym[27500], pol[0], 22k[0]
_switch_playstatus
from_id = 7 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 7 to 68 
update signal
_switch_playstatus
from_id = 68 to_id = 8
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 8 
on_epg_request_table_policy_switch
do scan pre open
set book flag
UI: deactive playback.........
set front panel
init static data
init scan
create timer for animation
_switch_playstatus
from_id = 8 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 8 to 9 
load sat id 0
PROCESS -> add/change sat[-2114396272]
PROCESS -> add/change tp
ADD TP -> freq[3150]
END ADD TP ->freq[3150]
PROCESS -> update progress
UPDATE PROGRESS -> 18
PROCESS -> update progress
UPDATE PROGRESS -> 36
PROCESS -> update progress
UPDATE PROGRESS -> 64
Found PG: s_id[6], v_pid[0], a_pid_0[915], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT FM], pmt_pid[357],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[7], v_pid[0], a_pid_0[916], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Ankara], pmt_pid[358],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[15], v_pid[0], a_pid_0[1117], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT EAST], pmt_pid[559],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[8], v_pid[0], a_pid_0[917], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 6], pmt_pid[359],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[10], v_pid[0], a_pid_0[1016], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WORLD], pmt_pid[457],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[11], v_pid[0], a_pid_0[1017], a_pid_1[0],a_pid_2[0], trace num[1], name[TSR TURKCE], pmt_pid[458],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[13], v_pid[0], a_pid_0[1115], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT NAGME], pmt_pid[557],scramble[0] 
impl_process_pg_list:new pg
PiEïROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[14], v_pid[0], a_pid_0[1116], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURKU], pmt_pid[558],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[25], v_pid[1312], a_pid_0[1313], a_pid_1[1314],a_pid_2[0], trace num[2], name[TRT SPOR], pmt_pid[1056],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[28], v_pid[0], a_pid_0[1316], a_pid_1[0],a_pid_2[0], trace num[1], name[DIS YAY ORTA DALGA ARAPCA], pmt_pid[1257],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[D]
END ADD PG -> name[D]
Found PG: s_id[22], v_pid[0], a_pid_0[1315], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WEST], pmt_pid[757],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[1], v_pid[512], a_pid_0[513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT iEï1], pmt_pid[256],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[5], v_pid[612], a_pid_0[613], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT HABER], pmt_pid[356],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[9], v_pid[712], a_pid_0[713], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURK], pmt_pid[456],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[12], v_pid[812], a_pid_0[813], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT MUZIK], pmt_pid[556],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[16], v_pid[912], a_pid_0[913], a_pid_1[914],a_pid_2[0], trace num[2], name[TRT COCUK], pmt_pid[656],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[21], v_pid[1012], a_pid_0[1013], a_piEïid_1[0],a_pid_2[0], trace num[1], name[TRT AVAZ], pmt_pid[756],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[23], v_pid[1112], a_pid_0[1113], a_pid_1[0],a_pid_2[0], trace num[1], name[EURONEWS TURKCE], pmt_pid[856],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[24], v_pid[1212], a_pid_0[1213], a_pid_1[1214],a_pid_2[0], trace num[2], name[TRT ARAPCA], pmt_pid[956],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[26], v_pid[1412], a_pid_0[1413], a_pid_1[1416],a_pid_2[0], trace num[2], name[TRT KURDI], pmt_pid[1156],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[27], v_pid[1512], a_pid_0[1513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT DIYANET], pmt_pid[1256],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[20], v_pid[0], a_pid_0[1217], a_pid_1[0],a_pid_2[0], trace num[1], name[Trabzon Radyosu], pmt_pid[659],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[19], v_pid[0], a_pid_0[1216], a_pid_1[0],a_pid_2[0], trace num[1], name[Erzurum Radyosu], pmt_pid[658],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[18], v_pid[0], a_pid_0[1215], a_pid_1[0],a_pid_2[0], trace num[1], name[Cukurova Radyosu], pmt_pid[657],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[C]
END ADD PG -> name[C]
Found PG: s_id[2], v_pid[0], a_pid_0[815], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 1], pmt_pid[257],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[3], v_pid[0], a_pid_0[816], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 3], pmt_pid[258],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[4], v_pid[0], a_pid_0[817], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Istanbul], pmt_pid[259],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[17], v_pid[0], a_pid_0[1018], a_pid_1[0],a_pid_2[0], trace num[1], name[Antalya Radyosu], pmt_pid[459],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[A]
END ADD PG -> name[A]
db done ok
PROCESS -> update progress
UPDATE PROGRESS -> 100
PROCESS -> finish
*************************on finished : 4503
p_cont[0x80af53f0], root[0]
_switch_playstatus
from_id = 9 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 24 
_switch_playstatus
from_id = 9 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 9 
*************************process finished : 6177
DO_SEARCH: before MSG_SAVE!
*************************do_search_post_close 1 : 6177
p_cont[0x80af53f0], root[0]
do_search_post_close: reset the desktop notify func
------------->>active ap playback
UI: active playback.........
*************************do_search_post_close 2 : 6205
_switch_playstatus
from_id = 9 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[0] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 9 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2445120, alloced_peak = 2983392, rest_size = 6590208

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818d0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
*************************close all menus : 6223
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 6315
_check_hd_prog unsupport_flag = 0 
ui_is_ttx_data_ready: -----1
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3196384, alloced_peak = 3215456, rest_size = 5838944

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
pg is scramble = 0, play type = 0
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 7085
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x19
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 7374
_check_hd_prog unsupport_flag = 0 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3196384, alloced_peak = 3216288, rest_size = 5838944

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
pg is scramble = 0, play type = 0
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 8425
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3214976, alloced_peak = 3216288, rest_size = 5820352

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 292 
_switch_playstatus : 297 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197792, alloced_peak = 3216992, rest_size = 5837536

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 2 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 2 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2446624, alloced_peak = 3217664, rest_size = 6588704

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818d0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
ui_is_ttx_data_ready: -----1
video_out_ticks 23497
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x5
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197984, alloced_peak = 3217664, rest_size = 5837344

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
ui_is_ttx_data_ready: -----1
video_out_ticks 24281
_check_hd_prog unsupport_flag = 0 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 292 
_switch_playstatus : 297 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197600, alloced_peak = 3217664, rest_size = 5837728

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 14, curn pg =14 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x9
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 25484
_check_hd_prog unsupport_flag = 0 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 292 
_switch_playstatus : 297 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3216416, alloced_peak = 3217664, rest_size = 5818912

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
---------------Time Stamp[16:04:48]----------------
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 3
###ui_nw_api_on_plug_out dev_type[1]
p_cont[0x80af4b38], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
thread usb_stor_control_thread exit
usb_bus notify device REMOVE 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
update signal
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports0 
 hub_add_new_dev hcd 80997fc0
hub_add_new_dev 80ad7c80
port_reset 80997fc0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8001205
###step1.2### 0 usb_hcd_poll_rh_status 
   #3device ADD cost 161 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af4b38], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
_switch_playstatus
from_id = 2 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 47 
UI: deactive playback.........
update signal

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af5200], root[0]
_switch_playstatus
from_id = 47 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 24 
_switch_playstatus
from_id = 47 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 47 
p_cont[0x80af5200], root[0]
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB98CCCCV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=213990 213974 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x8800000, status=0xff01
avcpu ver = AVCPU_VERSION:[501:723fde4cc841] Build Time:[Jul  4 2017, 
6:23:47]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b0d 48
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--16:04:52 symphony

 1. mem_start[8095b5c0]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 9035328
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:13
[AI][_ai_uio_init]Entry...ticks:13
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:14
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:63
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 809994C0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 809B6560 [AI][_ai_dmx_init]Entry...ticks:64
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:66
priv->cfg.p_dem_bus =0x809638e0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:200
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c40000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d40000], size[180000], align[400], cfg size[1c01000]
tcpip: Aug 25 2017 19:23:17/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:204
file_size 313141 p_data_buffer 80a92ca0 

 unzip resource. in_addr = 0x9e297d07, out_addr = 0x811f9400, in_len = 313141, out_len = 905568
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:233
[AI][_ai_eva_init]Entry...ticks:233
[AI][_ai_tuner_init]Entry...ticks:234
[AI][_ai_dvb_init]Entry...ticks:255
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:255
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:256
[AI][_ai_iconv_init]Entry...ticks:256
[AI][_ai_antenna_lnb_init]Entry...ticks:256
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:257
[AI][_ai_time_init]Entry...ticks:292
eve0
[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80997fc0
hub_add_new_dev 80ad7c80
port_reset 80997fc0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_i&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
d = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x818d0400
end desktop init
get ver 0
close_fast_logo
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2610752, alloced_peak = 2610752, rest_size = 6424576

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 0 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 31 
switch_autoclose: reset tmr 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[0] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filteiEïr info: net_id:0x2a,ts_id:0x3d,s_id:0x9
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
update signal
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2705824, alloced_peak = 2707744, rest_size = 6329504

EMON> [NW] Set 3g sts:2
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
update signal
   #3ui_is_ttx_data_ready: -----1
device ADD cost 159 ts 
[AI][_ai_usb_plug_in_cb]Enter...
ui_is_ttx_data_ready: -----1
video_out_ticks 477
_check_hd_prog unsupport_flag = 0 
ui_is_ttx_data_ready: -----1

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af4c30], root[0]
_switch_playstatus
from_id = 31 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 24 
switch_autoclose: destroy tmr 
on_ttx_ready: prog id = 15, curn pg =15 
on_ttx_ready: prog id = 15, curn pg =15 
_switch_playstatus
from_id = 31 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 31 
switch_autoclose: create tmr 
update signal

## timeshift exist is [1393786880]
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x5
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 1091
_check_hd_prog unsupport_flag = 0 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 1248
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3195456, alloced_peak = 3369568, rest_size = 5839872

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
_switch_playstatus
from_id = 2 to_id = 4
new_ps = 2 CURN_MENU_PLAY_STATE = 4
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 292 
_switch_playstatus : 297 
UI: swithced to PREV........
switch_autoclose: from 2 to 4 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
update signal
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
_switch_playstatus
from_id = 4 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 2
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 4 to 2 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 2 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 2 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2462880, alloced_peak = 3369568, rest_size = 6572448

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818d0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
on_ttx_ready: prog id = 13, curn pg =13 
Type[12], i[1]
video_out_ticks 2777
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 292 
_switch_playstatus : 297 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3195424, alloced_peak = 3369568, rest_size = 5839904

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 292 
_switch_playstatus : 297 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197792, alloced_peak = 3369568, rest_size = 5837536

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 3
###ui_nw_api_on_plug_out dev_type[1]
p_cont[0x80af4b38], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
thread usb_stor_control_thread exit
usb_bus notify device REMOVE 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
update signal
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports0 
 hub_add_new_dev hcd 80997fc0
hub_add_new_dev 80be88a0
port_reset 80997fc0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8001205
###step1.2### 0 usb_hcd_poll_rh_status 
device ADD cost 161 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af4b38], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
_switch_playstatus
from_id = 2 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 47 
UI: deactive playback.........
update signal

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af4e9c], root[0]
_switch_playstatus
from_id = 47 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 24 
_switch_playstatus
from_id = 47 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 47 
p_cont[0x80af4e9c], root[0]
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=213990 213974 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x8800000, status=0xff03
avcpu ver = AVCPU_VERSION:[501:723fde4cc841] Build Time:[Jul  4 2017, 
6:23:47]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b0d 48
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--16:07:45 symphony

 1. mem_start[8095b5c0]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 9035328
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:13
[AI][_ai_uio_init]Entry...ticks:13
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:14
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:63
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 809994C0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 809B6560 [AI][_ai_dmx_init]Entry...ticks:64
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:66
priv->cfg.p_dem_bus =0x809638e0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:200
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c40000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d40000], size[180000], align[400], cfg size[1c01000]
tcpip: Aug 25 2017 19:23:17/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:204
file_size 313141 p_data_buffer 80a92ca0 

 unzip resource. in_addr = 0x9e297d07, out_addr = 0x811f9400, in_len = 313141, out_len = 905568
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:233
[AI][_ai_eva_init]Entry...ticks:233
[AI][_ai_tuner_init]Entry...ticks:234
[AI][_ai_dvb_init]Entry...ticks:255
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:255
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:256
[AI][_ai_iconv_init]Entry...ticks:256
[AI][_ai_antenna_lnb_init]Entry...ticks:256
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:257
[AI][_ai_time_init]Entry...ticks:292
eve0
[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80997fc0
hub_add_new_dev 80ad7c80
port_reset 80997fc0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_i&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
d = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x818d0400
end desktop init
get ver 0
close_fast_logo
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2610752, alloced_peak = 2610752, rest_size = 6424576

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 0 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 31 
switch_autoclose: reset tmr 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[0] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epgiEï api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
update signal
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2705824, alloced_peak = 2707744, rest_size = 6329504

EMON> [NW] Set 3g sts:2
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
update signal
   #3ui_is_ttx_data_ready: -----1
device ADD cost 160 ts 
[AI][_ai_usb_plug_in_cb]Enter...
ui_is_ttx_data_ready: -----1
video_out_ticks 459
_check_hd_prog unsupport_flag = 0 
ui_is_ttx_data_ready: -----1

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af4c30], root[0]
_switch_playstatus
from_id = 31 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 24 
switch_autoclose: destroy tmr 
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 31 
switch_autoclose: create tmr 
update signal

## timeshift exist is [1393786880]
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 2 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 2 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2444320, alloced_peak = 3369440, rest_size = 6591008

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818d0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 1480
_check_hd_prog unsupport_flag = 0 
ui_is_ttx_data_ready: -----1
ui_is_ttx_data_ready: -----1
on_ttx_ready: prog id = 13, curn pg =13 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 1
UI: switch to PREV..........
UI: swithced to PREV........std=9
_switch_playstatus : 292 
_switch_playstatus : 297 
UI: swithced to PREV........
switch_autoclose: from 1 to 57 
switch_autoclose: destroy tmr 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 36
new_ps = 0 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 57 to 36 
---------------Time Stamp[16:09:48]----------------
_switch_playstatus
from_id = 36 to_id = 57
new_ps = 2 CURN_MENU_PLAY_STATE = 2
switch_autoclose: from 36 to 57 
update signal
_switch_playstatus
from_id = 57 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 2
UI: switch to PLAY..........
switch_autoclose: from 57 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197760, alloced_peak = 3369440, rest_size = 5837568

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 2 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 2 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2446656, alloced_peak = 3369440, rest_size = 6588672

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818d0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
ui_is_ttx_data_ready: -----1
video_out_ticks 4036
_check_hd_prog unsupport_flag = 0 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3216320, alloced_peak = 3369440, rest_size = 5819008

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 40 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197760, alloced_peak = 3369440, rest_size = 5837568

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
_switch_playstatus
from_id = 1 to_id = 40
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 40 
switch_autoclose: destroy tmr 
= 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 40 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3216320, alloced_peak = 3369440, rest_size = 5819008

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 13, curn pg =13 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x19
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 4955
_check_hd_prog unsupport_flag = 0 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x1
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x5
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 5485
_check_hd_prog unsupport_flag = 0 
pg is scramble = 0, play type = 0
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x9
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 5639
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 15, curn pg =15 
on_ttx_ready: prog id = 15, curn pg =15 
on_ttx_ready: prog id = 15, curn pg =15 
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
_switch_playstatus
from_id = 2 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 47 
UI: deactive playback.........
p_cont[0x80af4e9c], root[0]
_switch_playstatus
from_id = 47 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 24 
_switch_playstatus
from_id = 47 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 47 
p_cont[0x80af4e9c], root[0]
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB98CCCCV
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
 size1=213990 213974 
 main_start =0x83e10000 0x9e010410 

 load_secondary_core_boot_word : secondary_img_start = 0x83e10000 
concerto_check_cpu_ready: start

 ^-^ In main , ebase=0x83e01001, cause=0x8800000, status=0xff03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841] Build Time:[Jul  4 2017, 16:23:47]
concerto_check_cpu_ready: start
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8b0d 48
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--16:07:45 symphony

 1. mem_start[8095b5c0]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 9035328
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:13
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:14
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:65
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 809994C0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 809B6560 [AI][_ai_dmx_init]Entry...ticks:66
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x809638e0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:201
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c40000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d40000], size[180000], align[400], cfg size[1c01000]
tcpip: Aug 25 2017 19:23:17/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:205
file_size 313141 p_data_buffer 80a92ca0 

 unzip resource. in_addr = 0x9e297d07, out_addr = 0x811f9400, in_len = 313141, out_len = 905568
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:234
[AI][_ai_eva_init]Entry...ticks:235
[AI][_ai_tuner_init]Entry...ticks:235
[AI][_ai_dvb_init]Entry...ticks:256
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:256
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:280
[AI][_ai_iconv_init]Entry...ticks:280
[AI][_ai_antenna_lnb_init]Entry...ticks:281
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:281
[AI][_ai_time_init]Entry...ticks:316
eve0
[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80997fc0
hub_add_new_dev 80ad7c80
port_reset 80997fc0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
 = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x818d0400
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2639968, alloced_peak = 2640960, rest_size = 6395360

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 160 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af4b38], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
update signal

## timeshift exist is [1393786880]
_switch_playstatus
from_id = 2 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 68 
sat_id[0], sat_name[], lnb_low[5150], lnb_high[5150]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[0], freq[3000], sym[1000], pol[0], 22k[0]
p_cont[0x80af53f0], root[0]
_switch_playstatus
from_id = 68 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 24 
_switch_playstatus
from_id = 68 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 68 
p_cont[0x80af53f0], root[0]
Delete Book Node [0]
Delete Book Node [1]
Delete Book Node [2]
Delete Book Node [3]
Delete Book Node [4]
Delete Book Node [5]
Delete Book Node [6]
Delete Book Node [7]
Delete Book Node [8]
Delete Book Node [9]
Delete Book Node [10]
Delete Book Node [11]
Delete Book Node [12]
Delete Book Node [13]
Delete Book Node [14]
Delete Book Node [15]
Delete Book Node [16]
Delete Book Node [17]
Delete Book Node [18]
Delete Book Node [19]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 68 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 73 
_switch_playstatus
from_id = 73 to_id = 64
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 64 
_switch_playstatus
from_id = 64 to_id = 73
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 64 to 73 
ui_antenna_set: add sat is OK!
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 0
---freq = 3000
---symbol = 1000
---polarity = H
---tuner_id = 0
----------------------------------
_switch_playstatus
from_id = 73 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 73 to 68 
PROGBAR: can NOT get pg!
_switch_playstatus
from_id = 68 to_id = 7
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 7 
ui_tp_set: add tp is OK!
sat_id[0], sat_name[0], lnb_low[5150], lnb_high[5150]
--------------ui_set_antenna_and_transpond--------------------
- set antenna id = 0, p_sat->is_t2_sat: 0
---lnb low = 5150 high = 5150
---lnb pow = 0 22k = 0
---diseqc type = 0 port = 0
---nim type = 0
- set transpond id = 1
---freq = 3150
---symbol = 27500
---polarity = H
---tuner_id = 0
----------------------------------
tp_id[1], freq[3150], sym[27500], pol[0], 22k[0]
_switch_playstatus
from_id = 7 to_id = 68
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 7 to 68 
on_epg_request_table_policy_switch
update signal
_switch_playstatus
from_id = 68 to_id = 8
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 68 to 8 
do scan pre open
set book flag
UI: deactive playback.........
set front panel
init static data
init scan
create timer for animation
_switch_playstatus
from_id = 8 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 8 to 9 
load sat id 0
PROCESS -> add/change sat[-2114396272]
PROCESS -> add/change tp
ADD TP -> freq[3150]
END ADD TP ->freq[3150]
PROCESS -> update progress
UPDATE PROGRESS -> 18
PROCESS -> update progress
UPDATE PROGRESS -> 36
PROCESS -> update progress
UPDATE PROGRESS -> 64
Found PG: s_id[6], v_pid[0], a_pid_0[915], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT FM], pmt_pid[357],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[7], v_pid[0], a_pid_0[916], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Ankara], pmt_pid[358],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[15], v_pid[0], a_pid_0[1117], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT EAST], pmt_pid[559],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[8], v_pid[0], a_pid_0[917], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 6], pmt_pid[359],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[10], v_pid[0], a_pid_0[1016], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WORLD], pmt_pid[457],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[11], v_pid[0], a_pid_0[1017], a_pid_1[0],a_pid_2[0], trace num[1], name[TSR TURKCE], pmt_pid[458],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[13], v_pid[0], a_pid_0[1115], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT NAGME], pmt_pid[557],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> iEïadd prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[1], v_pid[512], a_pid_0[513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT 1], pmt_pid[256],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[2], v_pid[0], a_pid_0[815], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 1], pmt_pid[257],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[3], v_pid[0], a_pid_0[816], a_pid_1[0],a_pid_2[0], trace num[1], name[RADYO 3], pmt_pid[258],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[R]
END ADD PG -> name[R]
Found PG: s_id[4], v_pid[0], a_pid_0[817], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT Kent Radyo Istanbul], pmt_pid[259],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[5], v_pid[612], a_pid_0[613], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT HABER], pmt_pid[356],scramble[0]iEï 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[9], v_pid[712], a_pid_0[713], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURK], pmt_pid[456],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[12], v_pid[812], a_pid_0[813], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT MUZIK], pmt_pid[556],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[14], v_pid[0], a_pid_0[1116], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT TURKU], pmt_pid[558],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[16], v_pid[912], a_pid_0[913], a_pid_1[914],a_pid_2[0], trace num[2], name[TRT COCUK], pmt_pid[656],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[17], v_pid[0], a_pid_0[1018], a_pid_1[0],a_pid_2[0], trace num[1iEï], name[Antalya Radyosu], pmt_pid[459],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[A]
END ADD PG -> name[A]
Found PG: s_id[18], v_pid[0], a_pid_0[1215], a_pid_1[0],a_pid_2[0], trace num[1], name[Cukurova Radyosu], pmt_pid[657],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[C]
END ADD PG -> name[C]
Found PG: s_id[19], v_pid[0], a_pid_0[1216], a_pid_1[0],a_pid_2[0], trace num[1], name[Erzurum Radyosu], pmt_pid[658],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[20], v_pid[0], a_pid_0[1217], a_pid_1[0],a_pid_2[0], trace num[1], name[Trabzon Radyosu], pmt_pid[659],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[21], v_pid[1012], a_pid_0[1013], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT AVAZ], pmt_pid[756],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[22], v_pid[0], a_pid_0[1315], a_pid_1[0],a_pid_2[0], trace num[1], name[VOT WEST], pmt_pid[757],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[V]
END ADD PG -> name[V]
Found PG: s_id[23], v_pid[1112], a_pid_0[1113], a_pid_1[0],a_pid_2[0], trace num[1], name[EURONEWS TURKCE], pmt_pid[856],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[E]
END ADD PG -> name[E]
Found PG: s_id[24], v_pid[1212], a_pid_0[1213], a_pid_1[1214],a_pid_2[0], trace num[2], name[TRT ARAPCA], pmt_pid[956],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[25], v_pid[1312], a_pid_0[1313], a_pid_1[1314],a_pid_2[0], trace num[2], name[TRT SPOR], pmt_pid[1056],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[26], v_pid[1412], aiEï_pid_0[1413], a_pid_1[1416],a_pid_2[0], trace num[2], name[TRT KURDI], pmt_pid[1156],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[27], v_pid[1512], a_pid_0[1513], a_pid_1[0],a_pid_2[0], trace num[1], name[TRT DIYANET], pmt_pid[1256],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[T]
END ADD PG -> name[T]
Found PG: s_id[28], v_pid[0], a_pid_0[1316], a_pid_1[0],a_pid_2[0], trace num[1], name[DIS YAY ORTA DALGA ARAPCA], pmt_pid[1257],scramble[0] 
impl_process_pg_list:new pg
PROCESS -> add prog
ADD PG -> name[D]
END ADD PG -> name[D]
db done ok
PROCESS -> update progress
UPDATE PROGRESS -> 100
PROCESS -> finish
*************************on finished : 3533
p_cont[0x80af53f0], root[0]
_switch_playstatus
from_id = 9 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 24 
_switch_playstatus
from_id = 9 to_id = 9
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 9 to 9 
*************************process finished : 14670
DO_SEARCH: before MSG_SAVE!
*************************do_search_post_close 1 : 14670
p_cont[0x80af53f0], root[0]
do_search_post_close: reset the desktop notify func
------------->>active ap playback
UI: active playback.........
*************************do_search_post_close 2 : 14699
_switch_playstatus
from_id = 9 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 4
UI: switch to PLAY..........
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[0] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
switch_autoclose: from 9 to 1 
switch_autoclose: create tmr 
update signal
on open_nprog bar---
 mtos_mem_user_debug, alloced = 2445120, alloced_peak = 2983392, rest_size = 6590208

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_ui_epg_api_init epg addr 0x818d0400
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
*************************close all menus : 14717
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
ui_is_ttx_data_ready: -----1
video_out_ticks 14896
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 9, curn pg =9 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197856, alloced_peak = 3217600, rest_size = 5837472

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
on_ttx_ready: prog id = 9, curn pg =9 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197600, alloced_peak = 3217600, rest_size = 5837728

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3216416, alloced_peak = 3217600, rest_size = 5818912

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
on_ttx_ready: prog id = 9, curn pg =9 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197600, alloced_peak = 3218240, rest_size = 5837728

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197600, alloced_peak = 3218240, rest_size = 5837728

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
pg is scramble = 0, play type = 0
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x5
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 15845
_check_hd_prog unsupport_flag = 0 
on_ttx_ready: prog id = 13, curn pg =13 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3197600, alloced_peak = 3218240, rest_size = 5837728

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
Type[12], i[1]
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3216160, alloced_peak = 3218240, rest_size = 5819168

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
pg is scramble = 0, play type = 0
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[1] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
update signal
epg api set filter info: net_id:0x2a,ts_id:0x3d,s_id:0x9
UI: enable ttx.........
UI: set ttx language [eng].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
ui_is_ttx_data_ready: -----1
video_out_ticks 16460
_check_hd_prog unsupport_flag = 0 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on open_nprog bar---
 mtos_mem_user_debug, alloced = 3216160, alloced_peak = 3218240, rest_size = 5819168

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_id = 1 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 1 to 31 
switch_autoclose: reset tmr 
ui_is_ttx_data_ready: -----1
on_ttx_ready: prog id = 14, curn pg =14 
_switch_playstatus
from_id = 31 to_id = 63
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 63 
switch_autoclose: destroy tmr 
on_ttx_ready: prog id = 14, curn pg =14 
_switch_playstatus
from_id = 63 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 63 to 31 
switch_autoclose: create tmr 
update signal
_switch_playstatus
from_id = 31 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 1 
switch_autoclose: reset tmr 
on close epg before open mainmenu
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 1 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 1
UI: switch to STOP..........
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
switch_autoclose: from 1 to 2 
switch_autoclose: destroy tmr 
0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
---------------Time Stamp[16:14:48]----------------
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] c00000a
ehci_port_status: PORT_DISCONNECT
###step1.2### 3 usb_hcd_poll_rh_status 


 ###step2###3 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 3
###ui_nw_api_on_plug_out dev_type[1]
p_cont[0x80af4bb4], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
thread usb_stor_control_thread exit
usb_bus notify device REMOVE 
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 809994c0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 1803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate ports0 
 hub_add_new_dev hcd 80997fc0
hub_add_new_dev 80ad7c80
port_reset 80997fc0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8001205
###step1.2### 0 usb_hcd_poll_rh_status 
   #3device ADD cost 161 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
p_cont[0x80af4bb4], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 2 
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x11]
_switch_playstatus
from_id = 2 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 2 to 47 
UI: deactive playback.........
update signal

## timeshift exist is [1393786880]
p_cont[0x80af5200], root[0]
_switch_playstatus
from_id = 47 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 24 
_switch_playstatus
from_id = 47 to_id = 47
new_ps = 4 CURN_MENU_PLAY_STATE = 4
switch_autoclose: from 47 to 47 
Barcode thread exit
Upgrade thread exit
monitor exit
Serial Port Opened
monitor start
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync time out.
Sync Failed.
can't sync with btinit_ddr2_400m_debug.img
download failed!
monitor start
monitor stop
Serial Port Closed
upg or dump task  is canceled!
Serial Port Opened
monitor start
monitor stop
Serial Port Closed
upg or dump task  is canceled!
Serial Port Opened
monitor start
monitor stop
Barcode thread exit
Upgrade thread exit
monitor exit
Serial Port Opened
monitor start
[FastLogo][ap_init:740]End...
boot_para1: addr 0xbf140038 = 0x12340088
boot_para2: addr 0xbf14003c = 0x80008000
boot_para3: addr 0xbf30f060 = 0x12340001
FastLogo_TaskEnd, Jump:0x80100000
*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 0MiBytes
20 MiB
bootinit version: 37_4a35d9b5f498
U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:39)
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--16:15:50 symphony

 1. mem_start[809de108]

 2. whole memory size[4000000]

 3. sys partition size(free_mem) 8073976
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
lpower_symphony_attach
[AI][_ai_jpeg_init]Entry...ticks:2
[AI][_ai_i2c_qam_init]Entry...ticks:3
[AI][_ai_i2c_init]Entry...ticks:3
[AI][_ai_i2c_1_init]Entry...ticks:3
[AI][_ai_i2c_fp_init]Entry...ticks:4
[AI][_ai_i2c_hdmi_init]Entry...ticks:4
[AI][_ai_spi_init]Entry...ticks:4
[AI][_ai_dm_init]Entry...ticks:5
[AI][_ai_dm_init]dm init v2...ticks:5
[AI][_ai_dm_init]set header...ticks:6
[AI][_ai_uio_init]Entry...ticks:6
[_fp_attach]Entry..., type:2
lpower cfg :pd_key 0x0
 
                pd_key1 0x0
 
                pd_key_fp 0x57
 
                type 0x3
 
                raw_map [0x0][0x1][0x2][0x3][0x4][0x5][0x6][0x7]

[AI][_ai_hdmi_init]EntriEïy...ticks:8
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
hdmi_debug: p_priv->is_support_dvi_mode 0 p_priv->is_fastlogo_mode 0,p_priv 0x80a263e0,ahg_rw 1
hdmi in main code
HDMI:hdmi_anx8560_open, 5278
  hdmi is_initialized 1hdmi_anx8560_open receiver BKSV is 47 74 18 2b bb
[AI][_ai_audio_init]Entry...ticks:57
[AI][_ai_video_init]Entry...ticks:57
[AI][_ai_usb_init]Entry...ticks:60
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80A28380 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80A45420 [AI][_ai_dmx_init]Entry...ticks:61
dmx modify  version: 36142
dmx_symphony_tsi_set_es_buffer error !!!
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:63
priv->cfg.p_dem_bus =0x809e6420
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80a28380


 ###step3### msg.event 2
hdmi_hdcp: anx8560_service 3688    events 48 a1 0x0 irq_id 0x16
video format change line 2&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:196
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[83c20000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a1d20000], size[180000], align[400], cfg size[1c01000]
tcpip: Jul 19 2017 11:32:22/nthread task for ethernet 9 
attach wifi 5370 success
serial_open
[register_rtsp_stream][ERROR][ERROR] --do nothing !!!!!!!!!!
[register_rtsp_stream] please config ENABLE_DEMUX_RTSP = Y!!!!!! !!
[AI][_ai_mdl_init]Entry...ticks:201
file_size 345801 p_data_buffer 80b1c100 

 unzip resource. in_addr = 0x9e2c31a4, out_addr = 0x81191400, in_len = 345801, out_len = 989176
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:233
[AI][_ai_eva_init]Entry...ticks:234
[AI][_ai_tuner_init]Entry...ticks:234
[AI][_ai_dvb_init]Entry...ticks:255
[CA]: init
[AI][_ai_dmm_init]Entry...ticks:255
[AI][_ai_mdl_init]Software Ver[H0.95.80010S.021]
[AI][_ai_avc_init]Entry...ticks:256
[AI][_ai_iconv_init]Entry...ticks:256
[AI][_ai_antenna_lnb_init]Entry...ticks:257
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:257
hdmi_anx8560_video_config start res6, pn 2 
hdmi_tx_de_gen_en!


 @@@@@@@@@@@@@@@ cspace_y2r 0 up_sample 0 range_y2r 0 cspace_r2y 0 down_sample 0 p_output_cfg->csc 2
MISC_Reset!
hdmi_debug : hdcp off, g_hdmi_edid_result.is_hdmi 1



 new:  mute 0 is_in_mute 0 prio6 
hdmi_debug : g_hdmi_edid_result.is_hdmi 1
 !!!!!!!!!!!!!!!!!!!!!!!!!    hdmi analog reset   reg 0xbf157000, value 0x1000080 
 !!!!!!!!!!!!!!!!!!!!!!!!!     hdmi analog reset  reg 0xbf157000, value 0x1000000 
[AI][_ai_time_init]Entry...ticks:295
[CA]===>construct_cas_policy
[CA MANAGER]: type:0, para1:0, para2:0
set ca addr is 0x0
cas_adt_ncs_attach
0x000000000
7:b364a56bb03b
eve0
5876[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80a26e80
hub_add_new_dev 80b7da00
port_reset 80a26e80
close_fast_logo
mmi init
mmi ver 
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
[CA MANAGER]: type:12, para1:0&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
, para2:1
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x818b0400
[CA MANAGER]: type:1, para1:0, para2:0
end desktop init
get ver 0
[CA MANAGER]: type:2, para1:0, para2:0
close_fast_logo


======================================================

sn_num:[0000000000000000],mac_address:[000000000000]

======================================================

on open_nprog bar---
 mtos_mem_user_debug, alloced = 3201600, alloced_peak = 3201600, rest_size = 4872376

@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
ui epg already init!
_switch_playstatus
from_iiEïd = 0 to_id = 31
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 31 
switch_autoclose: reset tmr 
[CA MANAGER]: type:12, para1:0, para2:31
ui_start_tkgs_monitor
@ui_signal.c->clean_pg_scramble = [0]

 g_play_mode[0] curn_mode[1]
default, fast play!!!
default, fast play!!!need stop firstly.
[CA MANAGER]: type:5, para1:0, para2:0
CA: stop
910
update signal
[CA MANAGER]: type:4, para1:6, para2:0
ORBIT: 0
ca_sid.pmt_pid  = 4222 
CA: set sid pgid: 6
MCAS_VIDEO_STOP
audio cfg @HDMI_TX_SYS_CTRL1_REG@   3
audio_type = 0x02
config i2s channel, c = 0x04
config i2s format, c = 0x00
down sample, c = 0x00
audio sample rate set to 48K
Audio MCLK input mode is: 01
anx8560_audio_input_cfg 1742 
audio cfg success 
epg api set filter info: net_id:0x233a,ts_id:0x103e,s_id:0x107e
UI: enable ttx.........
UI: set ttx language [tur].........
UI: enable subt.........
ui_is_ttx_data_ready: -----1
update signal
[CA MANAGER]: type:3, para1:0, para2:0
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 3230720, alloced_peak = 3232640, rest_size = 4843256

TKGS IMPL DEBUG : function  iti_set_attach_block, line 276set attach block 
--rex----block_id 8, total_size 1310720-----
--rex--111--- total_size 1046992
--rex--2222--size=49152- total_size 1096144
--rex--2222--size=4000- total_size 1100144
EMON> [NW] Set 3g sts:2
audio cfg @HDMI_TX_SYS_CTRL1_REG@   3
audio_type = 0x02
config i2s channel, c = 0x84
config i2s format, c = 0x00
down sample, c = 0x01
audio sample rate set to 48K
Audio MCLK input mode is: 01
anx8560_audio_input_cfg 1742 
HDMI_TX_INFO_PKTCTRL2_REG = 1
HDMI_TX_INFO_PKTCTRL2_REG = 1
HDMI_TX_INFO_PKTCTRL2_REG = 1
audio cfg success 
update signal
video pid c9 descr id: 201
audio pid ca descr id: 102

ui_is_ttx_data_ready: -----1
   #3ui_is_ttx_data_ready: -----1
video_out_ticks 433
device ADD cost 159 ts 
[AI][_ai_usb_plug_in_cb]Enter...
on_subt_ready: prog id = 6, curn pg =6 

## timeshift exist is [1393786880]
[CA MANAGER]: type:10, para1:31, para2:0
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x10]
p_cont[0x80c276b0], root[0]
_switch_playstatus
from_id = 31 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 31 to 24 
switch_autoclose: destroy tmr 
[CA MANAGER]: type:12, para1:31, para2:24
ui_is_ttx_data_ready: -----1
on_subt_ready: prog id = 6, curn pg =6 
on_subt_ready: prog id = 6, curn pg =6 
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 1 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found
reading flash.bin

8388608 bytes read
do_spi_flash_uboot_save offset[0] len[800000]
spi0 is already setup!!!
SF: spi flash status register: 0x30, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
save uboot to flash
system will reboot
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBB99CCCCV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x30, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257588 257572 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: st ^-^
In main , ebase=0x87e01001, cause=0x8800000, status=0xda03
avcpu ver = AVCPU_VERSION:[501:723fde4bc841]couild Time:[Jul  4 2017, 16:23:
9]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x800a
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
10123
 MaincodeTaskStart

 Built at Aug 30 2017--15:48:31 symphony

 1. mem_start[80d1fbb0]

 2. whole memory size[8000000]

 3. sys partition size(free_mem) 30490704
**CDU UDQ**: 8d2e 4e
Os version pass!
Enable irq!
Message init!
Timer init!
Bus monitor init!
[AI][ap_init]Entry...
[AI][_ai_drv_init]Entry...
[AI][_ai_gpe_init]Entry...ticks:2
[AI][_ai_vbi_init]Entry...ticks:2
-- --0xBF13C010 -- get ---[0x220000]--
-- GPIO5---0xBF13C010 -- set---[0x221000]--
-- GPIO5---get -- GPIO_LEVEL_HIGH--old-HW---
-- after-GPIO5--read-,-reback--0xBF13C010 -- get ---[0x220000]----
[AI][_ai_jpeg_init]Entry...ticks:9
[AI][_ai_i2c_qam_init]Entry...ticks:9
[AI][_ai_i2c_init]Entry...ticks:10
[AI][_ai_i2c_1_init]Entry...ticks:10
[AI][_ai_i2c_fp_init]Entry...ticks:10
[AI][_ai_i2c_hdmi_init]Entry...ticks:10
[AI][_ai_spi_init]Entry...ticks:11
[AI][_ai_dm_init]Entry...ticks:12
[AI][_ai_dm_init]dm init v2...ticks:12
[AI][_ai_dm_init]set header...ticks:12
[AI][_ai_uio_init]Entry...ticks:12
[_fp_attach]Entry..., type:2
[AI][_ai_hdmi_init]Entry...ticks:13
=============>hdmi init..............
*********hdmi config value=12340001
*********hdmi is config
[AI][_ai_audio_init]Entry...ticks:60
[AI][_ai_video_init]Entry...ticks:60
[AI][_ai_usb_init]Entry...ticks:64
----usb_mass_stor_attach usb1------
g_usb_bus * g_usb_bus = 80D5CEC0 ----usb_mass_stor_attach usb0------
g_usb_bus * g_usb_bus = 80D79F60 [AI][_ai_dmx_init]Entry...ticks:65
#####0xbf156014[0]
#####0xbf156308[0]
#####0xbf15601c[0]
[AI][_ai_display_init]Entry...ticks:68
priv->cfg.p_dem_bus =0x80d272c0
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
###step1.2### 2 usb_hcd_poll_rh_status 


 ###step2###2 usb_hcd_poll_rh_status  msgq 0  hcd->bus 80d5cec0


 ###step3### msg.event 2
&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 803
ehci_port_status: PORT_CONNECT
USB @2 start enumerate p[AI][_ai_mute_set]Entry...ticks:202
[AI][_ai_av_buf_init]Enter...
[AI][_ai_av_buf_init]Audio Buf[87a80000], size[180000], align[400]
[AI][_ai_av_buf_init]video Buf[a44d8000], size[180000], align[400], cfg size[31ac000]
tcpip: Aug 25 2017 19:23:04/nthread task for ethernet 9 
rtl8188eus_ethernet_attach p_dev80dc3280 p_wifi_dev 80dc3380 p_lld 80dc32d0 p_lld_addr 80dc3284 
attach wifi 8188 success
attach wifi 5370 success
-------------attach_rt7601_dev---p_handle 80a76de0 --------
mtk_mt7601u_open. 
attach wifi 7601 success
-------------attach_lynx_dev---p_handle 80a76dfc --------
wifi dev = 0x80dc3600 
attach wifi lynx wi7000u success
serial_open
[AI][_ai_mdl_init]Entry...ticks:208
file_size 564795 p_data_buffer 80e56ba0 

 unzip resource. in_addr = 0x9e36275b, out_addr = 0x82a33c00, in_len = 564795, out_len = 1344464
**LCK UDQ**: 2b16
[AI][_ai_usb_monitor_init]Entry...ticks:258
[AI][_ai_eva_init]Entry...ticks:258
[AI][_ai_tuner_init]Entry...ticks:259
[AI][_ai_dvb_init]Entry...ticks:280
[CA]: Not init
[AI][_ai_dmm_init]Entry...ticks:280
update_userdb_version(512): ori sat = 0x0, tp = 0x0, pg = 0x0, cur sat = 0x44, tp = 0x18, pg = 0xc0.
load default start...
load default finish.
[AI][_ai_mdl_init]Software Ver[1000000]
[AI][_ai_avc_init]Entry...ticks:303
[AI][_ai_iconv_init]Entry...ticks:303
[AI][_ai_antenna_lnb_init]Entry...ticks:303
*********hdmi config value=12340000
[AI][_ai_hdmi_config]Entry...ticks:304
[AI][_ai_time_init]Entry...ticks:338
eve0
[AI][ap_init]End...
orts0 
 hub_add_new_dev hcd 80d5b9c0
hub_add_new_dev 80e9bd40
port_reset 80d5b9c0
close_fast_logo
mmi init
mmi ver 445:7ae10329f0a8
GUI partation is ok
rsc_init is ok
pre gdi_init is ok
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
desktop init
_switch_playstatus
from_id = 0 to_id&ehci->regs->port_status[0] bf070084
ehci->regs->port_status[0] 8000205
###step1.2### 0 usb_hcd_poll_rh_status 
 = 1
new_ps = 1 CURN_MENU_PLAY_STATE = 1
switch_autoclose: from 0 to 1 
switch_autoclose: create tmr 
menu manager inital
menu manager inital 1
menu manager inital 2
@@@ui_util_api_init_vsurf-------
------------->>active ap playback
UI: active playback.........
_ui_epg_api_init epg addr 0x83f9dc00
end desktop init
get ver 0
close_fast_logo
@@@ui_util_api_release_vsurf-------
@@@ui_util_api_init_vsurf-------
_switch_playstatus
from_id = 0 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 1
UI: switch to LOGO..........
on_factory_test_uart LINE:[207]
welcome toon_factory_test_uart LINE:[234]
stop type[1]
Before ui_set_subt_display
After ui_set_subt_display
UI: disable subt.........
Leave ui_enable_subt
UI: disable ttx.........
-----ui show logo v2 size 0xd599, 0, 179
switch_autoclose: from 0 to 2 
switch_autoclose: destroy tmr 
ui_main_prog finish---
 mtos_mem_user_debug, alloced = 2646560, alloced_peak = 2723680, rest_size = 27844144

0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 0x00 
[cy] off... 
EMON> [NW] Set 3g sts:2
   #3device ADD cost 159 ts 
[AI][_ai_usb_plug_in_cb]Enter...

## timeshift exist is [1393786880]
[USB]ui_upg_file_list_get:file count[0x22]
[USB]ui_upg_file_list_get:valid_file_cnt[0x8]

## timeshift exist is [1393786880]
p_cont[0x80eb8bf8], root[0]
_switch_playstatus
from_id = 2 to_id = 24
new_ps = 0 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 24 
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
update signal
---------------Time Stamp[16:45:07]----------------
---------------Time Stamp[16:50:07]----------------
---------------Time Stamp[16:55:07]----------------
---------------Time Stamp[17:00:07]----------------
---------------Time Stamp[17:05:07]----------------
---------------Time Stamp[17:10:07]----------------
---------------Time Stamp[17:15:07]----------------
---------------Time Stamp[17:20:07]----------------
---------------Time Stamp[17:25:07]----------------
---------------Time Stamp[17:30:07]----------------
---------------Time Stamp[17:35:07]----------------
