Serial Port Opened
monitor start
_switch_playstatus
from_id = 2 to_id = 2
new_ps = 3 CURN_MENU_PLAY_STATE = 3
switch_autoclose: from 2 to 2 
[CA MANAGER]: type:12, para1:2, para2:2
update signal

## timeshift exist is [426221568]

## timeshift exist is [426221568]

##ufs_open fail[4]:[C:\chip_id.txt]
--- file.txt write size 31
update signal
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run failed.
download failed!
monitor start
monitor stop
uboot run failed!
download successful!
monitor start
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run failed.
download failed!
monitor start
Serial Port Opened
monitor start
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x00000803 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001205 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... 2 USB Device(s) found
       scanning bus for storage devices... 0 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found

** Invalid boot device **
do_spi_flash_uboot_save offset[0] len[2d600000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected PN25F32 with erase size 64 KiB, total 4 MiB
ROSerial Port Closed
upg or dump task  is canceled!
monitor stop
Serial Port Opened
monitor start
Serial Port Closed
upg or dump task  is canceled!
monitor stop
Barcode thread exit
Upgrade thread exit
monitor exit
