Serial Port Opened
monitor start
ROM
MCPU: version:btinit VER 0.0.5_sym:[hg_37_4a35d9b5f498] Build Time:[Mar 23 2017, 09:26:03]BBBBBB9BBV


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8000
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 128MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready

pinmux:
REG[bf13c000] = 00000000
REG[bf13c004] = 00011000
REG[bf13c008] = 12212110
REG[bf13c00c] = 00000121
REG[bf13c010] = 00220000
REG[bf13c014] = 00111001
REG[bf15b400] = 00000000
REG[bf15b404] = 00000000

cpu_secondary_init_r: image file for secondary core should already locate where it should be
current boot media:0...
phy_clk = 405, clk=50
R_SPIN_CH0_BAUD: 40000009
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
Hit any key to stop autoboot:  0 
project flash size is 0x400000
 size1=257479 257463 
 main_start =0x87e10000 0x9e040410 

 load_secondary_core_boot_word : secondary_img_start = 0x87e10000 
runav 731 
concerto_check_cpu_ready: s ^rt 
n main , ebase=0x87e01001, cause=0x880005c, status=0x4602
avcpu ver = AVCPU_VERSION:[445:af7e48d68452] Build Time:[May 15 2017, 17:23:33]
concerto_check_cpu_ready: start
runav 736 
need go to fastlogo to checkgo_to_block_app 0x89 
10123**CDU UDQ**: 8afa 48
===========>dir:0


U-Boot 2012.04-hg1288-93997f6efda3-dirty (Mar 23 2017 - 10:51:49)

*****************************************
**  Board: mips CPU: sym - MIPS 24KEc
**  SOC name  : 0x8000
**  PACKET type : QFP 144
*****************************************
DRAM:  
DDR is 2050MiBytes
20 MiB
== OTP_VERSION:[hg_NA] Build Time:[Mar 23 2017, 10:51:49]
Using default environment

SPI: ready
Net:   mt_eth
main_loop entered: bootdelay=0

check boot type
boot is reback from APP!
project flash size is 0x400000
go_to_block_app 0x88 
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001a05 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... cannot reset port 1!?
1 USB Device(s) found
       scanning bus for storage devices... 0 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found

** Invalid boot device **
do_spi_flash_uboot_save offset[0] len[2d600000]
spi0 is already setup!!!
SF: spi flash status register: 0x14, 0x40
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001a05 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... cannot reset port 1!?
1 USB Device(s) found
       scanning bus for storage devices... 0 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found

** Invalid boot device **
do_spi_flash_uboot_save offset[0] len[2d600000]
spi0 is already setup!!!
SF: spi flash status register: 0x00, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
download start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x0c000000 port_sts1:0x00000803 
auto_detect_usb_port --- usb sel port 1
USB:   usb_debug 
need usb1 plug in.... 
usb1 device connect port status :0x1803 
port1 reset down port status :0x8001a05 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... cannot reset port 1!?
1 USB Device(s) found
       scanning bus for storage devices... 0 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found

** Invalid boot device **
do_spi_flash_uboot_save offset[0] len[2d600000]
spi0 is already setup!!!
SF: spi flash status register: 0x00, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
ROdownload start
Please reboot the STB manually.
Change baudrate to 115200.
monitor stop
Sync Succeed.
Sending boot init...
Send boot init completed.
boot init run successfully.
SendClient.
Sending Client is complete.
Client is up.
Client Functionality is good.
uboot run successful
download successful!
monitor start
usb start;fatload usb 0 83000000 flash.bin;sf burn 83000000 0 800000;
(Re)start USB...
auto_detect_usb_port --- usb default sel port 1
port_sts0:0x00000803 port_sts1:0x0c000000 
auto_detect_usb_port --- usb sel port 0
USB:   usb_debug 
need usb0 plug in.... 
usb0 device connect port status :0x1803 
port0 reset down port status :0x8001a05 
ehci_hcd_init...
Register 10011 NbrPorts 1
USB EHCI 1.00
scanning bus for devices... cannot reset port 1!?
1 USB Device(s) found
       scanning bus for storage devices... 0 Storage Device(s) found
       scanning bus for ethernet devices... 0 Ethernet Device(s) found

** Invalid boot device **
do_spi_flash_uboot_save offset[0] len[2d600000]
spi0 is already setup!!!
SF: spi flash status register: 0x00, 0x00
SPI: Detected GD25Q64 with erase size 64 KiB, total 8 MiB
---------------Time Stamp[09:49:44]----------------
---------------Time Stamp[09:54:44]----------------
monitor stop
Barcode thread exit
Upgrade thread exit
monitor exit
